# Changelog
The latest version may not be released!
See also the commit log at github: https://github.com/Arduino-IRremote/Arduino-IRremote/commits/master

# 4.7.0
- Added removed typedef `IRRawDataType` for backward compatibility.
- Modified and renamed function `setToggleBitValueForRC5AndRC6()` to `setNextToggleBitValueForRC5AndRC6()`.
- Fixed bug in sending RC6A.
- Updated `LG` protocol and removed useless `LG2` protocol.
- Added new functions `match*WithGreaterRange()`, e.g. `matchMarkWithGreaterRange()`.
- Improved B&O decoding using new functions.

# 4.6.1
- Fixed bug #1347 in RC5/RC6 autorepeat bit handling. Thanks to Craig Leres.
- Added function `setToggleBitValueForRC5AndRC6()`.

# 4.6.0
- Fixed missing ESP IRAM_ATTR for receiving interrupt.
- Changed `USE_DEFAULT_FEEDBACK_LED_PIN` from 0 to 0xFF, because megaTinyCore defines the not special pin PIN_PA4 as 0.
- Changed timer for **ATtiny16X4**.
- Fixed missing initialization with `pinMode()` for feedback LED.
- Fixed bitmask error in `sendBiphaseData()` when not sending start bit.
- Improved `decodeSamsung()`.
- `OpenLASIR` protocol added by [danielweidman](https://github.com/danielweidman).
- Added `DECODE_MARANTZ` and swapped parameter aMarantzExtension and aNumberOfRepeats of `sendMaranz()` to be consistent with other extensions.
- Improved biphase decoding.
- Improved debug output handling.
- Moved `IRCommandDispatcher` from demo to main library folder.
- Changed `IRRawDataType` to `IRDecodedRawDataType`.

# 4.5.0 - does not work for ESP platform, because of missing ESP IRAM_ATTR for receiving interrupt.
- Added support for **multiple receiver instances**.
- irparams_struct `irparams` is now member of IRrecv. Thus removed `rawDataPt`r (pointer to irparams) from `IrReceiver.decodedIRData`.
- Removed return value for all `decodePulseDistanceWidthData()` decoding functions, which returned a constant true.
- Removed parameter `aEnableLEDFeedback` in function `IRsend::begin(bool aEnableLEDFeedback, uint_fast8_t aFeedbackLEDPin)` and `IRsend::begin(uint_fast8_t aSendPin, bool aEnableLEDFeedback, uint_fast8_t aFeedbackLEDPin)`.
- **LED feedback is always enabled for sending**. It can only be disabled by using the macro `NO_LED_SEND_FEEDBACK_CODE`.
- Added output for UNKNOWN protocol to `printIRSendUsage()`.
- Added experimental `sendVelux()`.
- Added `sendMaranz()`.
- Fixed bug in ReceiveDemo.cpp if DEBUG_BUTTON_PIN is not defined. #1306.
- Fixed minor bugs in Denon decoder.
- Minor bug fixes for DEBUG.
- New handling of `MARK_EXCESS_MICROS` without strange rounding inconsistency.
- Added experimental threshold decoding.

# 4.4.3
- Added `USE_ACTIVE_LOW_OUTPUT_FOR_SEND_PIN` to make the software aware of send LED connected between VCC and send pin.
- Fixed backward compatibility bug for `printIRResultShort(Print *aSerial, bool aPrintRepeatGap, bool aCheckForRecordGapsMicros)`.
- Minor improvements.

# 4.4.2
- Support for `SAMD51` timer3 if timer 5 is not available (Adafruit ItsyBitsy M4).
- attachInterrupt() on `SAMD` has a different semantic :-(. See: https://www.arduino.cc/reference/tr/language/functions/external-interrupts/attachinterrupt/.
- Fixed overflow handling.
- Improved repeat detection for `DistanceWidthProtocol`.
- Print of IR frame duration in `printIRResultShort()`;
- `PulseDistanceWidthProtocolConstants` now in PROGMEM, this saves 190 bytes RAM for unit test.
- Support for PROGMEM PulseDistanceWidthProtocol data.
- Support duplicated 8 bit address for `sendSamsungLG()`.

# 4.4.1
- Support for **ESP core 3.x** by akellai.
- `restartTimer()` now uses variable sMicrosAtLastStopTimer to keep track of uncounted ticks between stopTimer() and restartTimer().
- **Removed functions** addTicksToInternalTickCounter() and addMicrosToInternalTickCounter(), which were added in 4.1.0.
- Version 2.2.0 of TinyIR with new `TinyReceiverDecode()` function to be used as **drop in for IrReceiver.decode()**.
- Support of `RC6A`.

# 4.4.0
- Using 8 bit raw timing buffer for all timings except frame gap (former rawbuf[0]).
- Renamed `decodedIRData.initialGap` to `decodedIRData.initialGapTicks`.
- `sendNEC()` and `sendNEC2()` now **accepts 16 bit command** to better map to **NECext protocol** found in IRDB databases.
- `ir_DistanceWidthProtocol()` now decodes up to 10 ms mark or spaces if RAM is bigger than 2 k.
- Improved sensitivity and decoding of `PULSE_DISTANCE` + `PULSE_WIDTH` protocols.
- Changed `TOLERANCE_FOR_DECODERS_MARK_OR_SPACE_MATCHING` to `TOLERANCE_FOR_DECODERS_MARK_OR_SPACE_MATCHING_PERCENT`.
- Improved examples AllProtocolsOnLCD, UnitTest and SimpleReceiver.
- New functions `decodePulseDistanceWidthData()` with 6 parameters and `decodePulseDistanceWidthDataStrict()` with 7 parameters.

# 4.3.2
- Added sendSonyMSB(unsigned long data, int nbits) as a clone of sendSony(unsigned long data, int nbits) to be more consistent.
- Added sendSamsungMSB(unsigned long data, int nbits) as a clone of sendSAMSUNG(unsigned long data, int nbits) to be more consistent.
- Added ESP32 core 3.x error message.

# 4.3.1
 - Fixed overflow bug for rawlen > 254.
 - Removed deprecated sendPulseDistance... functions with parameter aSendStopBit.

# 4.3.0
- Removed default value USE_DEFAULT_FEEDBACK_LED_PIN for last parameter of IRsend::begin(bool aEnableLEDFeedback, uint_fast8_t aFeedbackLEDPin).
    Therefore IrSender.begin(DISABLE_LED_FEEDBACK) will not longer work!
- Added convenience function isIRReceiverAttachedForTinyReceiver().
- Added Extended NEC Protocol macro to TinyIR by Buzzerb.
- Fixed sendSamsung() / sendSamsungLG() bug.
- Added functions stopTimer(), restartTimer() and restartTimerWithTicksToAdd().
- Added rawlen and initialGap to IRData.
- Added ReceiveAndSendHobToHood example.
- Changed RECORD_GAP_MICROS default value from 5000 to 8000.

# 4.2.1
- Fix wrong type of tEnableLEDFeedback in IRSend.hpp and IRReceive.hpp.
- TinyReceiver 2.0
  - New TinyIRReceiverData which is filled with address, command and flags.
  - Removed parameters address, command and flags from callback handleReceivedTinyIRData() and printTinyReceiverResultMinimal().
  - Callback function now only enabled if USE_CALLBACK_FOR_TINY_RECEIVER is activated.
- Fix changing IR_SEND_PIN dynamically for ESP32.
- Fix wrong type of tEnableLEDFeedback.
- Support for ESP32-C3.

# 4.2.0
- The old decode function is renamed to decode_old(decode_results *aResults). decode (decode_results *aResults) is only available in IRremote.h and prints a message.
- Added DECODE_ONKYO, to force 16 bit command and data decoding.
- Enable Bang&Olufsen 455 kHz if SEND_PWM_BY_TIMER is defined.
- Fixed bug: TinyReceiver throwing ISR not in IRAM on ESP8266.
- Usage of ATTinyCore pin numbering scheme e.g. PIN_PB2.
- Added ARDUINO_ARCH_NRF52 to support Seeed XIAO nRF52840 Sense.
- First untested support of Uno R4.
- Extracted version macros to IRVersion.h.

## 4.1.2
- Workaround for ESP32 RTOS delay() timing bug influencing the mark() function.

## 4.1.1
- SAMD51 use timer3 if timer5 not available.
- Disabled #define LOCAL_DEBUG in IRReceive.hpp, which was accidentally enabled at 4.1.0.

## 4.1.0
- Fixed bug in printing durations > 64535 in printIRResultRawFormatted().
- Narrowed constraints for RC5 RC6 number of bits.
- Changed the first parameter of printTinyReceiverResultMinimal() to &Serial.
- Removed 3 Serial prints for deprecation warnings to fix #1094.
- Version 1.2.0 of TinyIR. Now FAST protocol with 40 ms period and shorter header space.
- Removed field "bool hasStopBit" and parameter "bool aSendStopBit" from PulseDistanceWidthProtocolConstants structure and related functions.
- Changed a lot of "unsigned int" types to "uint16_t" types.
- Improved overflow handling.
- Improved software PWM generation.
- Added FAST protocol.
- Improved handling of PULSE_DISTANCE + PULSE_WIDTH protocols.
- New example ReceiveAndSendDistanceWidth.
- Removed the automatic restarting of the receiver timer after sending with SEND_PWM_BY_TIMER enabled.
- Split ISR into ISR and function IRPinChangeInterruptHandler().
- Added functions addTicksToInternalTickCounter() and addMicrosToInternalTickCounter().

## 4.0.0
- Added decoding of PulseDistanceWidth protocols and therefore changed function decodeDistance() to decodeDistanceWidth() and filename ir_DistanceProtocol.hpp to ir_DistanceWidthProtocol.hpp.
- Removed static function printIRSendUsage(), but kept class function printIRSendUsage().
- Changed type of decodedRawData and decodedRawDataArray which is now 64 bit for 32 bit platforms.
- Added receiver callback functionality and registerReceiveCompleteCallback() function.
- Introduced common structure PulseDistanceWidthProtocolConstants.
- Where possible, changed all send and decode functions to use PulseDistanceWidthProtocolConstants.
- Improved MSB/LSB handling
- New convenience functions bitreverse32Bit() and bitreverseOneByte().
- Improved Magiquest protocol.
- Fix for #1028 - Prevent long delay caused by overflow when frame duration < repeat period - Thanks to Stephen Humphries!
- Support for ATtiny816 - Thanks to elockman.
- Added Bang&Olufsen protocol. #1030.
- Third parameter of function "void begin(uint_fast8_t aSendPin, bool aEnableLEDFeedback, uint_fast8_t aFeedbackLEDPin)" is not optional anymore and this function is now only available if IR_SEND_PIN is not defined. #1033.
- Fixed bug in sendSony() for command parameter > 0x7F;
- Fixed bug with swapped LG2 header mark and space.
- Disabled strict checks while decoding. They can be enabled by defining DECODE_STRICT_CHECKS.
- Merged the 2 decode pulse width and distance functions.
- Changed macro names _REPEAT_SPACE to _REPEAT_DISTANCE.
- Improved TinyIRReceiver,added FAST protocol for it and added TinyIRSender.hpp and TinySender example, renamed TinyReceiver.h to TinyIR.h.
- Added DISABLE_CODE_FOR_RECEIVER to save program memory and RAM if receiving functionality is not required.
- Extracted protocol functions used by receive and send to IRProtocol.hpp.
- Analyzed Denon code table and therefore changed Denon from MSB to LSB first.
- Renamed sendRC6(aRawData...) to sendRC6Raw( aRawData...).
- Support for seeduino which lacks the print(unsigned long long...) method. Thanks to sklott https://stackoverflow.com/users/11680056/sklott
- Added support for attiny1614 by Joe Ostrander.
- Fixed SEND_PWM_BY_TIMER for ATtiny167 thanks to freskpe.
- Improved SHARP repeat decoding.
- Replaced macros TIMER_EN/DISABLE_RECEIVE_INTR and EN/DISABLE_SEND_PWM_BY_TIMER by functions.
- Added SAMSUNG48 protocol and sendSamsung48() function.

## 3.9.0
- Improved documentation with the help of [ElectronicsArchiver}(https://github.com/ElectronicsArchiver).
- Added NEC2 protocol.
- Improved Magiquest protocol.
- Renamed sendSamsungRepeat() to sendSamsungLGRepeat().
- Added function sendPulseDistanceWidth().
- Improved repeat detection for some protocols.

## 3.8.0
- Changed Samsung repeat handling. Old handling is available as SamsungLG.
- Added function printIRSendUsage().
- Reduced output size and improved format of printIRResultRawFormatted() to fasten up output (and getting repeats properly decoded).
- Fixed Bug in sendDenonRaw() and improved decodeDenon().
- Fixed potential bug in SendBiphase data for 1 bit.
- Fixed bug in send for RP4020.
- Fixed pin mapping problems especially for Teensy 2.0.
- Added support for decoding of "special" NEC repeats.
- Added SAMD51 support.
- Improved pin mapping for TinyReceiver.

## 3.7.1
- SendRaw now supports buffer length > 255.
- Improved DistanceProtocol decoder output.
- Fixed ESP32 send bug for 2.x ESP32 cores.

## 3.7.0
- Changed TOLERANCE to TOLERANCE_FOR_DECODERS_MARK_OR_SPACE_MATCHING and documented it.
- Changed last uint8_t to uint_fast8_t and uint16_t to unsigned integer.
- Improved MagiQuest protocol.
- Improved prints and documentation.
- Added IrReceiver.restartAfterSend() and inserted it in every send(). Closes #989
- Use IRAM_ATTR instead of deprecated ICACHE_RAM_ATTR for ESP8266.
- Removed pulse width decoding from ir_DistanceProtocol.

## 3.6.1
- Switched Bose internal protocol timing for 0 and 1 -> old 1 timing is now 0 and vice versa.

## 3.6.0
- Separated enable flag of send and receive feedback LED. Inspired by PR#970 from luvaihassanali.
- RP2040 support added.
- Refactored IRTimer.hpp.
- Refactored IR_SEND_PIN and IrSender.sendPin handling.
- Renamed IR_SEND_DUTY_CYCLE to IR_SEND_DUTY_CYCLE_PERCENT.
- Fixed bugs for SEND_PWM_BY_TIMER active.

## 3.5.2
- Improved support for Teensy boards by Paul Stoffregen.

## 3.5.1
- Renamed INFO_PRINT to IR_INFO_PRINT as well as for DEBUG and TRACE.
- Fixed error with DEBUG in TinyIRReceiver.hpp.
- Support for ATmega88 see issue #923. Thanks to Dolmant.
- NO_LED_FEEDBACK_CODE replaces and extends DISABLE_LED_FEEDBACK_FOR_RECEIVE.
- Removed NO_LEGACY_COMPATIBILITY macro, it was useless now.
- Fix ESP32 send bug see issue #927.

## 3.5.0
- Improved ir_DistanceProtocol.
- Tone for ESP32.
- last phase renamed *.cpp.h to .hpp.
- No deprecation print for ATtinies.
- Renamed ac_LG.cpp to ac_LG.hpp.
- Maintained MagiQuest by E. Stuart Hicks.
- Improved print Pronto by Asuki Kono.
- Added printActiveIRProtocols() function.
- Used IR_SEND_PIN to reduce code size and improved send timing for AVR.

## 3.4.0
- Added LG2 protocol.
- Added ATtiny167 (Digispark Pro) support.
- Renamed *.cpp.h to .hpp.
- organized carrier frequencies.
- Compiler switch USE_OPEN_DRAIN_OUTPUT_FOR_SEND_PIN added.
- Moved blink13() back to IRrecv class.
- Added Kaseikyo convenience functions like sendKaseikyo_Denon().
- Improved / adjusted LG protocol and added class Aircondition_LG based on real hardware supplied by makerspace 201 (https://wiki.hackerspaces.org/ZwoNullEins) from Cologne.
- Improved universal decoder for pulse distance protocols to support more than 32 bits.
- Added mbed support.

## 3.3.0
- Fix errors if LED_BUILTIN is not defined.
- Fixed error for AVR timer1. Thanks to alexbarcelo.
- New example IRremoteExtensionTest.
- Enabled megaAVR 0-series devices.
- Added universal decoder for pulse distance protocols.

## 3.2.0
- Fix for ESP32 send Error, removed `USE_SOFT_SEND_PWM` macro.
- Added Onkyo protocol.
- Support for old 2.x code by backwards compatible `decode(decode_results *aResults)` function.
- Removed USE_OLD_DECODE macro and added NO_LEGACY_COMPATIBILITY macro.
- Added ATtiny1604 support.
- New SendAndReceive example.
- Added ESP8266 support.
- Extended DEBUG output.

## 3.1.0
- Generation of PWM by software is active by default.
- Removed decode_results results.
- Renamed most irparams_struct values.
- Fixed LG send bug and added unit test.
- Replaced `#define DECODE_NEC 1/0` by defining/not defining.
- Use LED_BUILTIN instead of FEEDBACK_LED if FeedbackLEDPin is 0.
- Use F_CPU instead of SYSCLOCK.
- Removed SENDPIN_ON and SENDPIN_OFF macros.

- Refactored board specific code for timer and feedback LED.
- Extracted common LED feedback functions and implemented feedback for send.
- MATCH_MARK() etc. now available as matchMark().
- Added STM32F1 by (by Roger Clark) support.
- Added stm32 (by ST) support. Thanks to Paolo Malaspina.
- Added ATtiny88 support.

## 3.0.2
- Bug fix for USE_OLD_DECODE.
- Increase RECORD_GAP_MICROS to 11000.
- Fix overflow message. (#793).
- Improved handling for HASH decoder.
- Tested for ATtiny85.
- Added `printIRResultMinimal()`.
- Added missing IRAM_ATTR for ESP32.
- Adapted to TinyCore 0.0.7.
- Fixed decodeSony 20 bit bug #811.
- Replaced delayMicroseconds with customDelayMicroseconds and removed NoInterrupt() for send functions, removed SPIN_WAIT macro, sleepMicros() and sleepUntilMicros().
- Fixed LG checksum error.
- Fixed JVC repeat error.

## 3.0.0 + 3.0.1 2021/02
- New LSB first decoders are default.
- Added SendRaw with byte data.
- Fixed resume bug if irparams.rawlen >= RAW_BUFFER_LENGTH. Thanks to Iosif Peterfi
- Added `dumpPronto(String *aString, unsigned int frequency)` with String object as argument. Thanks to Iosif Peterfi
- Removed Test2 example.
- Fixed swapped cases in `getProtocolString()`. Thanks to Jim-2249
- Added compile option `IR_INPUT_IS_ACTIVE_HIGH`. Thanks to Jim-2249
- Corrected template. Thanks to Jim-2249
- Introduced standard decode and send functions.
- Added compatibility with tone for AVR's.
- New TinyIRreceiver does not require a timer.
- New MinimalReceiver and IRDispatcherDemo examples.
- Added TinyCore 32 / ATtiny3217 support.
- Added Apple protocol.

## 2.8.1 2020/10
- Fixed bug in Sony decode introduced in 2.8.0.

## 2.8.0 2020/10
- Changed License to MIT see https://github.com/Arduino-IRremote/Arduino-IRremote/issues/397.
- Added ATtiny timer 1 support.
- Changed wrong return code signature of decodePulseDistanceData() and its handling.
- Removed Mitsubishi protocol, since the implementation is in contradiction with all documentation I found and therefore supposed to be wrong.
- Removed AIWA implementation, since it is only for 1 device and at least the sending was implemented wrong.
- Added Lego_PF decode.
- Changed internal usage of custom_delay_usec.
- Moved dump/print functions from example to irReceiver.
- irPronto.cpp: Using Print instead of Stream saves 1020 bytes program memory. Changed from & to * parameter type to be more transparent and consistent with other code of IRremote.

## 2.7.0 2020/09
- Added ATmega328PB support.
- Renamed hardware specific macro and function names.
- Renamed `USE_SOFT_CARRIER`, `USE_NO_CARRIER`, `DUTY_CYCLE` macros to `USE_SOFT_SEND_PWM`, `USE_NO_SEND_PWM`, `IR_SEND_DUTY_CYCLE`.
- Removed blocking wait for ATmega32U4 Serial in examples.
- Deactivated default debug output.
- Optimized types in sendRC5ext and sendSharpAlt.
- Added `DECODE_NEC_STANDARD` and `SEND_NEC_STANDARD`.
- Renamed all IRrecv* examples to IRreceive*.
- Added functions `printIRResultShort(&Serial)` and `getProtocolString(decode_type_t aDecodeType)`.
- Added flag `decodedIRData.isRepeat`.
- Updated examples.

## 2.6.1 2020/08
- Adjusted JVC and LG timing.
- Fixed 4809 bug.

## 2.6.0 2020/08
- Added support for MagiQuest IR wands.
- Corrected Samsung timing.
- NEC repeat implementation.
- Formatting and changing `TIMER_CONFIG_KHZ` and `TIMER_CONFIG_NORMAL` macros to static functions.
- Added `IRAM_ATTR` for ESP32 ISR.
- Removed `#define HAS_AVR_INTERRUPT_H`.
- Changed Receiver States. Now starting with 0.
- Changed switch to if / else if in IRRemote.cpp because of ESP32 compiler bug.
- Changed `DEBUG` handling since compiler warns about empty "IF" or "ELSE" statements in IRRemote.cpp.

## 2.5.0 2020/06
- Corrected keywords.txt.
- BoseWave protocol added PR #690.
- Formatting comply to the new stylesheet.
- Renamed "boarddefs.h".
- Renamed `SEND_PIN` to `IR_SEND_PIN`.
- Renamed state macros.
- Enabled `DUTY_CYCLE` for send signal.
- Added sending for ESP32.
- Changed rawlen from uint8_t to unsigned int allowing bigger receive buffer and renamed `RAWBUF` to `RAW_BUFFER_LENGTH`.
- Introduced `USE_NO_CARRIER` for simulating an IR receiver.
Changes from #283 by bengtmartensson
- Added function sendRaw_P() for sending data from flash.
Changes from #268 by adamlhumphreys
- Optimized by reducing floating point operations as suggested by madmalkav (#193).
- Optimized with macros when using default `MICROS_PER_TICK` and `TOLERANCE`.
- Made decodeHash as a settable protocol defined by `DECODE_HASH`.
- Added Philips Extended RC-5 protocol support [PR #522] (https://github.com/Arduino-IRremote/Arduino-IRremote/pull/522)

## 2.4.0 - 2017/08/10
 - Cleanup of hardware dependencies. Merge in SAM support [PR #437](https://github.com/Arduino-IRremote/Arduino-IRremote/pull/437)

## 2.3.3 - 2017/03/31
- Added ESP32 IR receive support [PR #427](https://github.com/Arduino-IRremote/Arduino-IRremote/pull/425)

## 2.2.3 - 2017/03/27
- Fix calculation of pause length in LEGO PF protocol [PR #427](https://github.com/Arduino-IRremote/Arduino-IRremote/pull/427)

## 2.2.2 - 2017/01/20
- Fixed naming bug [PR #398](https://github.com/Arduino-IRremote/Arduino-IRremote/pull/398)

## 2.2.1 - 2016/07/27
- Added tests for Lego Power Functions Protocol [PR #336](https://github.com/Arduino-IRremote/Arduino-IRremote/pull/336)

## 2.2.0 - 2016/06/28
- Added support for ATmega8535
- Added support for ATmega16
- Added support for ATmega32
- Added support for ATmega164
- Added support for ATmega324
- Added support for ATmega644
- Added support for ATmega1284
- Added support for ATmega64
- Added support for ATmega128

[PR](https://github.com/Arduino-IRremote/Arduino-IRremote/pull/324)

## 2.1.1 - 2016/05/04
- Added Lego Power Functions Protocol [PR #309](https://github.com/Arduino-IRremote/Arduino-IRremote/pull/309)

## 2.1.0 - 2016/02/20
- Improved Debugging [PR #258](https://github.com/Arduino-IRremote/Arduino-IRremote/pull/258)
- Display TIME instead of TICKS [PR #258](https://github.com/Arduino-IRremote/Arduino-IRremote/pull/258)

## 2.0.4 - 2016/02/20
- Add Panasonic and JVC to IRrecord example [PR](https://github.com/Arduino-IRremote/Arduino-IRremote/pull/54)

## 2.0.3 - 2016/02/20
- Change IRSend Raw parameter to const [PR](https://github.com/Arduino-IRremote/Arduino-IRremote/pull/227)

## 2.0.2 - 2015/12/02
- Added IRremoteInfo Sketch - [PR](https://github.com/Arduino-IRremote/Arduino-IRremote/pull/241)
- Enforcing changelog.md

## 2.0.1 - 2015/07/26 - [Release](https://github.com/shirriff/Arduino-IRremote/releases/tag/BETA)
### Changes
- Updated README
- Updated Contributors
- Fixed #110 Mess
- Created Gitter Room
- Added Gitter Badge
- Standardized Code Base
- Clean Debug Output
- Optimized Send Loops
- Modularized Design
- Optimized and Updated Examples
- Improved Documentation
- Fixed and Improved many coding errors
- Fixed Aiwa RC-T501 Decoding
- Fixed Interrupt on ATmega8
- Switched to Stable Release of PlatformIO

### Additions
- Added Aiwa RC-T501 Protocol
- Added Denon Protocol
- Added Pronto Support
- Added compile options
- Added Template For New Protocols
- Added this changelog
- Added Teensy LC Support
- Added ATtiny84 Support
- Added ATtiny85 Support
- Added isIdle method

### Deletions
- Removed (Fixed) #110
- Broke Teensy 3 / 3.1 Support

### Not Working
- Teensy 3 / 3.1 Support is in Development