Overview
--------
The LS2080A Development System (QDS) is a high-performance computing,
evaluation, and development platform that supports the QorIQ LS2080A
and LS2088A Layerscape Architecture processor. The LS2080AQDS provides
validation and SW development platform for the Freescale LS2080A, LS2088A
processor series, with a complete debugging environment.

LS2080A, LS2088A SoC Overview
--------------------
Please refer arch/arm/cpu/armv8/fsl-layerscape/doc/README.soc for LS2080A,
LS2088A SoC overview.

 LS2080AQDS board Overview
 -----------------------
 - SERDES Connections, 16 lanes supporting:
      - PCI Express - 3.0
      - SGMII, SGMII 2.5
      - QSGMII
      - SATA 3.0
      - XAUI
      - 10GBase-R
 - DDR Controller
     - Two ports of 72-bits (8-bits ECC) DDR4. Each port supports four
       chip-selects and two DIMM connectors. Support is up to 2133MT/s.
     - One port of 40-bits (8-bits ECC) DDR4 which supports four chip-selects
       and two DIMM connectors. Support is up to 1600MT/s.
 -IFC/Local Bus
    - IFC rev. 2.0 implementation supporting Little Endian connection scheme.
    - One in-socket 128 MB NOR flash 16-bit data bus
    - One 512 MB NAND flash with ECC support
    - IFC Test Port
    - PromJet Port
    - FPGA connection
 - USB 3.0
    - Two high speed USB 3.0 ports
    - First USB 3.0 port configured as Host with Type-A connector
    - Second USB 3.0 port configured as OTG with micro-AB connector
 - SDHC: PCIe x1 Right Angle connector for supporting following cards
    - 1/4-/8-bit SD/MMC Legacy CARD supporting 3.3V devices only
    - 1-/4-/8-bit SD/MMC Card supporting 1.8V devices only
    - 4-bit eMMC Card Rev 4.4 (1.8V only)
    - 8-bit eMMC Card Rev 4.5 (1.8V only)
    - SD Card Rev 2.0 and Rev 3.0
 - DSPI: 3 high-speed flash Memory for storage
    - 16 MB high-speed flash Memory for boot code and storage (up to 108MHz)
    - 8 MB high-speed flash Memory (up to 104 MHz)
    - 512 MB low-speed flash Memory (up to 40 MHz)
 - QSPI: via NAND/QSPI Card
 - 4 I2C controllers
 - Two SATA onboard connectors
 - UART
   - Two 4-pin (HW control) or four 2-pin (SW control) serial ports at up to 115.2 Kbit/s
   - Two DB9 D-Type connectors supporting one Serial port each
 - ARM JTAG support

Memory map from core's view
----------------------------
0x00_0000_0000 .. 0x00_000F_FFFF	Boot Rom
0x00_0100_0000 .. 0x00_0FFF_FFFF	CCSR
0x00_1800_0000 .. 0x00_181F_FFFF	OCRAM
0x00_3000_0000 .. 0x00_3FFF_FFFF	IFC region #1
0x00_8000_0000 .. 0x00_FFFF_FFFF	DDR region #1
0x05_1000_0000 .. 0x05_FFFF_FFFF	IFC region #2
0x80_8000_0000 .. 0xFF_FFFF_FFFF	DDR region #2

Other addresses are either reserved, or not used directly by U-Boot.
This list should be updated when more addresses are used.

IFC region map from core's view
-------------------------------
During boot i.e. IFC Region #1:-
  0x30000000 - 0x37ffffff : 128MB : NOR flash
  0x38000000 - 0x3BFFFFFF : 64MB  : Promjet
  0x3C000000 - 0x40000000 : 64MB  : FPGA etc

After relocate to DDR i.e. IFC Region #2:-
  0x5_1000_0000..0x5_1fff_ffff	Memory Hole
  0x5_2000_0000..0x5_3fff_ffff	IFC CSx (FPGA, NAND and others 512MB)
  0x5_4000_0000..0x5_7fff_ffff	ASIC or others 1GB
  0x5_8000_0000..0x5_bfff_ffff	IFC CS0 1GB (NOR/Promjet)
  0x5_C000_0000..0x5_ffff_ffff	IFC CS1 1GB (NOR/Promjet)

Booting Options
---------------
a) Promjet Boot
b) NOR boot
c) NAND boot
d) SD boot
e) QSPI boot

Memory map for NOR boot
-------------------------
Image				Flash Offset
RCW+PBI				0x00000000
Boot firmware (U-Boot)		0x00100000
Boot firmware Environment	0x00300000
PPA firmware			0x00400000
Secure Headers			0x00600000
DPAA2 MC			0x00A00000
DPAA2 DPL			0x00D00000
DPAA2 DPC			0x00E00000
Kernel.itb			0x01000000

Memory map for SD boot
-------------------------
Image				Flash Offset	SD Card
						Start Block No.
RCW+PBI				0x00000000	0x00008
Boot firmware (U-Boot)		0x00100000	0x00800
Boot firmware Environment	0x00300000	0x01800
PPA firmware			0x00400000	0x02000
DPAA2 MC			0x00A00000	0x05000
DPAA2 DPL			0x00D00000	0x06800
DPAA2 DPC			0x00E00000	0x07000
Kernel.itb			0x01000000	0x08000

Environment Variables
---------------------
- mcboottimeout: MC boot timeout in milliseconds. If this variable is not defined
  the value CFG_SYS_LS_MC_BOOT_TIMEOUT_MS will be assumed.

- mcmemsize: MC DRAM block size. If this variable is not defined
  the value CFG_SYS_LS_MC_DRAM_BLOCK_MIN_SIZE will be assumed.

Booting Linux flavors which do not support 48-bit VA (< Linux 3.18)
-------------------------------------------------------------------
One needs to use appropriate bootargs to boot Linux flavors which do
not support 48-bit VA (for e.g. < Linux 3.18) by appending mem=2048M, as shown
below:

=> setenv bootargs 'console=ttyS1,115200 root=/dev/ram
   earlycon=uart8250,mmio,0x21c0600,115200 default_hugepagesz=2m hugepagesz=2m
   hugepages=16 mem=2048M'


X-QSGMII-16PORT riser card
----------------------------
The X-QSGMII-16PORT is a 4xQSGMII/8xSGMII riser card with eighth SerDes
interfaces implemented in PCIe form factor board.
It supports following:
 - Card can operate with up to 4 QSGMII lane simultaneously
 - Card can operate with up to 8 SGMII lane simultaneously

Supported card configuration
	- CSEL  : ON ON ON ON
	- MSEL1 : ON ON ON ON OFF OFF OFF OFF
	- MSEL2 : OFF OFF OFF OFF ON ON ON ON

To enable this card: modify hwconfig to add "xqsgmii" variable.

Supported PHY addresses during SGMII:
#define XQSGMII_CARD_PHY1_PORT0_ADDR 0x0
#define XQSGMII_CARD_PHY1_PORT2_ADDR 0x2
#define XQSGMII_CARD_PHY2_PORT0_ADDR 0x4
#define XQSGMII_CARD_PHY2_PORT2_ADDR 0x6
#define XQSGMII_CARD_PHY3_PORT0_ADDR 0x8
#define XQSGMII_CARD_PHY3_PORT2_ADDR 0xa
#define XQSGMII_CARD_PHY4_PORT0_ADDR 0xc
#define XQSGMII_CARD_PHY4_PORT2_ADDR 0xe

Mapping DPMACx to PHY during SGMII
DPMAC1 -> PHY1-P0
DPMAC2 -> PHY2-P0
DPMAC3 -> PHY3-P0
DPMAC4 -> PHY4-P0
DPMAC5 -> PHY3-P2
DPMAC6 -> PHY1-P2
DPMAC7 -> PHY4-P1
DPMAC8 -> PHY2-P2
DPMAC9 -> PHY1-P0
DPMAC10 -> PHY2-P0
DPMAC11 -> PHY3-P0
DPMAC12 -> PHY4-P0
DPMAC13 -> PHY3-P2
DPMAC14 -> PHY1-P2
DPMAC15 -> PHY4-P1
DPMAC16 -> PHY2-P2


Supported PHY address during QSGMII
#define XQSGMII_CARD_PHY1_PORT0_ADDR 0x0
#define XQSGMII_CARD_PHY1_PORT1_ADDR 0x1
#define XQSGMII_CARD_PHY1_PORT2_ADDR 0x2
#define XQSGMII_CARD_PHY1_PORT3_ADDR 0x3
#define XQSGMII_CARD_PHY2_PORT0_ADDR 0x4
#define XQSGMII_CARD_PHY2_PORT1_ADDR 0x5
#define XQSGMII_CARD_PHY2_PORT2_ADDR 0x6
#define XQSGMII_CARD_PHY2_PORT3_ADDR 0x7
#define XQSGMII_CARD_PHY3_PORT0_ADDR 0x8
#define XQSGMII_CARD_PHY3_PORT1_ADDR 0x9
#define XQSGMII_CARD_PHY3_PORT2_ADDR 0xa
#define XQSGMII_CARD_PHY3_PORT3_ADDR 0xb
#define XQSGMII_CARD_PHY4_PORT0_ADDR 0xc
#define XQSGMII_CARD_PHY4_PORT1_ADDR 0xd
#define XQSGMII_CARD_PHY4_PORT2_ADDR 0xe
#define XQSGMII_CARD_PHY4_PORT3_ADDR 0xf

Mapping DPMACx to PHY during QSGMII
DPMAC1 -> PHY1-P3
DPMAC2 -> PHY1-P2
DPMAC3 -> PHY1-P1
DPMAC4 -> PHY1-P0
DPMAC5 -> PHY2-P3
DPMAC6 -> PHY2-P2
DPMAC7 -> PHY2-P1
DPMAC8 -> PHY2-P0
DPMAC9 -> PHY3-P0
DPMAC10 -> PHY3-P1
DPMAC11 -> PHY3-P2
DPMAC12 -> PHY3-P3
DPMAC13 -> PHY4-P0
DPMAC14 -> PHY4-P1
DPMAC15 -> PHY4-P2
DPMAC16 -> PHY4-P3
