
.. _timer:

:c:type:`uv_timer_t` --- Timer handle
=====================================

Timer handles are used to schedule callbacks to be called in the future.


Data types
----------

.. c:type:: uv_timer_t

    Timer handle type.

.. c:type:: void (*uv_timer_cb)(uv_timer_t* handle)

    Type definition for callback passed to :c:func:`uv_timer_start`.


Public members
^^^^^^^^^^^^^^

N/A

.. seealso:: The :c:type:`uv_handle_t` members also apply.


API
---

.. c:function:: int uv_timer_init(uv_loop_t* loop, uv_timer_t* handle)

    Initialize the handle.

.. c:function:: int uv_timer_start(uv_timer_t* handle, uv_timer_cb cb, uint64_t timeout, uint64_t repeat)

    Start the timer. `timeout` and `repeat` are in milliseconds.

    If `timeout` is zero, the callback fires on the next event loop iteration.
    If `repeat` is non-zero, the callback fires first after `timeout`
    milliseconds and then repeatedly after `repeat` milliseconds.

.. c:function:: int uv_timer_stop(uv_timer_t* handle)

    Stop the timer, the callback will not be called anymore.

.. c:function:: int uv_timer_again(uv_timer_t* handle)

    Stop the timer, and if it is repeating restart it using the repeat value
    as the timeout. If the timer has never been started before it returns
    UV_EINVAL.

.. c:function:: void uv_timer_set_repeat(uv_timer_t* handle, uint64_t repeat)

    Set the repeat value in milliseconds.

    .. note::
        If the repeat value is set from a timer callback it does not immediately take effect.
        If the timer was non-repeating before, it will have been stopped. If it was repeating,
        then the old repeat value will have been used to schedule the next timeout.

.. c:function:: uint64_t uv_timer_get_repeat(const uv_timer_t* handle)

    Get the timer repeat value.

.. seealso:: The :c:type:`uv_handle_t` API functions also apply.
