.. _hardware_index:

The pyboard hardware
====================

For the pyboard:

* `PYBv1.0 schematics and layout <http://micropython.org/resources/PYBv10b.pdf>`_ (2.4MiB PDF)
* `PYBv1.0 metric dimensions <http://micropython.org/resources/PYBv10b-metric-dimensions.pdf>`_ (360KiB PDF)
* `PYBv1.0 imperial dimensions <http://micropython.org/resources/PYBv10b-imperial-dimensions.pdf>`_ (360KiB PDF)

For the official skin modules:

* `LCD32MKv1.0 schematics <http://micropython.org/resources/LCD32MKv10-schematics.pdf>`_ (194KiB PDF)
* `AMPv1.0 schematics <http://micropython.org/resources/AMPv10-schematics.pdf>`_ (209KiB PDF)

Datasheets for the components on the pyboard
============================================

* The microcontroller: `STM32F405RGT6 <http://www.st.com/web/catalog/mmc/FM141/SC1169/SS1577/LN1035/PF252144>`_ (link to manufacturer's site)
* The accelerometer: `Freescale MMA7660 <http://micropython.org/resources/datasheets/MMA7660FC.pdf>`_ (800kiB PDF)
* The LDO voltage regulator: `Microchip MCP1802 <http://micropython.org/resources/datasheets/MCP1802-22053C.pdf>`_ (400kiB PDF)

Datasheets for other components
===============================

* The LCD display on the LCD touch-sensor skin: `Newhaven Display NHD-C12832A1Z-FSW-FBW-3V3 <http://micropython.org/resources/datasheets/NHD-C12832A1Z-FSW-FBW-3V3.pdf>`_ (460KiB PDF)
* The touch sensor chip on the LCD touch-sensor skin: `Freescale MPR121 <http://micropython.org/resources/datasheets/MPR121.pdf>`_ (280KiB PDF)
* The digital potentiometer on the audio skin: `Microchip MCP4541 <http://micropython.org/resources/datasheets/MCP4541-22107B.pdf>`_ (2.7MiB PDF)
