# Clock2.Bas

```
 Program: clock2.bas
```
```
REM From the ZX Spectrum MANUAL
REM A Clock program

REM First we draw the Sphere
CLS
CIRCLE 132, 105, 86
FOR n = 1 to 12
    PRINT AT 10 - (10 * COS(n * PI / 6) - 0.5), 16 + (0.5 + 10 * SIN(n * PI / 6)); n
NEXT n
CIRCLE 132, 105, 70

PRINT AT 23, 0; "PRESS ANY KEY TO EXIT";

FUNCTION t AS ULONG
    RETURN INT((65536 * PEEK (23674) + 256 * PEEK(23673) + PEEK (23672))/50)
END FUNCTION

DIM t1 as FLOAT

OVER 1
WHILE INKEY$ = ""
    LET t1 = t()
    LET a = t1 / 30 * PI: REM a is the seconds pointer in radians
    LET sx = 72 * SIN a : LET sy = 72 * COS a
    PLOT 131, 107: DRAW sx, sy

    LET t2 = t()
    WHILE (t2 <= t1) AND (INKEY$ = "")
        REM WARNING: Empty loops might be optimized and removed
        let t2 = t()
    END WHILE : REM Wait until the moment to move it

    PLOT 131, 107: DRAW sx, sy
END WHILE
```
