# SAS Portal API (Testing) . nodes . nodes . devices

## Instance Methods

Creates a device under a node or customer. Returned devices are unordered.

Creates a device under a node or customer.

Creates a signed device under a

Lists devices under a node or customer.

Retrieves the next page of results.

### Method Details

`bulk(parent, body=None, x__xgafv=None)`

    Creates a device under a node or customer. Returned devices are unordered.

    Args:
      parent: string, Required. The name of the parent resource. (required)
      body: object, The request body.
        The object takes the form of:

    { # Request for BulkCreateDevice method.
        "csv": "A String", # Required. A csv with each row representing a [device]. Each row must
            # conform to the regulations described on CreateDeviceRequest's device field.
      }

      x__xgafv: string, V1 error format.
        Allowed values
          1 - v1 error format
          2 - v2 error format

    Returns:
      An object of the form:

        { # Response for BulkCreateDevice method.
        "devices": [ # Required. The devices that were imported.
          {
            "name": "A String", # Output only. The resource path name.
            "preloadedConfig": { # Information about the device configuration. # Configuration of the device, as specified via SAS Portal API.
              "userId": "A String", # The identifier of a device user.
              "installationParams": { # Information about the device installation parameters. # Installation parameters for the device.
                "cpeCbsdIndication": True or False, # If present, this parameter specifies whether the CBSD is a CPE-CBSD or not.
                "antennaModel": "A String", # If an external antenna is used, the antenna model is optionally
                    # provided in this field. The string has a maximum length of 128
                    # octets.
                "verticalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
                    # antenna vertical location. This optional parameter should only be
                    # present if its value is less than the FCC requirement of 3
                    # meters.
                "longitude": 3.14, # Longitude of the device antenna location. in degrees relative to
                    # the WGS 84 datum. The allowed range is from -180.000000 to
                    # +180.000000. Positive values represent longitudes east of the
                    # prime meridian; negative values west of the prime
                    # meridian.
                "indoorDeployment": True or False, # Whether the device antenna is indoor or not. True: indoor. False:
                    # outdoor.
                "horizontalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
                    # antenna horizontal location. This optional parameter should only
                    # be present if its value is less than the FCC requirement of 50
                    # meters.
                "eirpCapability": 42, # This parameter is the maximum device EIRP in units of dBm/10MHz
                    # and is an integer with a value between -127 and +47 (dBm/10 MHz)
                    # inclusive. If not included, SAS interprets it as maximum
                    # allowable EIRP in units of dBm/10MHz for device category.
                "antennaDowntilt": 42, # Antenna downtilt in degrees and is an integer with a value
                    # between -90 and +90 inclusive; a negative value means the antenna
                    # is tilted up (above horizontal). This parameter is optional for
                    # Category A devices and conditional for Category B devices.
                "latitude": 3.14, # Latitude of the device antenna location in degrees relative to
                    # the WGS 84 datum. The allowed range is from -90.000000 to
                    # +90.000000. Positive values represent latitudes north of the
                    # equator; negative values south of the equator.
                "height": 3.14, # Device antenna height in meters. When the heightType parameter
                    # value is "AGL", the antenna height should be given relative to
                    # ground level. When the heightType parameter value is "AMSL", it
                    # is given with respect to WGS84 datum.
                "antennaGain": 42, # Peak antenna gain in dBi. This parameter is an integer with a
                    # value between -127 and +128 (dBi) inclusive.
                "heightType": "A String", # Specifies how the height is measured.
                "antennaBeamwidth": 42, # 3-dB antenna beamwidth of the antenna in the horizontal-plane in
                    # degrees.  This parameter is an unsigned integer having a value
                    # between 0 and 360 (degrees) inclusive; it is optional for
                    # Category A devices and conditional for Category B devices.
                "antennaAzimuth": 42, # Boresight direction of the horizontal plane of the antenna in
                    # degrees with respect to true north. The value of this parameter
                    # is an integer with a value between 0 and 359 inclusive. A value
                    # of 0 degrees means true north; a value of 90 degrees means
                    # east. This parameter is optional for Category A devices and
                    # conditional for Category B devices.
              },
              "isSigned": True or False, # Output-only. Whether the configuration has been signed by a CPI.
              "updateTime": "A String", # Output-only. The last time the device configuration was edited.
              "measurementCapabilities": [ # Measurement reporting capabilities of the device.
                "A String",
              ],
              "state": "A String", # State of the configuration.
              "airInterface": { # Information about the device's air interface. # Information about this device's air interface.
                "supportedSpec": "A String", # This field is related to the radioTechnology field and provides the air
                    # interface specification that the CBSD is compliant with at the time of
                    # registration.
                    #
                    # Optional
                "radioTechnology": "A String", # This field specifies the radio access technology that is used for the CBSD.
                    #
                    # Conditional
              },
              "category": "A String", # FCC category of the device.
              "callSign": "A String", # The call sign of the device operator.
              "model": { # Information about the model of the device. # Information about this device model.
                "softwareVersion": "A String", # The software version of the device.
                "firmwareVersion": "A String", # The firmware version of the device.
                "hardwareVersion": "A String", # The hardware version of the device.
                "vendor": "A String", # The name of the device vendor.
                "name": "A String", # The name of the device model.
              },
            },
            "activeConfig": { # Information about the device configuration. # Output only. Current configuration of the device as registered to the SAS.
              "userId": "A String", # The identifier of a device user.
              "installationParams": { # Information about the device installation parameters. # Installation parameters for the device.
                "cpeCbsdIndication": True or False, # If present, this parameter specifies whether the CBSD is a CPE-CBSD or not.
                "antennaModel": "A String", # If an external antenna is used, the antenna model is optionally
                    # provided in this field. The string has a maximum length of 128
                    # octets.
                "verticalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
                    # antenna vertical location. This optional parameter should only be
                    # present if its value is less than the FCC requirement of 3
                    # meters.
                "longitude": 3.14, # Longitude of the device antenna location. in degrees relative to
                    # the WGS 84 datum. The allowed range is from -180.000000 to
                    # +180.000000. Positive values represent longitudes east of the
                    # prime meridian; negative values west of the prime
                    # meridian.
                "indoorDeployment": True or False, # Whether the device antenna is indoor or not. True: indoor. False:
                    # outdoor.
                "horizontalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
                    # antenna horizontal location. This optional parameter should only
                    # be present if its value is less than the FCC requirement of 50
                    # meters.
                "eirpCapability": 42, # This parameter is the maximum device EIRP in units of dBm/10MHz
                    # and is an integer with a value between -127 and +47 (dBm/10 MHz)
                    # inclusive. If not included, SAS interprets it as maximum
                    # allowable EIRP in units of dBm/10MHz for device category.
                "antennaDowntilt": 42, # Antenna downtilt in degrees and is an integer with a value
                    # between -90 and +90 inclusive; a negative value means the antenna
                    # is tilted up (above horizontal). This parameter is optional for
                    # Category A devices and conditional for Category B devices.
                "latitude": 3.14, # Latitude of the device antenna location in degrees relative to
                    # the WGS 84 datum. The allowed range is from -90.000000 to
                    # +90.000000. Positive values represent latitudes north of the
                    # equator; negative values south of the equator.
                "height": 3.14, # Device antenna height in meters. When the heightType parameter
                    # value is "AGL", the antenna height should be given relative to
                    # ground level. When the heightType parameter value is "AMSL", it
                    # is given with respect to WGS84 datum.
                "antennaGain": 42, # Peak antenna gain in dBi. This parameter is an integer with a
                    # value between -127 and +128 (dBi) inclusive.
                "heightType": "A String", # Specifies how the height is measured.
                "antennaBeamwidth": 42, # 3-dB antenna beamwidth of the antenna in the horizontal-plane in
                    # degrees.  This parameter is an unsigned integer having a value
                    # between 0 and 360 (degrees) inclusive; it is optional for
                    # Category A devices and conditional for Category B devices.
                "antennaAzimuth": 42, # Boresight direction of the horizontal plane of the antenna in
                    # degrees with respect to true north. The value of this parameter
                    # is an integer with a value between 0 and 359 inclusive. A value
                    # of 0 degrees means true north; a value of 90 degrees means
                    # east. This parameter is optional for Category A devices and
                    # conditional for Category B devices.
              },
              "isSigned": True or False, # Output-only. Whether the configuration has been signed by a CPI.
              "updateTime": "A String", # Output-only. The last time the device configuration was edited.
              "measurementCapabilities": [ # Measurement reporting capabilities of the device.
                "A String",
              ],
              "state": "A String", # State of the configuration.
              "airInterface": { # Information about the device's air interface. # Information about this device's air interface.
                "supportedSpec": "A String", # This field is related to the radioTechnology field and provides the air
                    # interface specification that the CBSD is compliant with at the time of
                    # registration.
                    #
                    # Optional
                "radioTechnology": "A String", # This field specifies the radio access technology that is used for the CBSD.
                    #
                    # Conditional
              },
              "category": "A String", # FCC category of the device.
              "callSign": "A String", # The call sign of the device operator.
              "model": { # Information about the model of the device. # Information about this device model.
                "softwareVersion": "A String", # The software version of the device.
                "firmwareVersion": "A String", # The firmware version of the device.
                "hardwareVersion": "A String", # The hardware version of the device.
                "vendor": "A String", # The name of the device vendor.
                "name": "A String", # The name of the device model.
              },
            },
            "fccId": "A String", # The FCC identifier of the device.
            "grants": [ # Output only. Grants held by the device.
              { # Device grant. It is an authorization provided by the Spectrum
                  # Access System to a device to transmit using specified operating
                  # parameters after a successful heartbeat by the device.
                "moveList": [ # The DPA move lists on which this grant appears.
                  { # An entry in a DPA's move list.
                    "frequencyRange": { # Frequency range from `low_frequency` to `high_frequency`. # The frequency range that the move list affects.
                      "lowFrequencyMhz": 3.14, # The lowest frequency of the frequency range in MHz.
                      "highFrequencyMhz": 3.14, # The highest frequency of the frequency range in MHz.
                    },
                    "dpaId": "A String", # The ID of the DPA.
                  },
                ],
                "suspensionReason": [ # If the grant is suspended, the reason(s) for suspension.
                  "A String",
                ],
                "channelType": "A String", # Type of channel used.
                "maxEirp": 3.14, # Maximum Equivalent Isotropically Radiated Power (EIRP) permitted
                    # by the grant. The maximum EIRP is in units of dBm/MHz. The
                    # value of maxEirp represents the average (RMS) EIRP that would be
                    # measured by the procedure defined in FCC part 96.41(e)(3).
                "state": "A String", # State of the grant.
                "expireTime": "A String", # The expiration time of the grant.
                "frequencyRange": { # Frequency range from `low_frequency` to `high_frequency`. # The transmission frequency range.
                  "lowFrequencyMhz": 3.14, # The lowest frequency of the frequency range in MHz.
                  "highFrequencyMhz": 3.14, # The highest frequency of the frequency range in MHz.
                },
              },
            ],
            "serialNumber": "A String", # A serial number assigned to the device by the device
                # manufacturer.
            "state": "A String", # Output only. Device state.
            "displayName": "A String", # Device display name.
          },
        ],
      }

`create(parent, body=None, x__xgafv=None)`

    Creates a device under a node or customer.

    Args:
      parent: string, Required. The name of the parent resource. (required)
      body: object, The request body.
        The object takes the form of:

    {
      "name": "A String", # Output only. The resource path name.
      "preloadedConfig": { # Information about the device configuration. # Configuration of the device, as specified via SAS Portal API.
        "userId": "A String", # The identifier of a device user.
        "installationParams": { # Information about the device installation parameters. # Installation parameters for the device.
          "cpeCbsdIndication": True or False, # If present, this parameter specifies whether the CBSD is a CPE-CBSD or not.
          "antennaModel": "A String", # If an external antenna is used, the antenna model is optionally
              # provided in this field. The string has a maximum length of 128
              # octets.
          "verticalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
              # antenna vertical location. This optional parameter should only be
              # present if its value is less than the FCC requirement of 3
              # meters.
          "longitude": 3.14, # Longitude of the device antenna location. in degrees relative to
              # the WGS 84 datum. The allowed range is from -180.000000 to
              # +180.000000. Positive values represent longitudes east of the
              # prime meridian; negative values west of the prime
              # meridian.
          "indoorDeployment": True or False, # Whether the device antenna is indoor or not. True: indoor. False:
              # outdoor.
          "horizontalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
              # antenna horizontal location. This optional parameter should only
              # be present if its value is less than the FCC requirement of 50
              # meters.
          "eirpCapability": 42, # This parameter is the maximum device EIRP in units of dBm/10MHz
              # and is an integer with a value between -127 and +47 (dBm/10 MHz)
              # inclusive. If not included, SAS interprets it as maximum
              # allowable EIRP in units of dBm/10MHz for device category.
          "antennaDowntilt": 42, # Antenna downtilt in degrees and is an integer with a value
              # between -90 and +90 inclusive; a negative value means the antenna
              # is tilted up (above horizontal). This parameter is optional for
              # Category A devices and conditional for Category B devices.
          "latitude": 3.14, # Latitude of the device antenna location in degrees relative to
              # the WGS 84 datum. The allowed range is from -90.000000 to
              # +90.000000. Positive values represent latitudes north of the
              # equator; negative values south of the equator.
          "height": 3.14, # Device antenna height in meters. When the heightType parameter
              # value is "AGL", the antenna height should be given relative to
              # ground level. When the heightType parameter value is "AMSL", it
              # is given with respect to WGS84 datum.
          "antennaGain": 42, # Peak antenna gain in dBi. This parameter is an integer with a
              # value between -127 and +128 (dBi) inclusive.
          "heightType": "A String", # Specifies how the height is measured.
          "antennaBeamwidth": 42, # 3-dB antenna beamwidth of the antenna in the horizontal-plane in
              # degrees.  This parameter is an unsigned integer having a value
              # between 0 and 360 (degrees) inclusive; it is optional for
              # Category A devices and conditional for Category B devices.
          "antennaAzimuth": 42, # Boresight direction of the horizontal plane of the antenna in
              # degrees with respect to true north. The value of this parameter
              # is an integer with a value between 0 and 359 inclusive. A value
              # of 0 degrees means true north; a value of 90 degrees means
              # east. This parameter is optional for Category A devices and
              # conditional for Category B devices.
        },
        "isSigned": True or False, # Output-only. Whether the configuration has been signed by a CPI.
        "updateTime": "A String", # Output-only. The last time the device configuration was edited.
        "measurementCapabilities": [ # Measurement reporting capabilities of the device.
          "A String",
        ],
        "state": "A String", # State of the configuration.
        "airInterface": { # Information about the device's air interface. # Information about this device's air interface.
          "supportedSpec": "A String", # This field is related to the radioTechnology field and provides the air
              # interface specification that the CBSD is compliant with at the time of
              # registration.
              #
              # Optional
          "radioTechnology": "A String", # This field specifies the radio access technology that is used for the CBSD.
              #
              # Conditional
        },
        "category": "A String", # FCC category of the device.
        "callSign": "A String", # The call sign of the device operator.
        "model": { # Information about the model of the device. # Information about this device model.
          "softwareVersion": "A String", # The software version of the device.
          "firmwareVersion": "A String", # The firmware version of the device.
          "hardwareVersion": "A String", # The hardware version of the device.
          "vendor": "A String", # The name of the device vendor.
          "name": "A String", # The name of the device model.
        },
      },
      "activeConfig": { # Information about the device configuration. # Output only. Current configuration of the device as registered to the SAS.
        "userId": "A String", # The identifier of a device user.
        "installationParams": { # Information about the device installation parameters. # Installation parameters for the device.
          "cpeCbsdIndication": True or False, # If present, this parameter specifies whether the CBSD is a CPE-CBSD or not.
          "antennaModel": "A String", # If an external antenna is used, the antenna model is optionally
              # provided in this field. The string has a maximum length of 128
              # octets.
          "verticalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
              # antenna vertical location. This optional parameter should only be
              # present if its value is less than the FCC requirement of 3
              # meters.
          "longitude": 3.14, # Longitude of the device antenna location. in degrees relative to
              # the WGS 84 datum. The allowed range is from -180.000000 to
              # +180.000000. Positive values represent longitudes east of the
              # prime meridian; negative values west of the prime
              # meridian.
          "indoorDeployment": True or False, # Whether the device antenna is indoor or not. True: indoor. False:
              # outdoor.
          "horizontalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
              # antenna horizontal location. This optional parameter should only
              # be present if its value is less than the FCC requirement of 50
              # meters.
          "eirpCapability": 42, # This parameter is the maximum device EIRP in units of dBm/10MHz
              # and is an integer with a value between -127 and +47 (dBm/10 MHz)
              # inclusive. If not included, SAS interprets it as maximum
              # allowable EIRP in units of dBm/10MHz for device category.
          "antennaDowntilt": 42, # Antenna downtilt in degrees and is an integer with a value
              # between -90 and +90 inclusive; a negative value means the antenna
              # is tilted up (above horizontal). This parameter is optional for
              # Category A devices and conditional for Category B devices.
          "latitude": 3.14, # Latitude of the device antenna location in degrees relative to
              # the WGS 84 datum. The allowed range is from -90.000000 to
              # +90.000000. Positive values represent latitudes north of the
              # equator; negative values south of the equator.
          "height": 3.14, # Device antenna height in meters. When the heightType parameter
              # value is "AGL", the antenna height should be given relative to
              # ground level. When the heightType parameter value is "AMSL", it
              # is given with respect to WGS84 datum.
          "antennaGain": 42, # Peak antenna gain in dBi. This parameter is an integer with a
              # value between -127 and +128 (dBi) inclusive.
          "heightType": "A String", # Specifies how the height is measured.
          "antennaBeamwidth": 42, # 3-dB antenna beamwidth of the antenna in the horizontal-plane in
              # degrees.  This parameter is an unsigned integer having a value
              # between 0 and 360 (degrees) inclusive; it is optional for
              # Category A devices and conditional for Category B devices.
          "antennaAzimuth": 42, # Boresight direction of the horizontal plane of the antenna in
              # degrees with respect to true north. The value of this parameter
              # is an integer with a value between 0 and 359 inclusive. A value
              # of 0 degrees means true north; a value of 90 degrees means
              # east. This parameter is optional for Category A devices and
              # conditional for Category B devices.
        },
        "isSigned": True or False, # Output-only. Whether the configuration has been signed by a CPI.
        "updateTime": "A String", # Output-only. The last time the device configuration was edited.
        "measurementCapabilities": [ # Measurement reporting capabilities of the device.
          "A String",
        ],
        "state": "A String", # State of the configuration.
        "airInterface": { # Information about the device's air interface. # Information about this device's air interface.
          "supportedSpec": "A String", # This field is related to the radioTechnology field and provides the air
              # interface specification that the CBSD is compliant with at the time of
              # registration.
              #
              # Optional
          "radioTechnology": "A String", # This field specifies the radio access technology that is used for the CBSD.
              #
              # Conditional
        },
        "category": "A String", # FCC category of the device.
        "callSign": "A String", # The call sign of the device operator.
        "model": { # Information about the model of the device. # Information about this device model.
          "softwareVersion": "A String", # The software version of the device.
          "firmwareVersion": "A String", # The firmware version of the device.
          "hardwareVersion": "A String", # The hardware version of the device.
          "vendor": "A String", # The name of the device vendor.
          "name": "A String", # The name of the device model.
        },
      },
      "fccId": "A String", # The FCC identifier of the device.
      "grants": [ # Output only. Grants held by the device.
        { # Device grant. It is an authorization provided by the Spectrum
            # Access System to a device to transmit using specified operating
            # parameters after a successful heartbeat by the device.
          "moveList": [ # The DPA move lists on which this grant appears.
            { # An entry in a DPA's move list.
              "frequencyRange": { # Frequency range from `low_frequency` to `high_frequency`. # The frequency range that the move list affects.
                "lowFrequencyMhz": 3.14, # The lowest frequency of the frequency range in MHz.
                "highFrequencyMhz": 3.14, # The highest frequency of the frequency range in MHz.
              },
              "dpaId": "A String", # The ID of the DPA.
            },
          ],
          "suspensionReason": [ # If the grant is suspended, the reason(s) for suspension.
            "A String",
          ],
          "channelType": "A String", # Type of channel used.
          "maxEirp": 3.14, # Maximum Equivalent Isotropically Radiated Power (EIRP) permitted
              # by the grant. The maximum EIRP is in units of dBm/MHz. The
              # value of maxEirp represents the average (RMS) EIRP that would be
              # measured by the procedure defined in FCC part 96.41(e)(3).
          "state": "A String", # State of the grant.
          "expireTime": "A String", # The expiration time of the grant.
          "frequencyRange": { # Frequency range from `low_frequency` to `high_frequency`. # The transmission frequency range.
            "lowFrequencyMhz": 3.14, # The lowest frequency of the frequency range in MHz.
            "highFrequencyMhz": 3.14, # The highest frequency of the frequency range in MHz.
          },
        },
      ],
      "serialNumber": "A String", # A serial number assigned to the device by the device
          # manufacturer.
      "state": "A String", # Output only. Device state.
      "displayName": "A String", # Device display name.
    }

      x__xgafv: string, V1 error format.
        Allowed values
          1 - v1 error format
          2 - v2 error format

    Returns:
      An object of the form:

        {
        "name": "A String", # Output only. The resource path name.
        "preloadedConfig": { # Information about the device configuration. # Configuration of the device, as specified via SAS Portal API.
          "userId": "A String", # The identifier of a device user.
          "installationParams": { # Information about the device installation parameters. # Installation parameters for the device.
            "cpeCbsdIndication": True or False, # If present, this parameter specifies whether the CBSD is a CPE-CBSD or not.
            "antennaModel": "A String", # If an external antenna is used, the antenna model is optionally
                # provided in this field. The string has a maximum length of 128
                # octets.
            "verticalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
                # antenna vertical location. This optional parameter should only be
                # present if its value is less than the FCC requirement of 3
                # meters.
            "longitude": 3.14, # Longitude of the device antenna location. in degrees relative to
                # the WGS 84 datum. The allowed range is from -180.000000 to
                # +180.000000. Positive values represent longitudes east of the
                # prime meridian; negative values west of the prime
                # meridian.
            "indoorDeployment": True or False, # Whether the device antenna is indoor or not. True: indoor. False:
                # outdoor.
            "horizontalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
                # antenna horizontal location. This optional parameter should only
                # be present if its value is less than the FCC requirement of 50
                # meters.
            "eirpCapability": 42, # This parameter is the maximum device EIRP in units of dBm/10MHz
                # and is an integer with a value between -127 and +47 (dBm/10 MHz)
                # inclusive. If not included, SAS interprets it as maximum
                # allowable EIRP in units of dBm/10MHz for device category.
            "antennaDowntilt": 42, # Antenna downtilt in degrees and is an integer with a value
                # between -90 and +90 inclusive; a negative value means the antenna
                # is tilted up (above horizontal). This parameter is optional for
                # Category A devices and conditional for Category B devices.
            "latitude": 3.14, # Latitude of the device antenna location in degrees relative to
                # the WGS 84 datum. The allowed range is from -90.000000 to
                # +90.000000. Positive values represent latitudes north of the
                # equator; negative values south of the equator.
            "height": 3.14, # Device antenna height in meters. When the heightType parameter
                # value is "AGL", the antenna height should be given relative to
                # ground level. When the heightType parameter value is "AMSL", it
                # is given with respect to WGS84 datum.
            "antennaGain": 42, # Peak antenna gain in dBi. This parameter is an integer with a
                # value between -127 and +128 (dBi) inclusive.
            "heightType": "A String", # Specifies how the height is measured.
            "antennaBeamwidth": 42, # 3-dB antenna beamwidth of the antenna in the horizontal-plane in
                # degrees.  This parameter is an unsigned integer having a value
                # between 0 and 360 (degrees) inclusive; it is optional for
                # Category A devices and conditional for Category B devices.
            "antennaAzimuth": 42, # Boresight direction of the horizontal plane of the antenna in
                # degrees with respect to true north. The value of this parameter
                # is an integer with a value between 0 and 359 inclusive. A value
                # of 0 degrees means true north; a value of 90 degrees means
                # east. This parameter is optional for Category A devices and
                # conditional for Category B devices.
          },
          "isSigned": True or False, # Output-only. Whether the configuration has been signed by a CPI.
          "updateTime": "A String", # Output-only. The last time the device configuration was edited.
          "measurementCapabilities": [ # Measurement reporting capabilities of the device.
            "A String",
          ],
          "state": "A String", # State of the configuration.
          "airInterface": { # Information about the device's air interface. # Information about this device's air interface.
            "supportedSpec": "A String", # This field is related to the radioTechnology field and provides the air
                # interface specification that the CBSD is compliant with at the time of
                # registration.
                #
                # Optional
            "radioTechnology": "A String", # This field specifies the radio access technology that is used for the CBSD.
                #
                # Conditional
          },
          "category": "A String", # FCC category of the device.
          "callSign": "A String", # The call sign of the device operator.
          "model": { # Information about the model of the device. # Information about this device model.
            "softwareVersion": "A String", # The software version of the device.
            "firmwareVersion": "A String", # The firmware version of the device.
            "hardwareVersion": "A String", # The hardware version of the device.
            "vendor": "A String", # The name of the device vendor.
            "name": "A String", # The name of the device model.
          },
        },
        "activeConfig": { # Information about the device configuration. # Output only. Current configuration of the device as registered to the SAS.
          "userId": "A String", # The identifier of a device user.
          "installationParams": { # Information about the device installation parameters. # Installation parameters for the device.
            "cpeCbsdIndication": True or False, # If present, this parameter specifies whether the CBSD is a CPE-CBSD or not.
            "antennaModel": "A String", # If an external antenna is used, the antenna model is optionally
                # provided in this field. The string has a maximum length of 128
                # octets.
            "verticalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
                # antenna vertical location. This optional parameter should only be
                # present if its value is less than the FCC requirement of 3
                # meters.
            "longitude": 3.14, # Longitude of the device antenna location. in degrees relative to
                # the WGS 84 datum. The allowed range is from -180.000000 to
                # +180.000000. Positive values represent longitudes east of the
                # prime meridian; negative values west of the prime
                # meridian.
            "indoorDeployment": True or False, # Whether the device antenna is indoor or not. True: indoor. False:
                # outdoor.
            "horizontalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
                # antenna horizontal location. This optional parameter should only
                # be present if its value is less than the FCC requirement of 50
                # meters.
            "eirpCapability": 42, # This parameter is the maximum device EIRP in units of dBm/10MHz
                # and is an integer with a value between -127 and +47 (dBm/10 MHz)
                # inclusive. If not included, SAS interprets it as maximum
                # allowable EIRP in units of dBm/10MHz for device category.
            "antennaDowntilt": 42, # Antenna downtilt in degrees and is an integer with a value
                # between -90 and +90 inclusive; a negative value means the antenna
                # is tilted up (above horizontal). This parameter is optional for
                # Category A devices and conditional for Category B devices.
            "latitude": 3.14, # Latitude of the device antenna location in degrees relative to
                # the WGS 84 datum. The allowed range is from -90.000000 to
                # +90.000000. Positive values represent latitudes north of the
                # equator; negative values south of the equator.
            "height": 3.14, # Device antenna height in meters. When the heightType parameter
                # value is "AGL", the antenna height should be given relative to
                # ground level. When the heightType parameter value is "AMSL", it
                # is given with respect to WGS84 datum.
            "antennaGain": 42, # Peak antenna gain in dBi. This parameter is an integer with a
                # value between -127 and +128 (dBi) inclusive.
            "heightType": "A String", # Specifies how the height is measured.
            "antennaBeamwidth": 42, # 3-dB antenna beamwidth of the antenna in the horizontal-plane in
                # degrees.  This parameter is an unsigned integer having a value
                # between 0 and 360 (degrees) inclusive; it is optional for
                # Category A devices and conditional for Category B devices.
            "antennaAzimuth": 42, # Boresight direction of the horizontal plane of the antenna in
                # degrees with respect to true north. The value of this parameter
                # is an integer with a value between 0 and 359 inclusive. A value
                # of 0 degrees means true north; a value of 90 degrees means
                # east. This parameter is optional for Category A devices and
                # conditional for Category B devices.
          },
          "isSigned": True or False, # Output-only. Whether the configuration has been signed by a CPI.
          "updateTime": "A String", # Output-only. The last time the device configuration was edited.
          "measurementCapabilities": [ # Measurement reporting capabilities of the device.
            "A String",
          ],
          "state": "A String", # State of the configuration.
          "airInterface": { # Information about the device's air interface. # Information about this device's air interface.
            "supportedSpec": "A String", # This field is related to the radioTechnology field and provides the air
                # interface specification that the CBSD is compliant with at the time of
                # registration.
                #
                # Optional
            "radioTechnology": "A String", # This field specifies the radio access technology that is used for the CBSD.
                #
                # Conditional
          },
          "category": "A String", # FCC category of the device.
          "callSign": "A String", # The call sign of the device operator.
          "model": { # Information about the model of the device. # Information about this device model.
            "softwareVersion": "A String", # The software version of the device.
            "firmwareVersion": "A String", # The firmware version of the device.
            "hardwareVersion": "A String", # The hardware version of the device.
            "vendor": "A String", # The name of the device vendor.
            "name": "A String", # The name of the device model.
          },
        },
        "fccId": "A String", # The FCC identifier of the device.
        "grants": [ # Output only. Grants held by the device.
          { # Device grant. It is an authorization provided by the Spectrum
              # Access System to a device to transmit using specified operating
              # parameters after a successful heartbeat by the device.
            "moveList": [ # The DPA move lists on which this grant appears.
              { # An entry in a DPA's move list.
                "frequencyRange": { # Frequency range from `low_frequency` to `high_frequency`. # The frequency range that the move list affects.
                  "lowFrequencyMhz": 3.14, # The lowest frequency of the frequency range in MHz.
                  "highFrequencyMhz": 3.14, # The highest frequency of the frequency range in MHz.
                },
                "dpaId": "A String", # The ID of the DPA.
              },
            ],
            "suspensionReason": [ # If the grant is suspended, the reason(s) for suspension.
              "A String",
            ],
            "channelType": "A String", # Type of channel used.
            "maxEirp": 3.14, # Maximum Equivalent Isotropically Radiated Power (EIRP) permitted
                # by the grant. The maximum EIRP is in units of dBm/MHz. The
                # value of maxEirp represents the average (RMS) EIRP that would be
                # measured by the procedure defined in FCC part 96.41(e)(3).
            "state": "A String", # State of the grant.
            "expireTime": "A String", # The expiration time of the grant.
            "frequencyRange": { # Frequency range from `low_frequency` to `high_frequency`. # The transmission frequency range.
              "lowFrequencyMhz": 3.14, # The lowest frequency of the frequency range in MHz.
              "highFrequencyMhz": 3.14, # The highest frequency of the frequency range in MHz.
            },
          },
        ],
        "serialNumber": "A String", # A serial number assigned to the device by the device
            # manufacturer.
        "state": "A String", # Output only. Device state.
        "displayName": "A String", # Device display name.
      }

`createSigned(parent, body=None, x__xgafv=None)`

    Creates a signed device under a
    node or customer.

    Args:
      parent: string, Required. The name of the parent resource. (required)
      body: object, The request body.
        The object takes the form of:

    { # Request for CreateSignedDevice method.
        "encodedDevice": "A String", # Required. JSON Web Token signed using a CPI private key. Payload
            # must be the JSON encoding of the [Device]. The user_id field must be set.
        "installerId": "A String", # Required. Unique installer id (cpiId) from the Certified Professional
            # Installers database.
      }

      x__xgafv: string, V1 error format.
        Allowed values
          1 - v1 error format
          2 - v2 error format

    Returns:
      An object of the form:

        {
        "name": "A String", # Output only. The resource path name.
        "preloadedConfig": { # Information about the device configuration. # Configuration of the device, as specified via SAS Portal API.
          "userId": "A String", # The identifier of a device user.
          "installationParams": { # Information about the device installation parameters. # Installation parameters for the device.
            "cpeCbsdIndication": True or False, # If present, this parameter specifies whether the CBSD is a CPE-CBSD or not.
            "antennaModel": "A String", # If an external antenna is used, the antenna model is optionally
                # provided in this field. The string has a maximum length of 128
                # octets.
            "verticalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
                # antenna vertical location. This optional parameter should only be
                # present if its value is less than the FCC requirement of 3
                # meters.
            "longitude": 3.14, # Longitude of the device antenna location. in degrees relative to
                # the WGS 84 datum. The allowed range is from -180.000000 to
                # +180.000000. Positive values represent longitudes east of the
                # prime meridian; negative values west of the prime
                # meridian.
            "indoorDeployment": True or False, # Whether the device antenna is indoor or not. True: indoor. False:
                # outdoor.
            "horizontalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
                # antenna horizontal location. This optional parameter should only
                # be present if its value is less than the FCC requirement of 50
                # meters.
            "eirpCapability": 42, # This parameter is the maximum device EIRP in units of dBm/10MHz
                # and is an integer with a value between -127 and +47 (dBm/10 MHz)
                # inclusive. If not included, SAS interprets it as maximum
                # allowable EIRP in units of dBm/10MHz for device category.
            "antennaDowntilt": 42, # Antenna downtilt in degrees and is an integer with a value
                # between -90 and +90 inclusive; a negative value means the antenna
                # is tilted up (above horizontal). This parameter is optional for
                # Category A devices and conditional for Category B devices.
            "latitude": 3.14, # Latitude of the device antenna location in degrees relative to
                # the WGS 84 datum. The allowed range is from -90.000000 to
                # +90.000000. Positive values represent latitudes north of the
                # equator; negative values south of the equator.
            "height": 3.14, # Device antenna height in meters. When the heightType parameter
                # value is "AGL", the antenna height should be given relative to
                # ground level. When the heightType parameter value is "AMSL", it
                # is given with respect to WGS84 datum.
            "antennaGain": 42, # Peak antenna gain in dBi. This parameter is an integer with a
                # value between -127 and +128 (dBi) inclusive.
            "heightType": "A String", # Specifies how the height is measured.
            "antennaBeamwidth": 42, # 3-dB antenna beamwidth of the antenna in the horizontal-plane in
                # degrees.  This parameter is an unsigned integer having a value
                # between 0 and 360 (degrees) inclusive; it is optional for
                # Category A devices and conditional for Category B devices.
            "antennaAzimuth": 42, # Boresight direction of the horizontal plane of the antenna in
                # degrees with respect to true north. The value of this parameter
                # is an integer with a value between 0 and 359 inclusive. A value
                # of 0 degrees means true north; a value of 90 degrees means
                # east. This parameter is optional for Category A devices and
                # conditional for Category B devices.
          },
          "isSigned": True or False, # Output-only. Whether the configuration has been signed by a CPI.
          "updateTime": "A String", # Output-only. The last time the device configuration was edited.
          "measurementCapabilities": [ # Measurement reporting capabilities of the device.
            "A String",
          ],
          "state": "A String", # State of the configuration.
          "airInterface": { # Information about the device's air interface. # Information about this device's air interface.
            "supportedSpec": "A String", # This field is related to the radioTechnology field and provides the air
                # interface specification that the CBSD is compliant with at the time of
                # registration.
                #
                # Optional
            "radioTechnology": "A String", # This field specifies the radio access technology that is used for the CBSD.
                #
                # Conditional
          },
          "category": "A String", # FCC category of the device.
          "callSign": "A String", # The call sign of the device operator.
          "model": { # Information about the model of the device. # Information about this device model.
            "softwareVersion": "A String", # The software version of the device.
            "firmwareVersion": "A String", # The firmware version of the device.
            "hardwareVersion": "A String", # The hardware version of the device.
            "vendor": "A String", # The name of the device vendor.
            "name": "A String", # The name of the device model.
          },
        },
        "activeConfig": { # Information about the device configuration. # Output only. Current configuration of the device as registered to the SAS.
          "userId": "A String", # The identifier of a device user.
          "installationParams": { # Information about the device installation parameters. # Installation parameters for the device.
            "cpeCbsdIndication": True or False, # If present, this parameter specifies whether the CBSD is a CPE-CBSD or not.
            "antennaModel": "A String", # If an external antenna is used, the antenna model is optionally
                # provided in this field. The string has a maximum length of 128
                # octets.
            "verticalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
                # antenna vertical location. This optional parameter should only be
                # present if its value is less than the FCC requirement of 3
                # meters.
            "longitude": 3.14, # Longitude of the device antenna location. in degrees relative to
                # the WGS 84 datum. The allowed range is from -180.000000 to
                # +180.000000. Positive values represent longitudes east of the
                # prime meridian; negative values west of the prime
                # meridian.
            "indoorDeployment": True or False, # Whether the device antenna is indoor or not. True: indoor. False:
                # outdoor.
            "horizontalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
                # antenna horizontal location. This optional parameter should only
                # be present if its value is less than the FCC requirement of 50
                # meters.
            "eirpCapability": 42, # This parameter is the maximum device EIRP in units of dBm/10MHz
                # and is an integer with a value between -127 and +47 (dBm/10 MHz)
                # inclusive. If not included, SAS interprets it as maximum
                # allowable EIRP in units of dBm/10MHz for device category.
            "antennaDowntilt": 42, # Antenna downtilt in degrees and is an integer with a value
                # between -90 and +90 inclusive; a negative value means the antenna
                # is tilted up (above horizontal). This parameter is optional for
                # Category A devices and conditional for Category B devices.
            "latitude": 3.14, # Latitude of the device antenna location in degrees relative to
                # the WGS 84 datum. The allowed range is from -90.000000 to
                # +90.000000. Positive values represent latitudes north of the
                # equator; negative values south of the equator.
            "height": 3.14, # Device antenna height in meters. When the heightType parameter
                # value is "AGL", the antenna height should be given relative to
                # ground level. When the heightType parameter value is "AMSL", it
                # is given with respect to WGS84 datum.
            "antennaGain": 42, # Peak antenna gain in dBi. This parameter is an integer with a
                # value between -127 and +128 (dBi) inclusive.
            "heightType": "A String", # Specifies how the height is measured.
            "antennaBeamwidth": 42, # 3-dB antenna beamwidth of the antenna in the horizontal-plane in
                # degrees.  This parameter is an unsigned integer having a value
                # between 0 and 360 (degrees) inclusive; it is optional for
                # Category A devices and conditional for Category B devices.
            "antennaAzimuth": 42, # Boresight direction of the horizontal plane of the antenna in
                # degrees with respect to true north. The value of this parameter
                # is an integer with a value between 0 and 359 inclusive. A value
                # of 0 degrees means true north; a value of 90 degrees means
                # east. This parameter is optional for Category A devices and
                # conditional for Category B devices.
          },
          "isSigned": True or False, # Output-only. Whether the configuration has been signed by a CPI.
          "updateTime": "A String", # Output-only. The last time the device configuration was edited.
          "measurementCapabilities": [ # Measurement reporting capabilities of the device.
            "A String",
          ],
          "state": "A String", # State of the configuration.
          "airInterface": { # Information about the device's air interface. # Information about this device's air interface.
            "supportedSpec": "A String", # This field is related to the radioTechnology field and provides the air
                # interface specification that the CBSD is compliant with at the time of
                # registration.
                #
                # Optional
            "radioTechnology": "A String", # This field specifies the radio access technology that is used for the CBSD.
                #
                # Conditional
          },
          "category": "A String", # FCC category of the device.
          "callSign": "A String", # The call sign of the device operator.
          "model": { # Information about the model of the device. # Information about this device model.
            "softwareVersion": "A String", # The software version of the device.
            "firmwareVersion": "A String", # The firmware version of the device.
            "hardwareVersion": "A String", # The hardware version of the device.
            "vendor": "A String", # The name of the device vendor.
            "name": "A String", # The name of the device model.
          },
        },
        "fccId": "A String", # The FCC identifier of the device.
        "grants": [ # Output only. Grants held by the device.
          { # Device grant. It is an authorization provided by the Spectrum
              # Access System to a device to transmit using specified operating
              # parameters after a successful heartbeat by the device.
            "moveList": [ # The DPA move lists on which this grant appears.
              { # An entry in a DPA's move list.
                "frequencyRange": { # Frequency range from `low_frequency` to `high_frequency`. # The frequency range that the move list affects.
                  "lowFrequencyMhz": 3.14, # The lowest frequency of the frequency range in MHz.
                  "highFrequencyMhz": 3.14, # The highest frequency of the frequency range in MHz.
                },
                "dpaId": "A String", # The ID of the DPA.
              },
            ],
            "suspensionReason": [ # If the grant is suspended, the reason(s) for suspension.
              "A String",
            ],
            "channelType": "A String", # Type of channel used.
            "maxEirp": 3.14, # Maximum Equivalent Isotropically Radiated Power (EIRP) permitted
                # by the grant. The maximum EIRP is in units of dBm/MHz. The
                # value of maxEirp represents the average (RMS) EIRP that would be
                # measured by the procedure defined in FCC part 96.41(e)(3).
            "state": "A String", # State of the grant.
            "expireTime": "A String", # The expiration time of the grant.
            "frequencyRange": { # Frequency range from `low_frequency` to `high_frequency`. # The transmission frequency range.
              "lowFrequencyMhz": 3.14, # The lowest frequency of the frequency range in MHz.
              "highFrequencyMhz": 3.14, # The highest frequency of the frequency range in MHz.
            },
          },
        ],
        "serialNumber": "A String", # A serial number assigned to the device by the device
            # manufacturer.
        "state": "A String", # Output only. Device state.
        "displayName": "A String", # Device display name.
      }

`list(parent, filter=None, pageSize=None, pageToken=None, x__xgafv=None)`

    Lists devices under a node or customer.

    Args:
      parent: string, Required. The name of the parent resource. (required)
      filter: string, The filter expression. The filter should have one of the following
    formats: "sn=123454" or "display_name=MyDevice". sn
    corresponds to serial_number of the device. The filter is case insensitive.
      pageSize: integer, The maximum number of devices to return in the response.
    If empty or zero, all devices will be listed.
    Must be in the range [0, 1000].
      pageToken: string, A pagination token returned from a previous call to ListDevices
    that indicates where this listing should continue from.
      x__xgafv: string, V1 error format.
        Allowed values
          1 - v1 error format
          2 - v2 error format

    Returns:
      An object of the form:

        { # Response for ListDevices method.
        "devices": [ # The devices that match the request.
          {
            "name": "A String", # Output only. The resource path name.
            "preloadedConfig": { # Information about the device configuration. # Configuration of the device, as specified via SAS Portal API.
              "userId": "A String", # The identifier of a device user.
              "installationParams": { # Information about the device installation parameters. # Installation parameters for the device.
                "cpeCbsdIndication": True or False, # If present, this parameter specifies whether the CBSD is a CPE-CBSD or not.
                "antennaModel": "A String", # If an external antenna is used, the antenna model is optionally
                    # provided in this field. The string has a maximum length of 128
                    # octets.
                "verticalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
                    # antenna vertical location. This optional parameter should only be
                    # present if its value is less than the FCC requirement of 3
                    # meters.
                "longitude": 3.14, # Longitude of the device antenna location. in degrees relative to
                    # the WGS 84 datum. The allowed range is from -180.000000 to
                    # +180.000000. Positive values represent longitudes east of the
                    # prime meridian; negative values west of the prime
                    # meridian.
                "indoorDeployment": True or False, # Whether the device antenna is indoor or not. True: indoor. False:
                    # outdoor.
                "horizontalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
                    # antenna horizontal location. This optional parameter should only
                    # be present if its value is less than the FCC requirement of 50
                    # meters.
                "eirpCapability": 42, # This parameter is the maximum device EIRP in units of dBm/10MHz
                    # and is an integer with a value between -127 and +47 (dBm/10 MHz)
                    # inclusive. If not included, SAS interprets it as maximum
                    # allowable EIRP in units of dBm/10MHz for device category.
                "antennaDowntilt": 42, # Antenna downtilt in degrees and is an integer with a value
                    # between -90 and +90 inclusive; a negative value means the antenna
                    # is tilted up (above horizontal). This parameter is optional for
                    # Category A devices and conditional for Category B devices.
                "latitude": 3.14, # Latitude of the device antenna location in degrees relative to
                    # the WGS 84 datum. The allowed range is from -90.000000 to
                    # +90.000000. Positive values represent latitudes north of the
                    # equator; negative values south of the equator.
                "height": 3.14, # Device antenna height in meters. When the heightType parameter
                    # value is "AGL", the antenna height should be given relative to
                    # ground level. When the heightType parameter value is "AMSL", it
                    # is given with respect to WGS84 datum.
                "antennaGain": 42, # Peak antenna gain in dBi. This parameter is an integer with a
                    # value between -127 and +128 (dBi) inclusive.
                "heightType": "A String", # Specifies how the height is measured.
                "antennaBeamwidth": 42, # 3-dB antenna beamwidth of the antenna in the horizontal-plane in
                    # degrees.  This parameter is an unsigned integer having a value
                    # between 0 and 360 (degrees) inclusive; it is optional for
                    # Category A devices and conditional for Category B devices.
                "antennaAzimuth": 42, # Boresight direction of the horizontal plane of the antenna in
                    # degrees with respect to true north. The value of this parameter
                    # is an integer with a value between 0 and 359 inclusive. A value
                    # of 0 degrees means true north; a value of 90 degrees means
                    # east. This parameter is optional for Category A devices and
                    # conditional for Category B devices.
              },
              "isSigned": True or False, # Output-only. Whether the configuration has been signed by a CPI.
              "updateTime": "A String", # Output-only. The last time the device configuration was edited.
              "measurementCapabilities": [ # Measurement reporting capabilities of the device.
                "A String",
              ],
              "state": "A String", # State of the configuration.
              "airInterface": { # Information about the device's air interface. # Information about this device's air interface.
                "supportedSpec": "A String", # This field is related to the radioTechnology field and provides the air
                    # interface specification that the CBSD is compliant with at the time of
                    # registration.
                    #
                    # Optional
                "radioTechnology": "A String", # This field specifies the radio access technology that is used for the CBSD.
                    #
                    # Conditional
              },
              "category": "A String", # FCC category of the device.
              "callSign": "A String", # The call sign of the device operator.
              "model": { # Information about the model of the device. # Information about this device model.
                "softwareVersion": "A String", # The software version of the device.
                "firmwareVersion": "A String", # The firmware version of the device.
                "hardwareVersion": "A String", # The hardware version of the device.
                "vendor": "A String", # The name of the device vendor.
                "name": "A String", # The name of the device model.
              },
            },
            "activeConfig": { # Information about the device configuration. # Output only. Current configuration of the device as registered to the SAS.
              "userId": "A String", # The identifier of a device user.
              "installationParams": { # Information about the device installation parameters. # Installation parameters for the device.
                "cpeCbsdIndication": True or False, # If present, this parameter specifies whether the CBSD is a CPE-CBSD or not.
                "antennaModel": "A String", # If an external antenna is used, the antenna model is optionally
                    # provided in this field. The string has a maximum length of 128
                    # octets.
                "verticalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
                    # antenna vertical location. This optional parameter should only be
                    # present if its value is less than the FCC requirement of 3
                    # meters.
                "longitude": 3.14, # Longitude of the device antenna location. in degrees relative to
                    # the WGS 84 datum. The allowed range is from -180.000000 to
                    # +180.000000. Positive values represent longitudes east of the
                    # prime meridian; negative values west of the prime
                    # meridian.
                "indoorDeployment": True or False, # Whether the device antenna is indoor or not. True: indoor. False:
                    # outdoor.
                "horizontalAccuracy": 3.14, # A positive number in meters to indicate accuracy of the device
                    # antenna horizontal location. This optional parameter should only
                    # be present if its value is less than the FCC requirement of 50
                    # meters.
                "eirpCapability": 42, # This parameter is the maximum device EIRP in units of dBm/10MHz
                    # and is an integer with a value between -127 and +47 (dBm/10 MHz)
                    # inclusive. If not included, SAS interprets it as maximum
                    # allowable EIRP in units of dBm/10MHz for device category.
                "antennaDowntilt": 42, # Antenna downtilt in degrees and is an integer with a value
                    # between -90 and +90 inclusive; a negative value means the antenna
                    # is tilted up (above horizontal). This parameter is optional for
                    # Category A devices and conditional for Category B devices.
                "latitude": 3.14, # Latitude of the device antenna location in degrees relative to
                    # the WGS 84 datum. The allowed range is from -90.000000 to
                    # +90.000000. Positive values represent latitudes north of the
                    # equator; negative values south of the equator.
                "height": 3.14, # Device antenna height in meters. When the heightType parameter
                    # value is "AGL", the antenna height should be given relative to
                    # ground level. When the heightType parameter value is "AMSL", it
                    # is given with respect to WGS84 datum.
                "antennaGain": 42, # Peak antenna gain in dBi. This parameter is an integer with a
                    # value between -127 and +128 (dBi) inclusive.
                "heightType": "A String", # Specifies how the height is measured.
                "antennaBeamwidth": 42, # 3-dB antenna beamwidth of the antenna in the horizontal-plane in
                    # degrees.  This parameter is an unsigned integer having a value
                    # between 0 and 360 (degrees) inclusive; it is optional for
                    # Category A devices and conditional for Category B devices.
                "antennaAzimuth": 42, # Boresight direction of the horizontal plane of the antenna in
                    # degrees with respect to true north. The value of this parameter
                    # is an integer with a value between 0 and 359 inclusive. A value
                    # of 0 degrees means true north; a value of 90 degrees means
                    # east. This parameter is optional for Category A devices and
                    # conditional for Category B devices.
              },
              "isSigned": True or False, # Output-only. Whether the configuration has been signed by a CPI.
              "updateTime": "A String", # Output-only. The last time the device configuration was edited.
              "measurementCapabilities": [ # Measurement reporting capabilities of the device.
                "A String",
              ],
              "state": "A String", # State of the configuration.
              "airInterface": { # Information about the device's air interface. # Information about this device's air interface.
                "supportedSpec": "A String", # This field is related to the radioTechnology field and provides the air
                    # interface specification that the CBSD is compliant with at the time of
                    # registration.
                    #
                    # Optional
                "radioTechnology": "A String", # This field specifies the radio access technology that is used for the CBSD.
                    #
                    # Conditional
              },
              "category": "A String", # FCC category of the device.
              "callSign": "A String", # The call sign of the device operator.
              "model": { # Information about the model of the device. # Information about this device model.
                "softwareVersion": "A String", # The software version of the device.
                "firmwareVersion": "A String", # The firmware version of the device.
                "hardwareVersion": "A String", # The hardware version of the device.
                "vendor": "A String", # The name of the device vendor.
                "name": "A String", # The name of the device model.
              },
            },
            "fccId": "A String", # The FCC identifier of the device.
            "grants": [ # Output only. Grants held by the device.
              { # Device grant. It is an authorization provided by the Spectrum
                  # Access System to a device to transmit using specified operating
                  # parameters after a successful heartbeat by the device.
                "moveList": [ # The DPA move lists on which this grant appears.
                  { # An entry in a DPA's move list.
                    "frequencyRange": { # Frequency range from `low_frequency` to `high_frequency`. # The frequency range that the move list affects.
                      "lowFrequencyMhz": 3.14, # The lowest frequency of the frequency range in MHz.
                      "highFrequencyMhz": 3.14, # The highest frequency of the frequency range in MHz.
                    },
                    "dpaId": "A String", # The ID of the DPA.
                  },
                ],
                "suspensionReason": [ # If the grant is suspended, the reason(s) for suspension.
                  "A String",
                ],
                "channelType": "A String", # Type of channel used.
                "maxEirp": 3.14, # Maximum Equivalent Isotropically Radiated Power (EIRP) permitted
                    # by the grant. The maximum EIRP is in units of dBm/MHz. The
                    # value of maxEirp represents the average (RMS) EIRP that would be
                    # measured by the procedure defined in FCC part 96.41(e)(3).
                "state": "A String", # State of the grant.
                "expireTime": "A String", # The expiration time of the grant.
                "frequencyRange": { # Frequency range from `low_frequency` to `high_frequency`. # The transmission frequency range.
                  "lowFrequencyMhz": 3.14, # The lowest frequency of the frequency range in MHz.
                  "highFrequencyMhz": 3.14, # The highest frequency of the frequency range in MHz.
                },
              },
            ],
            "serialNumber": "A String", # A serial number assigned to the device by the device
                # manufacturer.
            "state": "A String", # Output only. Device state.
            "displayName": "A String", # Device display name.
          },
        ],
        "nextPageToken": "A String", # A pagination token returned from a previous call to ListDevices method
            # that indicates from where listing should continue. If the field
            # is missing or empty, it means there is no more devices.
      }

`list_next(previous_request, previous_response)`

    Retrieves the next page of results.

    Args:
      previous_request: The request for the previous page. (required)
      previous_response: The response from the request for the previous page. (required)

    Returns:
      A request object that you can call 'execute()' on to request the next
      page. Returns None if there are no more items in the collection.