

# V1alpha1LimitedPriorityLevelConfiguration

LimitedPriorityLevelConfiguration specifies how to handle requests that are subject to limits. It addresses two issues:  * How are requests for this priority level limited?  * What should be done with requests that exceed the limit?
## Properties

Name | Type | Description | Notes
------------ | ------------- | ------------- | -------------
**assuredConcurrencyShares** | **Integer** | &#x60;assuredConcurrencyShares&#x60; (ACS) configures the execution limit, which is a limit on the number of requests of this priority level that may be exeucting at a given time.  ACS must be a positive number. The server&#39;s concurrency limit (SCL) is divided among the concurrency-controlled priority levels in proportion to their assured concurrency shares. This produces the assured concurrency value (ACV) --- the number of requests that may be executing at a time --- for each such priority level:              ACV(l) &#x3D; ceil( SCL * ACS(l) / ( sum[priority levels k] ACS(k) ) )  bigger numbers of ACS mean more reserved concurrent requests (at the expense of every other PL). This field has a default value of 30. |  [optional]
**limitResponse** | [**V1alpha1LimitResponse**](V1alpha1LimitResponse.md) |  |  [optional]



