:mod:`sys` -- system specific functions
=======================================

.. include:: ../templates/unsupported_in_circuitpython.inc

.. module:: sys
   :synopsis: system specific functions

|see_cpython_module| :mod:`cpython:sys`.

Functions
---------

.. function:: exit(retval=0)

   Terminate current program with a given exit code. Underlyingly, this
   function raise as `SystemExit` exception. If an argument is given, its
   value given as an argument to `SystemExit`.

.. function:: print_exception(exc, file=sys.stdout)

   Print exception with a traceback to a file-like object *file* (or
   `sys.stdout` by default).

   .. admonition:: Difference to CPython
      :class: attention

      This is simplified version of a function which appears in the
      ``traceback`` module in CPython. Unlike ``traceback.print_exception()``,
      this function takes just exception value instead of exception type,
      exception value, and traceback object; *file* argument should be
      positional; further arguments are not supported.

Constants
---------

.. data:: argv

   A mutable list of arguments the current program was started with.

.. data:: byteorder

   The byte order of the system (``"little"`` or ``"big"``).

.. data:: implementation

   Object with information about the current Python implementation. For
   CircuitPython, it has following attributes:

   * *name* - string "circuitpython"
   * *version* - tuple (major, minor, micro), e.g. (1, 7, 0)

   This object is the recommended way to distinguish CircuitPython from other
   Python implementations (note that it still may not exist in the very
   minimal ports).

   .. admonition:: Difference to CPython
      :class: attention

      CPython mandates more attributes for this object, but the actual useful
      bare minimum is implemented in CircuitPython.

.. data:: maxsize

   Maximum value which a native integer type can hold on the current platform,
   or maximum value representable by CircuitPython integer type, if it's smaller
   than platform max value (that is the case for CircuitPython ports without
   long int support).

   This attribute is useful for detecting "bitness" of a platform (32-bit vs
   64-bit, etc.). It's recommended to not compare this attribute to some
   value directly, but instead count number of bits in it::

    bits = 0
    v = sys.maxsize
    while v:
        bits += 1
        v >>= 1
    if bits > 32:
        # 64-bit (or more) platform
        ...
    else:
        # 32-bit (or less) platform
        # Note that on 32-bit platform, value of bits may be less than 32
        # (e.g. 31) due to peculiarities described above, so use "> 16",
        # "> 32", "> 64" style of comparisons.

.. data:: modules

   Dictionary of loaded modules. On some ports, it may not include builtin
   modules.

.. data:: path

   A mutable list of directories to search for imported modules.

.. data:: platform

   The platform that CircuitPython is running on. For OS/RTOS ports, this is
   usually an identifier of the OS, e.g. ``"linux"``. For baremetal ports it
   is an identifier of the chip on a board, e.g. ``"MicroChip SAMD51"``.
   It thus can be used to distinguish one board from another.
   If you need to check whether your program runs on CircuitPython (vs other
   Python implementation), use `sys.implementation` instead.

.. data:: stderr

   Standard error stream.

.. data:: stdin

   Standard input stream.

.. data:: stdout

   Standard output stream.

.. data:: version

   Python language version that this implementation conforms to, as a string.

.. data:: version_info

   Python language version that this implementation conforms to, as a tuple of ints.
