# Compute Engine API . interconnectAttachments

## Instance Methods

Retrieves an aggregated list of interconnect attachments.

Retrieves the next page of results.

Close httplib2 connections.

Deletes the specified interconnect attachment.

Returns the specified interconnect attachment.

Gets the access control policy for a resource. May be empty if no such policy or resource exists.

Creates an InterconnectAttachment in the specified project using the data included in the request.

Retrieves the list of interconnect attachments contained within the specified region.

Retrieves the next page of results.

Updates the specified interconnect attachment with the data included in the request. This method supports PATCH semantics and uses the JSON merge patch format and processing rules.

Sets the access control policy on the specified resource. Replaces any existing policy.

Sets the labels on an InterconnectAttachment. To learn more about labels, read the Labeling Resources documentation.

Returns permissions that a caller has on the specified resource.

### Method Details

`aggregatedList(project, filter=None, includeAllScopes=None, maxResults=None, orderBy=None, pageToken=None, returnPartialSuccess=None, x__xgafv=None)`

    Retrieves an aggregated list of interconnect attachments.

    Args:
      project: string, Project ID for this request. (required)
      filter: string, A filter expression that filters resources listed in the response. The expression must specify the field name, a comparison operator, and the value that you want to use for filtering. The value must be a string, a number, or a boolean. The comparison operator must be either `=`, `!=`, `>`, or `<`. For example, if you are filtering Compute Engine instances, you can exclude instances named `example-instance` by specifying `name != example-instance`. You can also filter nested fields. For example, you could specify `scheduling.automaticRestart = false` to include instances only if they are not scheduled for automatic restarts. You can use filtering on nested fields to filter based on resource labels. To filter on multiple expressions, provide each separate expression within parentheses. For example: ``` (scheduling.automaticRestart = true) (cpuPlatform = "Intel Skylake") ``` By default, each expression is an `AND` expression. However, you can include `AND` and `OR` expressions explicitly. For example: ``` (cpuPlatform = "Intel Skylake") OR (cpuPlatform = "Intel Broadwell") AND (scheduling.automaticRestart = true) ```
      includeAllScopes: boolean, Indicates whether every visible scope for each scope type (zone, region, global) should be included in the response. For new resource types added after this field, the flag has no effect as new resource types will always include every visible scope for each scope type in response. For resource types which predate this field, if this flag is omitted or false, only scopes of the scope types where the resource type is expected to be found will be included.
      maxResults: integer, The maximum number of results per page that should be returned. If the number of available results is larger than `maxResults`, Compute Engine returns a `nextPageToken` that can be used to get the next page of results in subsequent list requests. Acceptable values are `0` to `500`, inclusive. (Default: `500`)
      orderBy: string, Sorts list results by a certain order. By default, results are returned in alphanumerical order based on the resource name. You can also sort results in descending order based on the creation timestamp using `orderBy="creationTimestamp desc"`. This sorts results based on the `creationTimestamp` field in reverse chronological order (newest result first). Use this to sort resources like operations so that the newest operation is returned first. Currently, only sorting by `name` or `creationTimestamp desc` is supported.
      pageToken: string, Specifies a page token to use. Set `pageToken` to the `nextPageToken` returned by a previous list request to get the next page of results.
      returnPartialSuccess: boolean, Opt-in for partial success behavior which provides partial results in case of failure. The default value is false.
      x__xgafv: string, V1 error format.
        Allowed values
          1 - v1 error format
          2 - v2 error format

    Returns:
      An object of the form:

        {
      "id": "A String", # [Output Only] Unique identifier for the resource; defined by the server.
      "items": { # A list of InterconnectAttachmentsScopedList resources.
        "a_key": { # Name of the scope containing this set of interconnect attachments.
          "interconnectAttachments": [ # A list of interconnect attachments contained in this scope.
            { # Represents an Interconnect Attachment (VLAN) resource. You can use Interconnect attachments (VLANS) to connect your Virtual Private Cloud networks to your on-premises networks through an Interconnect. For more information, read Creating VLAN Attachments.
              "adminEnabled": True or False, # Determines whether this Attachment will carry packets. Not present for PARTNER_PROVIDER.
              "bandwidth": "A String", # Provisioned bandwidth capacity for the interconnect attachment. For attachments of type DEDICATED, the user can set the bandwidth. For attachments of type PARTNER, the Google Partner that is operating the interconnect must set the bandwidth. Output only for PARTNER type, mutable for PARTNER_PROVIDER and DEDICATED, and can take one of the following values: - BPS_50M: 50 Mbit/s - BPS_100M: 100 Mbit/s - BPS_200M: 200 Mbit/s - BPS_300M: 300 Mbit/s - BPS_400M: 400 Mbit/s - BPS_500M: 500 Mbit/s - BPS_1G: 1 Gbit/s - BPS_2G: 2 Gbit/s - BPS_5G: 5 Gbit/s - BPS_10G: 10 Gbit/s - BPS_20G: 20 Gbit/s - BPS_50G: 50 Gbit/s
              "candidateIpv6Subnets": [ # Up to 16 candidate prefixes that control the allocation of cloudRouterIpv6Address and customerRouterIpv6Address for this attachment. Each prefix must be in the Global Unique Address (GUA) space. It is highly recommended that it be in a range owned by the requestor. A GUA in a range owned by Google will cause the request to fail. Google will select an available prefix from the supplied candidates or fail the request. If not supplied, a /125 from a Google-owned GUA block will be selected.
                "A String",
              ],
              "candidateSubnets": [ # Up to 16 candidate prefixes that can be used to restrict the allocation of cloudRouterIpAddress and customerRouterIpAddress for this attachment. All prefixes must be within link-local address space (169.254.0.0/16) and must be /29 or shorter (/28, /27, etc). Google will attempt to select an unused /29 from the supplied candidate prefix(es). The request will fail if all possible /29s are in use on Google's edge. If not supplied, Google will randomly select an unused /29 from all of link-local space.
                "A String",
              ],
              "cloudRouterIpAddress": "A String", # [Output Only] IPv4 address + prefix length to be configured on Cloud Router Interface for this interconnect attachment.
              "cloudRouterIpv6Address": "A String", # [Output Only] IPv6 address + prefix length to be configured on Cloud Router Interface for this interconnect attachment.
              "cloudRouterIpv6InterfaceId": "A String", # If supplied, the interface id (index within the subnet) to be used for the cloud router address. The id must be in the range of 1 to 6. If a subnet mask is supplied, it must be /125, and the subnet should either be 0 or match the selected subnet.
              "creationTimestamp": "A String", # [Output Only] Creation timestamp in RFC3339 text format.
              "customerRouterIpAddress": "A String", # [Output Only] IPv4 address + prefix length to be configured on the customer router subinterface for this interconnect attachment.
              "customerRouterIpv6Address": "A String", # [Output Only] IPv6 address + prefix length to be configured on the customer router subinterface for this interconnect attachment.
              "customerRouterIpv6InterfaceId": "A String", # If supplied, the interface id (index within the subnet) to be used for the customer router address. The id must be in the range of 1 to 6. If a subnet mask is supplied, it must be /125, and the subnet should either be 0 or match the selected subnet.
              "dataplaneVersion": 42, # [Output Only] Dataplane version for this InterconnectAttachment.
              "description": "A String", # An optional description of this resource.
              "edgeAvailabilityDomain": "A String", # Desired availability domain for the attachment. Only available for type PARTNER, at creation time, and can take one of the following values: - AVAILABILITY_DOMAIN_ANY - AVAILABILITY_DOMAIN_1 - AVAILABILITY_DOMAIN_2 For improved reliability, customers should configure a pair of attachments, one per availability domain. The selected availability domain will be provided to the Partner via the pairing key, so that the provisioned circuit will lie in the specified domain. If not specified, the value will default to AVAILABILITY_DOMAIN_ANY.
              "encryption": "A String", # Indicates the user-supplied encryption option of this VLAN attachment (interconnectAttachment). Can only be specified at attachment creation for PARTNER or DEDICATED attachments. Possible values are: - NONE - This is the default value, which means that the VLAN attachment carries unencrypted traffic. VMs are able to send traffic to, or receive traffic from, such a VLAN attachment. - IPSEC - The VLAN attachment carries only encrypted traffic that is encrypted by an IPsec device, such as an HA VPN gateway or third-party IPsec VPN. VMs cannot directly send traffic to, or receive traffic from, such a VLAN attachment. To use *IPsec-encrypted Cloud Interconnect*, the VLAN attachment must be created with this option. Not currently available publicly.
              "googleReferenceId": "A String", # [Output Only] Google reference ID, to be used when raising support tickets with Google or otherwise to debug backend connectivity issues. [Deprecated] This field is not used.
              "id": "A String", # [Output Only] The unique identifier for the resource. This identifier is defined by the server.
              "interconnect": "A String", # URL of the underlying Interconnect object that this attachment's traffic will traverse through.
              "ipsecInternalAddresses": [ # A list of URLs of addresses that have been reserved for the VLAN attachment. Used only for the VLAN attachment that has the encryption option as IPSEC. The addresses must be regional internal IP address ranges. When creating an HA VPN gateway over the VLAN attachment, if the attachment is configured to use a regional internal IP address, then the VPN gateway's IP address is allocated from the IP address range specified here. For example, if the HA VPN gateway's interface 0 is paired to this VLAN attachment, then a regional internal IP address for the VPN gateway interface 0 will be allocated from the IP address specified for this VLAN attachment. If this field is not specified when creating the VLAN attachment, then later on when creating an HA VPN gateway on this VLAN attachment, the HA VPN gateway's IP address is allocated from the regional external IP address pool. Not currently available publicly.
                "A String",
              ],
              "kind": "compute#interconnectAttachment", # [Output Only] Type of the resource. Always compute#interconnectAttachment for interconnect attachments.
              "labelFingerprint": "A String", # A fingerprint for the labels being applied to this InterconnectAttachment, which is essentially a hash of the labels set used for optimistic locking. The fingerprint is initially generated by Compute Engine and changes after every request to modify or update labels. You must always provide an up-to-date fingerprint hash in order to update or change labels, otherwise the request will fail with error 412 conditionNotMet. To see the latest fingerprint, make a get() request to retrieve an InterconnectAttachment.
              "labels": { # Labels for this resource. These can only be added or modified by the setLabels method. Each label key/value pair must comply with RFC1035. Label values may be empty.
                "a_key": "A String",
              },
              "mtu": 42, # Maximum Transmission Unit (MTU), in bytes, of packets passing through this interconnect attachment. Only 1440 and 1500 are allowed. If not specified, the value will default to 1440.
              "name": "A String", # Name of the resource. Provided by the client when the resource is created. The name must be 1-63 characters long, and comply with RFC1035. Specifically, the name must be 1-63 characters long and match the regular expression `[a-z]([-a-z0-9]*[a-z0-9])?` which means the first character must be a lowercase letter, and all following characters must be a dash, lowercase letter, or digit, except the last character, which cannot be a dash.
              "operationalStatus": "A String", # [Output Only] The current status of whether or not this interconnect attachment is functional, which can take one of the following values: - OS_ACTIVE: The attachment has been turned up and is ready to use. - OS_UNPROVISIONED: The attachment is not ready to use yet, because turnup is not complete.
              "pairingKey": "A String", # [Output only for type PARTNER. Input only for PARTNER_PROVIDER. Not present for DEDICATED]. The opaque identifier of an PARTNER attachment used to initiate provisioning with a selected partner. Of the form "XXXXX/region/domain"
              "partnerAsn": "A String", # Optional BGP ASN for the router supplied by a Layer 3 Partner if they configured BGP on behalf of the customer. Output only for PARTNER type, input only for PARTNER_PROVIDER, not available for DEDICATED.
              "partnerMetadata": { # Informational metadata about Partner attachments from Partners to display to customers. These fields are propagated from PARTNER_PROVIDER attachments to their corresponding PARTNER attachments. # Informational metadata about Partner attachments from Partners to display to customers. Output only for for PARTNER type, mutable for PARTNER_PROVIDER, not available for DEDICATED.
                "interconnectName": "A String", # Plain text name of the Interconnect this attachment is connected to, as displayed in the Partner's portal. For instance "Chicago 1". This value may be validated to match approved Partner values.
                "partnerName": "A String", # Plain text name of the Partner providing this attachment. This value may be validated to match approved Partner values.
                "portalUrl": "A String", # URL of the Partner's portal for this Attachment. Partners may customise this to be a deep link to the specific resource on the Partner portal. This value may be validated to match approved Partner values.
              },
              "privateInterconnectInfo": { # Information for an interconnect attachment when this belongs to an interconnect of type DEDICATED. # [Output Only] Information specific to an InterconnectAttachment. This property is populated if the interconnect that this is attached to is of type DEDICATED.
                "tag8021q": 42, # [Output Only] 802.1q encapsulation tag to be used for traffic between Google and the customer, going to and from this network and region.
              },
              "region": "A String", # [Output Only] URL of the region where the regional interconnect attachment resides. You must specify this field as part of the HTTP request URL. It is not settable as a field in the request body.
              "router": "A String", # URL of the Cloud Router to be used for dynamic routing. This router must be in the same region as this InterconnectAttachment. The InterconnectAttachment will automatically connect the Interconnect to the network & region within which the Cloud Router is configured.
              "satisfiesPzs": True or False, # [Output Only] Set to true if the resource satisfies the zone separation organization policy constraints and false otherwise. Defaults to false if the field is not present.
              "selfLink": "A String", # [Output Only] Server-defined URL for the resource.
              "selfLinkWithId": "A String", # [Output Only] Server-defined URL for this resource with the resource id.
              "stackType": "A String", # The stack type for this interconnect attachment to identify whether the IPv6 feature is enabled or not. If not specified, IPV4_ONLY will be used. This field can be both set at interconnect attachments creation and update interconnect attachment operations.
              "state": "A String", # [Output Only] The current state of this attachment's functionality. Enum values ACTIVE and UNPROVISIONED are shared by DEDICATED/PRIVATE, PARTNER, and PARTNER_PROVIDER interconnect attachments, while enum values PENDING_PARTNER, PARTNER_REQUEST_RECEIVED, and PENDING_CUSTOMER are used for only PARTNER and PARTNER_PROVIDER interconnect attachments. This state can take one of the following values: - ACTIVE: The attachment has been turned up and is ready to use. - UNPROVISIONED: The attachment is not ready to use yet, because turnup is not complete. - PENDING_PARTNER: A newly-created PARTNER attachment that has not yet been configured on the Partner side. - PARTNER_REQUEST_RECEIVED: A PARTNER attachment is in the process of provisioning after a PARTNER_PROVIDER attachment was created that references it. - PENDING_CUSTOMER: A PARTNER or PARTNER_PROVIDER attachment that is waiting for a customer to activate it. - DEFUNCT: The attachment was deleted externally and is no longer functional. This could be because the associated Interconnect was removed, or because the other side of a Partner attachment was deleted.
              "type": "A String", # The type of interconnect attachment this is, which can take one of the following values: - DEDICATED: an attachment to a Dedicated Interconnect. - PARTNER: an attachment to a Partner Interconnect, created by the customer. - PARTNER_PROVIDER: an attachment to a Partner Interconnect, created by the partner.
              "vlanTag8021q": 42, # The IEEE 802.1Q VLAN tag for this attachment, in the range 2-4094. Only specified at creation time.
            },
          ],
          "warning": { # Informational warning which replaces the list of addresses when the list is empty.
            "code": "A String", # [Output Only] A warning code, if applicable. For example, Compute Engine returns NO_RESULTS_ON_PAGE if there are no results in the response.
            "data": [ # [Output Only] Metadata about this warning in key: value format. For example: "data": [ { "key": "scope", "value": "zones/us-east1-d" }
              {
                "key": "A String", # [Output Only] A key that provides more detail on the warning being returned. For example, for warnings where there are no results in a list request for a particular zone, this key might be scope and the key value might be the zone name. Other examples might be a key indicating a deprecated resource and a suggested replacement, or a warning about invalid network settings (for example, if an instance attempts to perform IP forwarding but is not enabled for IP forwarding).
                "value": "A String", # [Output Only] A warning data value corresponding to the key.
              },
            ],
            "message": "A String", # [Output Only] A human-readable description of the warning code.
          },
        },
      },
      "kind": "compute#interconnectAttachmentAggregatedList", # [Output Only] Type of resource. Always compute#interconnectAttachmentAggregatedList for aggregated lists of interconnect attachments.
      "nextPageToken": "A String", # [Output Only] This token allows you to get the next page of results for list requests. If the number of results is larger than maxResults, use the nextPageToken as a value for the query parameter pageToken in the next list request. Subsequent list requests will have their own nextPageToken to continue paging through the results.
      "selfLink": "A String", # [Output Only] Server-defined URL for this resource.
      "unreachables": [ # [Output Only] Unreachable resources.
        "A String",
      ],
      "warning": { # [Output Only] Informational warning message.
        "code": "A String", # [Output Only] A warning code, if applicable. For example, Compute Engine returns NO_RESULTS_ON_PAGE if there are no results in the response.
        "data": [ # [Output Only] Metadata about this warning in key: value format. For example: "data": [ { "key": "scope", "value": "zones/us-east1-d" }
          {
            "key": "A String", # [Output Only] A key that provides more detail on the warning being returned. For example, for warnings where there are no results in a list request for a particular zone, this key might be scope and the key value might be the zone name. Other examples might be a key indicating a deprecated resource and a suggested replacement, or a warning about invalid network settings (for example, if an instance attempts to perform IP forwarding but is not enabled for IP forwarding).
            "value": "A String", # [Output Only] A warning data value corresponding to the key.
          },
        ],
        "message": "A String", # [Output Only] A human-readable description of the warning code.
      },
    }

`aggregatedList_next(previous_request, previous_response)`

    Retrieves the next page of results.

    Args:
      previous_request: The request for the previous page. (required)
      previous_response: The response from the request for the previous page. (required)

    Returns:
      A request object that you can call 'execute()' on to request the next
      page. Returns None if there are no more items in the collection.

`close()`

    Close httplib2 connections.

`delete(project, region, interconnectAttachment, requestId=None, x__xgafv=None)`

    Deletes the specified interconnect attachment.

    Args:
      project: string, Project ID for this request. (required)
      region: string, Name of the region for this request. (required)
      interconnectAttachment: string, Name of the interconnect attachment to delete. (required)
      requestId: string, An optional request ID to identify requests. Specify a unique request ID so that if you must retry your request, the server will know to ignore the request if it has already been completed. For example, consider a situation where you make an initial request and the request times out. If you make the request again with the same request ID, the server can check if original operation with the same request ID was received, and if so, will ignore the second request. This prevents clients from accidentally creating duplicate commitments. The request ID must be a valid UUID with the exception that zero UUID is not supported ( 00000000-0000-0000-0000-000000000000).
      x__xgafv: string, V1 error format.
        Allowed values
          1 - v1 error format
          2 - v2 error format

    Returns:
      An object of the form:

        { # Represents an Operation resource. Google Compute Engine has three Operation resources: * [Global](/compute/docs/reference/rest/alpha/globalOperations) * [Regional](/compute/docs/reference/rest/alpha/regionOperations) * [Zonal](/compute/docs/reference/rest/alpha/zoneOperations) You can use an operation resource to manage asynchronous API requests. For more information, read Handling API responses. Operations can be global, regional or zonal. - For global operations, use the `globalOperations` resource. - For regional operations, use the `regionOperations` resource. - For zonal operations, use the `zonalOperations` resource. For more information, read Global, Regional, and Zonal Resources.
      "clientOperationId": "A String", # [Output Only] The value of `requestId` if you provided it in the request. Not present otherwise.
      "creationTimestamp": "A String", # [Deprecated] This field is deprecated.
      "description": "A String", # [Output Only] A textual description of the operation, which is set when the operation is created.
      "endTime": "A String", # [Output Only] The time that this operation was completed. This value is in RFC3339 text format.
      "error": { # [Output Only] If errors are generated during processing of the operation, this field will be populated.
        "errors": [ # [Output Only] The array of errors encountered while processing this operation.
          {
            "code": "A String", # [Output Only] The error type identifier for this error.
            "location": "A String", # [Output Only] Indicates the field in the request that caused the error. This property is optional.
            "message": "A String", # [Output Only] An optional, human-readable error message.
          },
        ],
      },
      "httpErrorMessage": "A String", # [Output Only] If the operation fails, this field contains the HTTP error message that was returned, such as `NOT FOUND`.
      "httpErrorStatusCode": 42, # [Output Only] If the operation fails, this field contains the HTTP error status code that was returned. For example, a `404` means the resource was not found.
      "id": "A String", # [Output Only] The unique identifier for the operation. This identifier is defined by the server.
      "insertTime": "A String", # [Output Only] The time that this operation was requested. This value is in RFC3339 text format.
      "kind": "compute#operation", # [Output Only] Type of the resource. Always `compute#operation` for Operation resources.
      "name": "A String", # [Output Only] Name of the operation.
      "operationGroupId": "A String", # [Output Only] An ID that represents a group of operations, such as when a group of operations results from a `bulkInsert` API request.
      "operationType": "A String", # [Output Only] The type of operation, such as `insert`, `update`, or `delete`, and so on.
      "progress": 42, # [Output Only] An optional progress indicator that ranges from 0 to 100. There is no requirement that this be linear or support any granularity of operations. This should not be used to guess when the operation will be complete. This number should monotonically increase as the operation progresses.
      "region": "A String", # [Output Only] The URL of the region where the operation resides. Only applicable when performing regional operations.
      "selfLink": "A String", # [Output Only] Server-defined URL for the resource.
      "selfLinkWithId": "A String", # [Output Only] Server-defined URL for this resource with the resource id.
      "startTime": "A String", # [Output Only] The time that this operation was started by the server. This value is in RFC3339 text format.
      "status": "A String", # [Output Only] The status of the operation, which can be one of the following: `PENDING`, `RUNNING`, or `DONE`.
      "statusMessage": "A String", # [Output Only] An optional textual description of the current status of the operation.
      "targetId": "A String", # [Output Only] The unique target ID, which identifies a specific incarnation of the target resource.
      "targetLink": "A String", # [Output Only] The URL of the resource that the operation modifies. For operations related to creating a snapshot, this points to the persistent disk that the snapshot was created from.
      "user": "A String", # [Output Only] User who requested the operation, for example: `user@example.com`.
      "warnings": [ # [Output Only] If warning messages are generated during processing of the operation, this field will be populated.
        {
          "code": "A String", # [Output Only] A warning code, if applicable. For example, Compute Engine returns NO_RESULTS_ON_PAGE if there are no results in the response.
          "data": [ # [Output Only] Metadata about this warning in key: value format. For example: "data": [ { "key": "scope", "value": "zones/us-east1-d" }
            {
              "key": "A String", # [Output Only] A key that provides more detail on the warning being returned. For example, for warnings where there are no results in a list request for a particular zone, this key might be scope and the key value might be the zone name. Other examples might be a key indicating a deprecated resource and a suggested replacement, or a warning about invalid network settings (for example, if an instance attempts to perform IP forwarding but is not enabled for IP forwarding).
              "value": "A String", # [Output Only] A warning data value corresponding to the key.
            },
          ],
          "message": "A String", # [Output Only] A human-readable description of the warning code.
        },
      ],
      "zone": "A String", # [Output Only] The URL of the zone where the operation resides. Only applicable when performing per-zone operations.
    }

`get(project, region, interconnectAttachment, x__xgafv=None)`

    Returns the specified interconnect attachment.

    Args:
      project: string, Project ID for this request. (required)
      region: string, Name of the region for this request. (required)
      interconnectAttachment: string, Name of the interconnect attachment to return. (required)
      x__xgafv: string, V1 error format.
        Allowed values
          1 - v1 error format
          2 - v2 error format

    Returns:
      An object of the form:

        { # Represents an Interconnect Attachment (VLAN) resource. You can use Interconnect attachments (VLANS) to connect your Virtual Private Cloud networks to your on-premises networks through an Interconnect. For more information, read Creating VLAN Attachments.
      "adminEnabled": True or False, # Determines whether this Attachment will carry packets. Not present for PARTNER_PROVIDER.
      "bandwidth": "A String", # Provisioned bandwidth capacity for the interconnect attachment. For attachments of type DEDICATED, the user can set the bandwidth. For attachments of type PARTNER, the Google Partner that is operating the interconnect must set the bandwidth. Output only for PARTNER type, mutable for PARTNER_PROVIDER and DEDICATED, and can take one of the following values: - BPS_50M: 50 Mbit/s - BPS_100M: 100 Mbit/s - BPS_200M: 200 Mbit/s - BPS_300M: 300 Mbit/s - BPS_400M: 400 Mbit/s - BPS_500M: 500 Mbit/s - BPS_1G: 1 Gbit/s - BPS_2G: 2 Gbit/s - BPS_5G: 5 Gbit/s - BPS_10G: 10 Gbit/s - BPS_20G: 20 Gbit/s - BPS_50G: 50 Gbit/s
      "candidateIpv6Subnets": [ # Up to 16 candidate prefixes that control the allocation of cloudRouterIpv6Address and customerRouterIpv6Address for this attachment. Each prefix must be in the Global Unique Address (GUA) space. It is highly recommended that it be in a range owned by the requestor. A GUA in a range owned by Google will cause the request to fail. Google will select an available prefix from the supplied candidates or fail the request. If not supplied, a /125 from a Google-owned GUA block will be selected.
        "A String",
      ],
      "candidateSubnets": [ # Up to 16 candidate prefixes that can be used to restrict the allocation of cloudRouterIpAddress and customerRouterIpAddress for this attachment. All prefixes must be within link-local address space (169.254.0.0/16) and must be /29 or shorter (/28, /27, etc). Google will attempt to select an unused /29 from the supplied candidate prefix(es). The request will fail if all possible /29s are in use on Google's edge. If not supplied, Google will randomly select an unused /29 from all of link-local space.
        "A String",
      ],
      "cloudRouterIpAddress": "A String", # [Output Only] IPv4 address + prefix length to be configured on Cloud Router Interface for this interconnect attachment.
      "cloudRouterIpv6Address": "A String", # [Output Only] IPv6 address + prefix length to be configured on Cloud Router Interface for this interconnect attachment.
      "cloudRouterIpv6InterfaceId": "A String", # If supplied, the interface id (index within the subnet) to be used for the cloud router address. The id must be in the range of 1 to 6. If a subnet mask is supplied, it must be /125, and the subnet should either be 0 or match the selected subnet.
      "creationTimestamp": "A String", # [Output Only] Creation timestamp in RFC3339 text format.
      "customerRouterIpAddress": "A String", # [Output Only] IPv4 address + prefix length to be configured on the customer router subinterface for this interconnect attachment.
      "customerRouterIpv6Address": "A String", # [Output Only] IPv6 address + prefix length to be configured on the customer router subinterface for this interconnect attachment.
      "customerRouterIpv6InterfaceId": "A String", # If supplied, the interface id (index within the subnet) to be used for the customer router address. The id must be in the range of 1 to 6. If a subnet mask is supplied, it must be /125, and the subnet should either be 0 or match the selected subnet.
      "dataplaneVersion": 42, # [Output Only] Dataplane version for this InterconnectAttachment.
      "description": "A String", # An optional description of this resource.
      "edgeAvailabilityDomain": "A String", # Desired availability domain for the attachment. Only available for type PARTNER, at creation time, and can take one of the following values: - AVAILABILITY_DOMAIN_ANY - AVAILABILITY_DOMAIN_1 - AVAILABILITY_DOMAIN_2 For improved reliability, customers should configure a pair of attachments, one per availability domain. The selected availability domain will be provided to the Partner via the pairing key, so that the provisioned circuit will lie in the specified domain. If not specified, the value will default to AVAILABILITY_DOMAIN_ANY.
      "encryption": "A String", # Indicates the user-supplied encryption option of this VLAN attachment (interconnectAttachment). Can only be specified at attachment creation for PARTNER or DEDICATED attachments. Possible values are: - NONE - This is the default value, which means that the VLAN attachment carries unencrypted traffic. VMs are able to send traffic to, or receive traffic from, such a VLAN attachment. - IPSEC - The VLAN attachment carries only encrypted traffic that is encrypted by an IPsec device, such as an HA VPN gateway or third-party IPsec VPN. VMs cannot directly send traffic to, or receive traffic from, such a VLAN attachment. To use *IPsec-encrypted Cloud Interconnect*, the VLAN attachment must be created with this option. Not currently available publicly.
      "googleReferenceId": "A String", # [Output Only] Google reference ID, to be used when raising support tickets with Google or otherwise to debug backend connectivity issues. [Deprecated] This field is not used.
      "id": "A String", # [Output Only] The unique identifier for the resource. This identifier is defined by the server.
      "interconnect": "A String", # URL of the underlying Interconnect object that this attachment's traffic will traverse through.
      "ipsecInternalAddresses": [ # A list of URLs of addresses that have been reserved for the VLAN attachment. Used only for the VLAN attachment that has the encryption option as IPSEC. The addresses must be regional internal IP address ranges. When creating an HA VPN gateway over the VLAN attachment, if the attachment is configured to use a regional internal IP address, then the VPN gateway's IP address is allocated from the IP address range specified here. For example, if the HA VPN gateway's interface 0 is paired to this VLAN attachment, then a regional internal IP address for the VPN gateway interface 0 will be allocated from the IP address specified for this VLAN attachment. If this field is not specified when creating the VLAN attachment, then later on when creating an HA VPN gateway on this VLAN attachment, the HA VPN gateway's IP address is allocated from the regional external IP address pool. Not currently available publicly.
        "A String",
      ],
      "kind": "compute#interconnectAttachment", # [Output Only] Type of the resource. Always compute#interconnectAttachment for interconnect attachments.
      "labelFingerprint": "A String", # A fingerprint for the labels being applied to this InterconnectAttachment, which is essentially a hash of the labels set used for optimistic locking. The fingerprint is initially generated by Compute Engine and changes after every request to modify or update labels. You must always provide an up-to-date fingerprint hash in order to update or change labels, otherwise the request will fail with error 412 conditionNotMet. To see the latest fingerprint, make a get() request to retrieve an InterconnectAttachment.
      "labels": { # Labels for this resource. These can only be added or modified by the setLabels method. Each label key/value pair must comply with RFC1035. Label values may be empty.
        "a_key": "A String",
      },
      "mtu": 42, # Maximum Transmission Unit (MTU), in bytes, of packets passing through this interconnect attachment. Only 1440 and 1500 are allowed. If not specified, the value will default to 1440.
      "name": "A String", # Name of the resource. Provided by the client when the resource is created. The name must be 1-63 characters long, and comply with RFC1035. Specifically, the name must be 1-63 characters long and match the regular expression `[a-z]([-a-z0-9]*[a-z0-9])?` which means the first character must be a lowercase letter, and all following characters must be a dash, lowercase letter, or digit, except the last character, which cannot be a dash.
      "operationalStatus": "A String", # [Output Only] The current status of whether or not this interconnect attachment is functional, which can take one of the following values: - OS_ACTIVE: The attachment has been turned up and is ready to use. - OS_UNPROVISIONED: The attachment is not ready to use yet, because turnup is not complete.
      "pairingKey": "A String", # [Output only for type PARTNER. Input only for PARTNER_PROVIDER. Not present for DEDICATED]. The opaque identifier of an PARTNER attachment used to initiate provisioning with a selected partner. Of the form "XXXXX/region/domain"
      "partnerAsn": "A String", # Optional BGP ASN for the router supplied by a Layer 3 Partner if they configured BGP on behalf of the customer. Output only for PARTNER type, input only for PARTNER_PROVIDER, not available for DEDICATED.
      "partnerMetadata": { # Informational metadata about Partner attachments from Partners to display to customers. These fields are propagated from PARTNER_PROVIDER attachments to their corresponding PARTNER attachments. # Informational metadata about Partner attachments from Partners to display to customers. Output only for for PARTNER type, mutable for PARTNER_PROVIDER, not available for DEDICATED.
        "interconnectName": "A String", # Plain text name of the Interconnect this attachment is connected to, as displayed in the Partner's portal. For instance "Chicago 1". This value may be validated to match approved Partner values.
        "partnerName": "A String", # Plain text name of the Partner providing this attachment. This value may be validated to match approved Partner values.
        "portalUrl": "A String", # URL of the Partner's portal for this Attachment. Partners may customise this to be a deep link to the specific resource on the Partner portal. This value may be validated to match approved Partner values.
      },
      "privateInterconnectInfo": { # Information for an interconnect attachment when this belongs to an interconnect of type DEDICATED. # [Output Only] Information specific to an InterconnectAttachment. This property is populated if the interconnect that this is attached to is of type DEDICATED.
        "tag8021q": 42, # [Output Only] 802.1q encapsulation tag to be used for traffic between Google and the customer, going to and from this network and region.
      },
      "region": "A String", # [Output Only] URL of the region where the regional interconnect attachment resides. You must specify this field as part of the HTTP request URL. It is not settable as a field in the request body.
      "router": "A String", # URL of the Cloud Router to be used for dynamic routing. This router must be in the same region as this InterconnectAttachment. The InterconnectAttachment will automatically connect the Interconnect to the network & region within which the Cloud Router is configured.
      "satisfiesPzs": True or False, # [Output Only] Set to true if the resource satisfies the zone separation organization policy constraints and false otherwise. Defaults to false if the field is not present.
      "selfLink": "A String", # [Output Only] Server-defined URL for the resource.
      "selfLinkWithId": "A String", # [Output Only] Server-defined URL for this resource with the resource id.
      "stackType": "A String", # The stack type for this interconnect attachment to identify whether the IPv6 feature is enabled or not. If not specified, IPV4_ONLY will be used. This field can be both set at interconnect attachments creation and update interconnect attachment operations.
      "state": "A String", # [Output Only] The current state of this attachment's functionality. Enum values ACTIVE and UNPROVISIONED are shared by DEDICATED/PRIVATE, PARTNER, and PARTNER_PROVIDER interconnect attachments, while enum values PENDING_PARTNER, PARTNER_REQUEST_RECEIVED, and PENDING_CUSTOMER are used for only PARTNER and PARTNER_PROVIDER interconnect attachments. This state can take one of the following values: - ACTIVE: The attachment has been turned up and is ready to use. - UNPROVISIONED: The attachment is not ready to use yet, because turnup is not complete. - PENDING_PARTNER: A newly-created PARTNER attachment that has not yet been configured on the Partner side. - PARTNER_REQUEST_RECEIVED: A PARTNER attachment is in the process of provisioning after a PARTNER_PROVIDER attachment was created that references it. - PENDING_CUSTOMER: A PARTNER or PARTNER_PROVIDER attachment that is waiting for a customer to activate it. - DEFUNCT: The attachment was deleted externally and is no longer functional. This could be because the associated Interconnect was removed, or because the other side of a Partner attachment was deleted.
      "type": "A String", # The type of interconnect attachment this is, which can take one of the following values: - DEDICATED: an attachment to a Dedicated Interconnect. - PARTNER: an attachment to a Partner Interconnect, created by the customer. - PARTNER_PROVIDER: an attachment to a Partner Interconnect, created by the partner.
      "vlanTag8021q": 42, # The IEEE 802.1Q VLAN tag for this attachment, in the range 2-4094. Only specified at creation time.
    }

`getIamPolicy(project, region, resource, optionsRequestedPolicyVersion=None, x__xgafv=None)`

    Gets the access control policy for a resource. May be empty if no such policy or resource exists.

    Args:
      project: string, Project ID for this request. (required)
      region: string, The name of the region for this request. (required)
      resource: string, Name or id of the resource for this request. (required)
      optionsRequestedPolicyVersion: integer, Requested IAM Policy version.
      x__xgafv: string, V1 error format.
        Allowed values
          1 - v1 error format
          2 - v2 error format

    Returns:
      An object of the form:

        { # An Identity and Access Management (IAM) policy, which specifies access controls for Google Cloud resources. A `Policy` is a collection of `bindings`. A `binding` binds one or more `members` to a single `role`. Members can be user accounts, service accounts, Google groups, and domains (such as G Suite). A `role` is a named list of permissions; each `role` can be an IAM predefined role or a user-created custom role. For some types of Google Cloud resources, a `binding` can also specify a `condition`, which is a logical expression that allows access to a resource only if the expression evaluates to `true`. A condition can add constraints based on attributes of the request, the resource, or both. To learn which resources support conditions in their IAM policies, see the [IAM documentation](https://cloud.google.com/iam/help/conditions/resource-policies). **JSON example:** { "bindings": [ { "role": "roles/resourcemanager.organizationAdmin", "members": [ "user:mike@example.com", "group:admins@example.com", "domain:google.com", "serviceAccount:my-project-id@appspot.gserviceaccount.com" ] }, { "role": "roles/resourcemanager.organizationViewer", "members": [ "user:eve@example.com" ], "condition": { "title": "expirable access", "description": "Does not grant access after Sep 2020", "expression": "request.time < timestamp('2020-10-01T00:00:00.000Z')", } } ], "etag": "BwWWja0YfJA=", "version": 3 } **YAML example:** bindings: - members: - user:mike@example.com - group:admins@example.com - domain:google.com - serviceAccount:my-project-id@appspot.gserviceaccount.com role: roles/resourcemanager.organizationAdmin - members: - user:eve@example.com role: roles/resourcemanager.organizationViewer condition: title: expirable access description: Does not grant access after Sep 2020 expression: request.time < timestamp('2020-10-01T00:00:00.000Z') etag: BwWWja0YfJA= version: 3 For a description of IAM and its features, see the [IAM documentation](https://cloud.google.com/iam/docs/).
      "auditConfigs": [ # Specifies cloud audit logging configuration for this policy.
        { # Specifies the audit configuration for a service. The configuration determines which permission types are logged, and what identities, if any, are exempted from logging. An AuditConfig must have one or more AuditLogConfigs. If there are AuditConfigs for both `allServices` and a specific service, the union of the two AuditConfigs is used for that service: the log_types specified in each AuditConfig are enabled, and the exempted_members in each AuditLogConfig are exempted. Example Policy with multiple AuditConfigs: { "audit_configs": [ { "service": "allServices", "audit_log_configs": [ { "log_type": "DATA_READ", "exempted_members": [ "user:jose@example.com" ] }, { "log_type": "DATA_WRITE" }, { "log_type": "ADMIN_READ" } ] }, { "service": "sampleservice.googleapis.com", "audit_log_configs": [ { "log_type": "DATA_READ" }, { "log_type": "DATA_WRITE", "exempted_members": [ "user:aliya@example.com" ] } ] } ] } For sampleservice, this policy enables DATA_READ, DATA_WRITE and ADMIN_READ logging. It also exempts jose@example.com from DATA_READ logging, and aliya@example.com from DATA_WRITE logging.
          "auditLogConfigs": [ # The configuration for logging of each type of permission.
            { # Provides the configuration for logging a type of permissions. Example: { "audit_log_configs": [ { "log_type": "DATA_READ", "exempted_members": [ "user:jose@example.com" ] }, { "log_type": "DATA_WRITE" } ] } This enables 'DATA_READ' and 'DATA_WRITE' logging, while exempting jose@example.com from DATA_READ logging.
              "exemptedMembers": [ # Specifies the identities that do not cause logging for this type of permission. Follows the same format of Binding.members.
                "A String",
              ],
              "ignoreChildExemptions": True or False, # This is deprecated and has no effect. Do not use.
              "logType": "A String", # The log type that this config enables.
            },
          ],
          "exemptedMembers": [ # This is deprecated and has no effect. Do not use.
            "A String",
          ],
          "service": "A String", # Specifies a service that will be enabled for audit logging. For example, `storage.googleapis.com`, `cloudsql.googleapis.com`. `allServices` is a special value that covers all services.
        },
      ],
      "bindings": [ # Associates a list of `members` to a `role`. Optionally, may specify a `condition` that determines how and when the `bindings` are applied. Each of the `bindings` must contain at least one member.
        { # Associates `members` with a `role`.
          "bindingId": "A String", # This is deprecated and has no effect. Do not use.
          "condition": { # Represents a textual expression in the Common Expression Language (CEL) syntax. CEL is a C-like expression language. The syntax and semantics of CEL are documented at https://github.com/google/cel-spec. Example (Comparison): title: "Summary size limit" description: "Determines if a summary is less than 100 chars" expression: "document.summary.size() < 100" Example (Equality): title: "Requestor is owner" description: "Determines if requestor is the document owner" expression: "document.owner == request.auth.claims.email" Example (Logic): title: "Public documents" description: "Determine whether the document should be publicly visible" expression: "document.type != 'private' && document.type != 'internal'" Example (Data Manipulation): title: "Notification string" description: "Create a notification string with a timestamp." expression: "'New message received at ' + string(document.create_time)" The exact variables and functions that may be referenced within an expression are determined by the service that evaluates it. See the service documentation for additional information. # The condition that is associated with this binding. If the condition evaluates to `true`, then this binding applies to the current request. If the condition evaluates to `false`, then this binding does not apply to the current request. However, a different role binding might grant the same role to one or more of the members in this binding. To learn which resources support conditions in their IAM policies, see the [IAM documentation](https://cloud.google.com/iam/help/conditions/resource-policies).
            "description": "A String", # Optional. Description of the expression. This is a longer text which describes the expression, e.g. when hovered over it in a UI.
            "expression": "A String", # Textual representation of an expression in Common Expression Language syntax.
            "location": "A String", # Optional. String indicating the location of the expression for error reporting, e.g. a file name and a position in the file.
            "title": "A String", # Optional. Title for the expression, i.e. a short string describing its purpose. This can be used e.g. in UIs which allow to enter the expression.
          },
          "members": [ # Specifies the identities requesting access for a Cloud Platform resource. `members` can have the following values: * `allUsers`: A special identifier that represents anyone who is on the internet; with or without a Google account. * `allAuthenticatedUsers`: A special identifier that represents anyone who is authenticated with a Google account or a service account. * `user:{emailid}`: An email address that represents a specific Google account. For example, `alice@example.com` . * `serviceAccount:{emailid}`: An email address that represents a service account. For example, `my-other-app@appspot.gserviceaccount.com`. * `group:{emailid}`: An email address that represents a Google group. For example, `admins@example.com`. * `deleted:user:{emailid}?uid={uniqueid}`: An email address (plus unique identifier) representing a user that has been recently deleted. For example, `alice@example.com?uid=123456789012345678901`. If the user is recovered, this value reverts to `user:{emailid}` and the recovered user retains the role in the binding. * `deleted:serviceAccount:{emailid}?uid={uniqueid}`: An email address (plus unique identifier) representing a service account that has been recently deleted. For example, `my-other-app@appspot.gserviceaccount.com?uid=123456789012345678901`. If the service account is undeleted, this value reverts to `serviceAccount:{emailid}` and the undeleted service account retains the role in the binding. * `deleted:group:{emailid}?uid={uniqueid}`: An email address (plus unique identifier) representing a Google group that has been recently deleted. For example, `admins@example.com?uid=123456789012345678901`. If the group is recovered, this value reverts to `group:{emailid}` and the recovered group retains the role in the binding. * `domain:{domain}`: The G Suite domain (primary) that represents all the users of that domain. For example, `google.com` or `example.com`.
            "A String",
          ],
          "role": "A String", # Role that is assigned to `members`. For example, `roles/viewer`, `roles/editor`, or `roles/owner`.
        },
      ],
      "etag": "A String", # `etag` is used for optimistic concurrency control as a way to help prevent simultaneous updates of a policy from overwriting each other. It is strongly suggested that systems make use of the `etag` in the read-modify-write cycle to perform policy updates in order to avoid race conditions: An `etag` is returned in the response to `getIamPolicy`, and systems are expected to put that etag in the request to `setIamPolicy` to ensure that their change will be applied to the same version of the policy. **Important:** If you use IAM Conditions, you must include the `etag` field whenever you call `setIamPolicy`. If you omit this field, then IAM allows you to overwrite a version `3` policy with a version `1` policy, and all of the conditions in the version `3` policy are lost.
      "iamOwned": True or False, # This is deprecated and has no effect. Do not use.
      "rules": [ # This is deprecated and has no effect. Do not use.
        { # This is deprecated and has no effect. Do not use.
          "action": "A String", # This is deprecated and has no effect. Do not use.
          "conditions": [ # This is deprecated and has no effect. Do not use.
            { # This is deprecated and has no effect. Do not use.
              "iam": "A String", # This is deprecated and has no effect. Do not use.
              "op": "A String", # This is deprecated and has no effect. Do not use.
              "svc": "A String", # This is deprecated and has no effect. Do not use.
              "sys": "A String", # This is deprecated and has no effect. Do not use.
              "values": [ # This is deprecated and has no effect. Do not use.
                "A String",
              ],
            },
          ],
          "description": "A String", # This is deprecated and has no effect. Do not use.
          "ins": [ # This is deprecated and has no effect. Do not use.
            "A String",
          ],
          "logConfigs": [ # This is deprecated and has no effect. Do not use.
            { # This is deprecated and has no effect. Do not use.
              "cloudAudit": { # This is deprecated and has no effect. Do not use. # This is deprecated and has no effect. Do not use.
                "authorizationLoggingOptions": { # This is deprecated and has no effect. Do not use. # This is deprecated and has no effect. Do not use.
                  "permissionType": "A String", # This is deprecated and has no effect. Do not use.
                },
                "logName": "A String", # This is deprecated and has no effect. Do not use.
              },
              "counter": { # This is deprecated and has no effect. Do not use. # This is deprecated and has no effect. Do not use.
                "customFields": [ # This is deprecated and has no effect. Do not use.
                  { # This is deprecated and has no effect. Do not use.
                    "name": "A String", # This is deprecated and has no effect. Do not use.
                    "value": "A String", # This is deprecated and has no effect. Do not use.
                  },
                ],
                "field": "A String", # This is deprecated and has no effect. Do not use.
                "metric": "A String", # This is deprecated and has no effect. Do not use.
              },
              "dataAccess": { # This is deprecated and has no effect. Do not use. # This is deprecated and has no effect. Do not use.
                "logMode": "A String", # This is deprecated and has no effect. Do not use.
              },
            },
          ],
          "notIns": [ # This is deprecated and has no effect. Do not use.
            "A String",
          ],
          "permissions": [ # This is deprecated and has no effect. Do not use.
            "A String",
          ],
        },
      ],
      "version": 42, # Specifies the format of the policy. Valid values are `0`, `1`, and `3`. Requests that specify an invalid value are rejected. Any operation that affects conditional role bindings must specify version `3`. This requirement applies to the following operations: * Getting a policy that includes a conditional role binding * Adding a conditional role binding to a policy * Changing a conditional role binding in a policy * Removing any role binding, with or without a condition, from a policy that includes conditions **Important:** If you use IAM Conditions, you must include the `etag` field whenever you call `setIamPolicy`. If you omit this field, then IAM allows you to overwrite a version `3` policy with a version `1` policy, and all of the conditions in the version `3` policy are lost. If a policy does not include any conditions, operations on that policy may specify any valid version or leave the field unset. To learn which resources support conditions in their IAM policies, see the [IAM documentation](https://cloud.google.com/iam/help/conditions/resource-policies).
    }

`insert(project, region, body=None, requestId=None, validateOnly=None, x__xgafv=None)`

    Creates an InterconnectAttachment in the specified project using the data included in the request.

    Args:
      project: string, Project ID for this request. (required)
      region: string, Name of the region for this request. (required)
      body: object, The request body.
        The object takes the form of:

    { # Represents an Interconnect Attachment (VLAN) resource. You can use Interconnect attachments (VLANS) to connect your Virtual Private Cloud networks to your on-premises networks through an Interconnect. For more information, read Creating VLAN Attachments.
      "adminEnabled": True or False, # Determines whether this Attachment will carry packets. Not present for PARTNER_PROVIDER.
      "bandwidth": "A String", # Provisioned bandwidth capacity for the interconnect attachment. For attachments of type DEDICATED, the user can set the bandwidth. For attachments of type PARTNER, the Google Partner that is operating the interconnect must set the bandwidth. Output only for PARTNER type, mutable for PARTNER_PROVIDER and DEDICATED, and can take one of the following values: - BPS_50M: 50 Mbit/s - BPS_100M: 100 Mbit/s - BPS_200M: 200 Mbit/s - BPS_300M: 300 Mbit/s - BPS_400M: 400 Mbit/s - BPS_500M: 500 Mbit/s - BPS_1G: 1 Gbit/s - BPS_2G: 2 Gbit/s - BPS_5G: 5 Gbit/s - BPS_10G: 10 Gbit/s - BPS_20G: 20 Gbit/s - BPS_50G: 50 Gbit/s
      "candidateIpv6Subnets": [ # Up to 16 candidate prefixes that control the allocation of cloudRouterIpv6Address and customerRouterIpv6Address for this attachment. Each prefix must be in the Global Unique Address (GUA) space. It is highly recommended that it be in a range owned by the requestor. A GUA in a range owned by Google will cause the request to fail. Google will select an available prefix from the supplied candidates or fail the request. If not supplied, a /125 from a Google-owned GUA block will be selected.
        "A String",
      ],
      "candidateSubnets": [ # Up to 16 candidate prefixes that can be used to restrict the allocation of cloudRouterIpAddress and customerRouterIpAddress for this attachment. All prefixes must be within link-local address space (169.254.0.0/16) and must be /29 or shorter (/28, /27, etc). Google will attempt to select an unused /29 from the supplied candidate prefix(es). The request will fail if all possible /29s are in use on Google's edge. If not supplied, Google will randomly select an unused /29 from all of link-local space.
        "A String",
      ],
      "cloudRouterIpAddress": "A String", # [Output Only] IPv4 address + prefix length to be configured on Cloud Router Interface for this interconnect attachment.
      "cloudRouterIpv6Address": "A String", # [Output Only] IPv6 address + prefix length to be configured on Cloud Router Interface for this interconnect attachment.
      "cloudRouterIpv6InterfaceId": "A String", # If supplied, the interface id (index within the subnet) to be used for the cloud router address. The id must be in the range of 1 to 6. If a subnet mask is supplied, it must be /125, and the subnet should either be 0 or match the selected subnet.
      "creationTimestamp": "A String", # [Output Only] Creation timestamp in RFC3339 text format.
      "customerRouterIpAddress": "A String", # [Output Only] IPv4 address + prefix length to be configured on the customer router subinterface for this interconnect attachment.
      "customerRouterIpv6Address": "A String", # [Output Only] IPv6 address + prefix length to be configured on the customer router subinterface for this interconnect attachment.
      "customerRouterIpv6InterfaceId": "A String", # If supplied, the interface id (index within the subnet) to be used for the customer router address. The id must be in the range of 1 to 6. If a subnet mask is supplied, it must be /125, and the subnet should either be 0 or match the selected subnet.
      "dataplaneVersion": 42, # [Output Only] Dataplane version for this InterconnectAttachment.
      "description": "A String", # An optional description of this resource.
      "edgeAvailabilityDomain": "A String", # Desired availability domain for the attachment. Only available for type PARTNER, at creation time, and can take one of the following values: - AVAILABILITY_DOMAIN_ANY - AVAILABILITY_DOMAIN_1 - AVAILABILITY_DOMAIN_2 For improved reliability, customers should configure a pair of attachments, one per availability domain. The selected availability domain will be provided to the Partner via the pairing key, so that the provisioned circuit will lie in the specified domain. If not specified, the value will default to AVAILABILITY_DOMAIN_ANY.
      "encryption": "A String", # Indicates the user-supplied encryption option of this VLAN attachment (interconnectAttachment). Can only be specified at attachment creation for PARTNER or DEDICATED attachments. Possible values are: - NONE - This is the default value, which means that the VLAN attachment carries unencrypted traffic. VMs are able to send traffic to, or receive traffic from, such a VLAN attachment. - IPSEC - The VLAN attachment carries only encrypted traffic that is encrypted by an IPsec device, such as an HA VPN gateway or third-party IPsec VPN. VMs cannot directly send traffic to, or receive traffic from, such a VLAN attachment. To use *IPsec-encrypted Cloud Interconnect*, the VLAN attachment must be created with this option. Not currently available publicly.
      "googleReferenceId": "A String", # [Output Only] Google reference ID, to be used when raising support tickets with Google or otherwise to debug backend connectivity issues. [Deprecated] This field is not used.
      "id": "A String", # [Output Only] The unique identifier for the resource. This identifier is defined by the server.
      "interconnect": "A String", # URL of the underlying Interconnect object that this attachment's traffic will traverse through.
      "ipsecInternalAddresses": [ # A list of URLs of addresses that have been reserved for the VLAN attachment. Used only for the VLAN attachment that has the encryption option as IPSEC. The addresses must be regional internal IP address ranges. When creating an HA VPN gateway over the VLAN attachment, if the attachment is configured to use a regional internal IP address, then the VPN gateway's IP address is allocated from the IP address range specified here. For example, if the HA VPN gateway's interface 0 is paired to this VLAN attachment, then a regional internal IP address for the VPN gateway interface 0 will be allocated from the IP address specified for this VLAN attachment. If this field is not specified when creating the VLAN attachment, then later on when creating an HA VPN gateway on this VLAN attachment, the HA VPN gateway's IP address is allocated from the regional external IP address pool. Not currently available publicly.
        "A String",
      ],
      "kind": "compute#interconnectAttachment", # [Output Only] Type of the resource. Always compute#interconnectAttachment for interconnect attachments.
      "labelFingerprint": "A String", # A fingerprint for the labels being applied to this InterconnectAttachment, which is essentially a hash of the labels set used for optimistic locking. The fingerprint is initially generated by Compute Engine and changes after every request to modify or update labels. You must always provide an up-to-date fingerprint hash in order to update or change labels, otherwise the request will fail with error 412 conditionNotMet. To see the latest fingerprint, make a get() request to retrieve an InterconnectAttachment.
      "labels": { # Labels for this resource. These can only be added or modified by the setLabels method. Each label key/value pair must comply with RFC1035. Label values may be empty.
        "a_key": "A String",
      },
      "mtu": 42, # Maximum Transmission Unit (MTU), in bytes, of packets passing through this interconnect attachment. Only 1440 and 1500 are allowed. If not specified, the value will default to 1440.
      "name": "A String", # Name of the resource. Provided by the client when the resource is created. The name must be 1-63 characters long, and comply with RFC1035. Specifically, the name must be 1-63 characters long and match the regular expression `[a-z]([-a-z0-9]*[a-z0-9])?` which means the first character must be a lowercase letter, and all following characters must be a dash, lowercase letter, or digit, except the last character, which cannot be a dash.
      "operationalStatus": "A String", # [Output Only] The current status of whether or not this interconnect attachment is functional, which can take one of the following values: - OS_ACTIVE: The attachment has been turned up and is ready to use. - OS_UNPROVISIONED: The attachment is not ready to use yet, because turnup is not complete.
      "pairingKey": "A String", # [Output only for type PARTNER. Input only for PARTNER_PROVIDER. Not present for DEDICATED]. The opaque identifier of an PARTNER attachment used to initiate provisioning with a selected partner. Of the form "XXXXX/region/domain"
      "partnerAsn": "A String", # Optional BGP ASN for the router supplied by a Layer 3 Partner if they configured BGP on behalf of the customer. Output only for PARTNER type, input only for PARTNER_PROVIDER, not available for DEDICATED.
      "partnerMetadata": { # Informational metadata about Partner attachments from Partners to display to customers. These fields are propagated from PARTNER_PROVIDER attachments to their corresponding PARTNER attachments. # Informational metadata about Partner attachments from Partners to display to customers. Output only for for PARTNER type, mutable for PARTNER_PROVIDER, not available for DEDICATED.
        "interconnectName": "A String", # Plain text name of the Interconnect this attachment is connected to, as displayed in the Partner's portal. For instance "Chicago 1". This value may be validated to match approved Partner values.
        "partnerName": "A String", # Plain text name of the Partner providing this attachment. This value may be validated to match approved Partner values.
        "portalUrl": "A String", # URL of the Partner's portal for this Attachment. Partners may customise this to be a deep link to the specific resource on the Partner portal. This value may be validated to match approved Partner values.
      },
      "privateInterconnectInfo": { # Information for an interconnect attachment when this belongs to an interconnect of type DEDICATED. # [Output Only] Information specific to an InterconnectAttachment. This property is populated if the interconnect that this is attached to is of type DEDICATED.
        "tag8021q": 42, # [Output Only] 802.1q encapsulation tag to be used for traffic between Google and the customer, going to and from this network and region.
      },
      "region": "A String", # [Output Only] URL of the region where the regional interconnect attachment resides. You must specify this field as part of the HTTP request URL. It is not settable as a field in the request body.
      "router": "A String", # URL of the Cloud Router to be used for dynamic routing. This router must be in the same region as this InterconnectAttachment. The InterconnectAttachment will automatically connect the Interconnect to the network & region within which the Cloud Router is configured.
      "satisfiesPzs": True or False, # [Output Only] Set to true if the resource satisfies the zone separation organization policy constraints and false otherwise. Defaults to false if the field is not present.
      "selfLink": "A String", # [Output Only] Server-defined URL for the resource.
      "selfLinkWithId": "A String", # [Output Only] Server-defined URL for this resource with the resource id.
      "stackType": "A String", # The stack type for this interconnect attachment to identify whether the IPv6 feature is enabled or not. If not specified, IPV4_ONLY will be used. This field can be both set at interconnect attachments creation and update interconnect attachment operations.
      "state": "A String", # [Output Only] The current state of this attachment's functionality. Enum values ACTIVE and UNPROVISIONED are shared by DEDICATED/PRIVATE, PARTNER, and PARTNER_PROVIDER interconnect attachments, while enum values PENDING_PARTNER, PARTNER_REQUEST_RECEIVED, and PENDING_CUSTOMER are used for only PARTNER and PARTNER_PROVIDER interconnect attachments. This state can take one of the following values: - ACTIVE: The attachment has been turned up and is ready to use. - UNPROVISIONED: The attachment is not ready to use yet, because turnup is not complete. - PENDING_PARTNER: A newly-created PARTNER attachment that has not yet been configured on the Partner side. - PARTNER_REQUEST_RECEIVED: A PARTNER attachment is in the process of provisioning after a PARTNER_PROVIDER attachment was created that references it. - PENDING_CUSTOMER: A PARTNER or PARTNER_PROVIDER attachment that is waiting for a customer to activate it. - DEFUNCT: The attachment was deleted externally and is no longer functional. This could be because the associated Interconnect was removed, or because the other side of a Partner attachment was deleted.
      "type": "A String", # The type of interconnect attachment this is, which can take one of the following values: - DEDICATED: an attachment to a Dedicated Interconnect. - PARTNER: an attachment to a Partner Interconnect, created by the customer. - PARTNER_PROVIDER: an attachment to a Partner Interconnect, created by the partner.
      "vlanTag8021q": 42, # The IEEE 802.1Q VLAN tag for this attachment, in the range 2-4094. Only specified at creation time.
    }

      requestId: string, An optional request ID to identify requests. Specify a unique request ID so that if you must retry your request, the server will know to ignore the request if it has already been completed. For example, consider a situation where you make an initial request and the request times out. If you make the request again with the same request ID, the server can check if original operation with the same request ID was received, and if so, will ignore the second request. This prevents clients from accidentally creating duplicate commitments. The request ID must be a valid UUID with the exception that zero UUID is not supported ( 00000000-0000-0000-0000-000000000000).
      validateOnly: boolean, If true, the request will not be committed.
      x__xgafv: string, V1 error format.
        Allowed values
          1 - v1 error format
          2 - v2 error format

    Returns:
      An object of the form:

        { # Represents an Operation resource. Google Compute Engine has three Operation resources: * [Global](/compute/docs/reference/rest/alpha/globalOperations) * [Regional](/compute/docs/reference/rest/alpha/regionOperations) * [Zonal](/compute/docs/reference/rest/alpha/zoneOperations) You can use an operation resource to manage asynchronous API requests. For more information, read Handling API responses. Operations can be global, regional or zonal. - For global operations, use the `globalOperations` resource. - For regional operations, use the `regionOperations` resource. - For zonal operations, use the `zonalOperations` resource. For more information, read Global, Regional, and Zonal Resources.
      "clientOperationId": "A String", # [Output Only] The value of `requestId` if you provided it in the request. Not present otherwise.
      "creationTimestamp": "A String", # [Deprecated] This field is deprecated.
      "description": "A String", # [Output Only] A textual description of the operation, which is set when the operation is created.
      "endTime": "A String", # [Output Only] The time that this operation was completed. This value is in RFC3339 text format.
      "error": { # [Output Only] If errors are generated during processing of the operation, this field will be populated.
        "errors": [ # [Output Only] The array of errors encountered while processing this operation.
          {
            "code": "A String", # [Output Only] The error type identifier for this error.
            "location": "A String", # [Output Only] Indicates the field in the request that caused the error. This property is optional.
            "message": "A String", # [Output Only] An optional, human-readable error message.
          },
        ],
      },
      "httpErrorMessage": "A String", # [Output Only] If the operation fails, this field contains the HTTP error message that was returned, such as `NOT FOUND`.
      "httpErrorStatusCode": 42, # [Output Only] If the operation fails, this field contains the HTTP error status code that was returned. For example, a `404` means the resource was not found.
      "id": "A String", # [Output Only] The unique identifier for the operation. This identifier is defined by the server.
      "insertTime": "A String", # [Output Only] The time that this operation was requested. This value is in RFC3339 text format.
      "kind": "compute#operation", # [Output Only] Type of the resource. Always `compute#operation` for Operation resources.
      "name": "A String", # [Output Only] Name of the operation.
      "operationGroupId": "A String", # [Output Only] An ID that represents a group of operations, such as when a group of operations results from a `bulkInsert` API request.
      "operationType": "A String", # [Output Only] The type of operation, such as `insert`, `update`, or `delete`, and so on.
      "progress": 42, # [Output Only] An optional progress indicator that ranges from 0 to 100. There is no requirement that this be linear or support any granularity of operations. This should not be used to guess when the operation will be complete. This number should monotonically increase as the operation progresses.
      "region": "A String", # [Output Only] The URL of the region where the operation resides. Only applicable when performing regional operations.
      "selfLink": "A String", # [Output Only] Server-defined URL for the resource.
      "selfLinkWithId": "A String", # [Output Only] Server-defined URL for this resource with the resource id.
      "startTime": "A String", # [Output Only] The time that this operation was started by the server. This value is in RFC3339 text format.
      "status": "A String", # [Output Only] The status of the operation, which can be one of the following: `PENDING`, `RUNNING`, or `DONE`.
      "statusMessage": "A String", # [Output Only] An optional textual description of the current status of the operation.
      "targetId": "A String", # [Output Only] The unique target ID, which identifies a specific incarnation of the target resource.
      "targetLink": "A String", # [Output Only] The URL of the resource that the operation modifies. For operations related to creating a snapshot, this points to the persistent disk that the snapshot was created from.
      "user": "A String", # [Output Only] User who requested the operation, for example: `user@example.com`.
      "warnings": [ # [Output Only] If warning messages are generated during processing of the operation, this field will be populated.
        {
          "code": "A String", # [Output Only] A warning code, if applicable. For example, Compute Engine returns NO_RESULTS_ON_PAGE if there are no results in the response.
          "data": [ # [Output Only] Metadata about this warning in key: value format. For example: "data": [ { "key": "scope", "value": "zones/us-east1-d" }
            {
              "key": "A String", # [Output Only] A key that provides more detail on the warning being returned. For example, for warnings where there are no results in a list request for a particular zone, this key might be scope and the key value might be the zone name. Other examples might be a key indicating a deprecated resource and a suggested replacement, or a warning about invalid network settings (for example, if an instance attempts to perform IP forwarding but is not enabled for IP forwarding).
              "value": "A String", # [Output Only] A warning data value corresponding to the key.
            },
          ],
          "message": "A String", # [Output Only] A human-readable description of the warning code.
        },
      ],
      "zone": "A String", # [Output Only] The URL of the zone where the operation resides. Only applicable when performing per-zone operations.
    }

`list(project, region, filter=None, maxResults=None, orderBy=None, pageToken=None, returnPartialSuccess=None, x__xgafv=None)`

    Retrieves the list of interconnect attachments contained within the specified region.

    Args:
      project: string, Project ID for this request. (required)
      region: string, Name of the region for this request. (required)
      filter: string, A filter expression that filters resources listed in the response. The expression must specify the field name, a comparison operator, and the value that you want to use for filtering. The value must be a string, a number, or a boolean. The comparison operator must be either `=`, `!=`, `>`, or `<`. For example, if you are filtering Compute Engine instances, you can exclude instances named `example-instance` by specifying `name != example-instance`. You can also filter nested fields. For example, you could specify `scheduling.automaticRestart = false` to include instances only if they are not scheduled for automatic restarts. You can use filtering on nested fields to filter based on resource labels. To filter on multiple expressions, provide each separate expression within parentheses. For example: ``` (scheduling.automaticRestart = true) (cpuPlatform = "Intel Skylake") ``` By default, each expression is an `AND` expression. However, you can include `AND` and `OR` expressions explicitly. For example: ``` (cpuPlatform = "Intel Skylake") OR (cpuPlatform = "Intel Broadwell") AND (scheduling.automaticRestart = true) ```
      maxResults: integer, The maximum number of results per page that should be returned. If the number of available results is larger than `maxResults`, Compute Engine returns a `nextPageToken` that can be used to get the next page of results in subsequent list requests. Acceptable values are `0` to `500`, inclusive. (Default: `500`)
      orderBy: string, Sorts list results by a certain order. By default, results are returned in alphanumerical order based on the resource name. You can also sort results in descending order based on the creation timestamp using `orderBy="creationTimestamp desc"`. This sorts results based on the `creationTimestamp` field in reverse chronological order (newest result first). Use this to sort resources like operations so that the newest operation is returned first. Currently, only sorting by `name` or `creationTimestamp desc` is supported.
      pageToken: string, Specifies a page token to use. Set `pageToken` to the `nextPageToken` returned by a previous list request to get the next page of results.
      returnPartialSuccess: boolean, Opt-in for partial success behavior which provides partial results in case of failure. The default value is false.
      x__xgafv: string, V1 error format.
        Allowed values
          1 - v1 error format
          2 - v2 error format

    Returns:
      An object of the form:

        { # Response to the list request, and contains a list of interconnect attachments.
      "id": "A String", # [Output Only] Unique identifier for the resource; defined by the server.
      "items": [ # A list of InterconnectAttachment resources.
        { # Represents an Interconnect Attachment (VLAN) resource. You can use Interconnect attachments (VLANS) to connect your Virtual Private Cloud networks to your on-premises networks through an Interconnect. For more information, read Creating VLAN Attachments.
          "adminEnabled": True or False, # Determines whether this Attachment will carry packets. Not present for PARTNER_PROVIDER.
          "bandwidth": "A String", # Provisioned bandwidth capacity for the interconnect attachment. For attachments of type DEDICATED, the user can set the bandwidth. For attachments of type PARTNER, the Google Partner that is operating the interconnect must set the bandwidth. Output only for PARTNER type, mutable for PARTNER_PROVIDER and DEDICATED, and can take one of the following values: - BPS_50M: 50 Mbit/s - BPS_100M: 100 Mbit/s - BPS_200M: 200 Mbit/s - BPS_300M: 300 Mbit/s - BPS_400M: 400 Mbit/s - BPS_500M: 500 Mbit/s - BPS_1G: 1 Gbit/s - BPS_2G: 2 Gbit/s - BPS_5G: 5 Gbit/s - BPS_10G: 10 Gbit/s - BPS_20G: 20 Gbit/s - BPS_50G: 50 Gbit/s
          "candidateIpv6Subnets": [ # Up to 16 candidate prefixes that control the allocation of cloudRouterIpv6Address and customerRouterIpv6Address for this attachment. Each prefix must be in the Global Unique Address (GUA) space. It is highly recommended that it be in a range owned by the requestor. A GUA in a range owned by Google will cause the request to fail. Google will select an available prefix from the supplied candidates or fail the request. If not supplied, a /125 from a Google-owned GUA block will be selected.
            "A String",
          ],
          "candidateSubnets": [ # Up to 16 candidate prefixes that can be used to restrict the allocation of cloudRouterIpAddress and customerRouterIpAddress for this attachment. All prefixes must be within link-local address space (169.254.0.0/16) and must be /29 or shorter (/28, /27, etc). Google will attempt to select an unused /29 from the supplied candidate prefix(es). The request will fail if all possible /29s are in use on Google's edge. If not supplied, Google will randomly select an unused /29 from all of link-local space.
            "A String",
          ],
          "cloudRouterIpAddress": "A String", # [Output Only] IPv4 address + prefix length to be configured on Cloud Router Interface for this interconnect attachment.
          "cloudRouterIpv6Address": "A String", # [Output Only] IPv6 address + prefix length to be configured on Cloud Router Interface for this interconnect attachment.
          "cloudRouterIpv6InterfaceId": "A String", # If supplied, the interface id (index within the subnet) to be used for the cloud router address. The id must be in the range of 1 to 6. If a subnet mask is supplied, it must be /125, and the subnet should either be 0 or match the selected subnet.
          "creationTimestamp": "A String", # [Output Only] Creation timestamp in RFC3339 text format.
          "customerRouterIpAddress": "A String", # [Output Only] IPv4 address + prefix length to be configured on the customer router subinterface for this interconnect attachment.
          "customerRouterIpv6Address": "A String", # [Output Only] IPv6 address + prefix length to be configured on the customer router subinterface for this interconnect attachment.
          "customerRouterIpv6InterfaceId": "A String", # If supplied, the interface id (index within the subnet) to be used for the customer router address. The id must be in the range of 1 to 6. If a subnet mask is supplied, it must be /125, and the subnet should either be 0 or match the selected subnet.
          "dataplaneVersion": 42, # [Output Only] Dataplane version for this InterconnectAttachment.
          "description": "A String", # An optional description of this resource.
          "edgeAvailabilityDomain": "A String", # Desired availability domain for the attachment. Only available for type PARTNER, at creation time, and can take one of the following values: - AVAILABILITY_DOMAIN_ANY - AVAILABILITY_DOMAIN_1 - AVAILABILITY_DOMAIN_2 For improved reliability, customers should configure a pair of attachments, one per availability domain. The selected availability domain will be provided to the Partner via the pairing key, so that the provisioned circuit will lie in the specified domain. If not specified, the value will default to AVAILABILITY_DOMAIN_ANY.
          "encryption": "A String", # Indicates the user-supplied encryption option of this VLAN attachment (interconnectAttachment). Can only be specified at attachment creation for PARTNER or DEDICATED attachments. Possible values are: - NONE - This is the default value, which means that the VLAN attachment carries unencrypted traffic. VMs are able to send traffic to, or receive traffic from, such a VLAN attachment. - IPSEC - The VLAN attachment carries only encrypted traffic that is encrypted by an IPsec device, such as an HA VPN gateway or third-party IPsec VPN. VMs cannot directly send traffic to, or receive traffic from, such a VLAN attachment. To use *IPsec-encrypted Cloud Interconnect*, the VLAN attachment must be created with this option. Not currently available publicly.
          "googleReferenceId": "A String", # [Output Only] Google reference ID, to be used when raising support tickets with Google or otherwise to debug backend connectivity issues. [Deprecated] This field is not used.
          "id": "A String", # [Output Only] The unique identifier for the resource. This identifier is defined by the server.
          "interconnect": "A String", # URL of the underlying Interconnect object that this attachment's traffic will traverse through.
          "ipsecInternalAddresses": [ # A list of URLs of addresses that have been reserved for the VLAN attachment. Used only for the VLAN attachment that has the encryption option as IPSEC. The addresses must be regional internal IP address ranges. When creating an HA VPN gateway over the VLAN attachment, if the attachment is configured to use a regional internal IP address, then the VPN gateway's IP address is allocated from the IP address range specified here. For example, if the HA VPN gateway's interface 0 is paired to this VLAN attachment, then a regional internal IP address for the VPN gateway interface 0 will be allocated from the IP address specified for this VLAN attachment. If this field is not specified when creating the VLAN attachment, then later on when creating an HA VPN gateway on this VLAN attachment, the HA VPN gateway's IP address is allocated from the regional external IP address pool. Not currently available publicly.
            "A String",
          ],
          "kind": "compute#interconnectAttachment", # [Output Only] Type of the resource. Always compute#interconnectAttachment for interconnect attachments.
          "labelFingerprint": "A String", # A fingerprint for the labels being applied to this InterconnectAttachment, which is essentially a hash of the labels set used for optimistic locking. The fingerprint is initially generated by Compute Engine and changes after every request to modify or update labels. You must always provide an up-to-date fingerprint hash in order to update or change labels, otherwise the request will fail with error 412 conditionNotMet. To see the latest fingerprint, make a get() request to retrieve an InterconnectAttachment.
          "labels": { # Labels for this resource. These can only be added or modified by the setLabels method. Each label key/value pair must comply with RFC1035. Label values may be empty.
            "a_key": "A String",
          },
          "mtu": 42, # Maximum Transmission Unit (MTU), in bytes, of packets passing through this interconnect attachment. Only 1440 and 1500 are allowed. If not specified, the value will default to 1440.
          "name": "A String", # Name of the resource. Provided by the client when the resource is created. The name must be 1-63 characters long, and comply with RFC1035. Specifically, the name must be 1-63 characters long and match the regular expression `[a-z]([-a-z0-9]*[a-z0-9])?` which means the first character must be a lowercase letter, and all following characters must be a dash, lowercase letter, or digit, except the last character, which cannot be a dash.
          "operationalStatus": "A String", # [Output Only] The current status of whether or not this interconnect attachment is functional, which can take one of the following values: - OS_ACTIVE: The attachment has been turned up and is ready to use. - OS_UNPROVISIONED: The attachment is not ready to use yet, because turnup is not complete.
          "pairingKey": "A String", # [Output only for type PARTNER. Input only for PARTNER_PROVIDER. Not present for DEDICATED]. The opaque identifier of an PARTNER attachment used to initiate provisioning with a selected partner. Of the form "XXXXX/region/domain"
          "partnerAsn": "A String", # Optional BGP ASN for the router supplied by a Layer 3 Partner if they configured BGP on behalf of the customer. Output only for PARTNER type, input only for PARTNER_PROVIDER, not available for DEDICATED.
          "partnerMetadata": { # Informational metadata about Partner attachments from Partners to display to customers. These fields are propagated from PARTNER_PROVIDER attachments to their corresponding PARTNER attachments. # Informational metadata about Partner attachments from Partners to display to customers. Output only for for PARTNER type, mutable for PARTNER_PROVIDER, not available for DEDICATED.
            "interconnectName": "A String", # Plain text name of the Interconnect this attachment is connected to, as displayed in the Partner's portal. For instance "Chicago 1". This value may be validated to match approved Partner values.
            "partnerName": "A String", # Plain text name of the Partner providing this attachment. This value may be validated to match approved Partner values.
            "portalUrl": "A String", # URL of the Partner's portal for this Attachment. Partners may customise this to be a deep link to the specific resource on the Partner portal. This value may be validated to match approved Partner values.
          },
          "privateInterconnectInfo": { # Information for an interconnect attachment when this belongs to an interconnect of type DEDICATED. # [Output Only] Information specific to an InterconnectAttachment. This property is populated if the interconnect that this is attached to is of type DEDICATED.
            "tag8021q": 42, # [Output Only] 802.1q encapsulation tag to be used for traffic between Google and the customer, going to and from this network and region.
          },
          "region": "A String", # [Output Only] URL of the region where the regional interconnect attachment resides. You must specify this field as part of the HTTP request URL. It is not settable as a field in the request body.
          "router": "A String", # URL of the Cloud Router to be used for dynamic routing. This router must be in the same region as this InterconnectAttachment. The InterconnectAttachment will automatically connect the Interconnect to the network & region within which the Cloud Router is configured.
          "satisfiesPzs": True or False, # [Output Only] Set to true if the resource satisfies the zone separation organization policy constraints and false otherwise. Defaults to false if the field is not present.
          "selfLink": "A String", # [Output Only] Server-defined URL for the resource.
          "selfLinkWithId": "A String", # [Output Only] Server-defined URL for this resource with the resource id.
          "stackType": "A String", # The stack type for this interconnect attachment to identify whether the IPv6 feature is enabled or not. If not specified, IPV4_ONLY will be used. This field can be both set at interconnect attachments creation and update interconnect attachment operations.
          "state": "A String", # [Output Only] The current state of this attachment's functionality. Enum values ACTIVE and UNPROVISIONED are shared by DEDICATED/PRIVATE, PARTNER, and PARTNER_PROVIDER interconnect attachments, while enum values PENDING_PARTNER, PARTNER_REQUEST_RECEIVED, and PENDING_CUSTOMER are used for only PARTNER and PARTNER_PROVIDER interconnect attachments. This state can take one of the following values: - ACTIVE: The attachment has been turned up and is ready to use. - UNPROVISIONED: The attachment is not ready to use yet, because turnup is not complete. - PENDING_PARTNER: A newly-created PARTNER attachment that has not yet been configured on the Partner side. - PARTNER_REQUEST_RECEIVED: A PARTNER attachment is in the process of provisioning after a PARTNER_PROVIDER attachment was created that references it. - PENDING_CUSTOMER: A PARTNER or PARTNER_PROVIDER attachment that is waiting for a customer to activate it. - DEFUNCT: The attachment was deleted externally and is no longer functional. This could be because the associated Interconnect was removed, or because the other side of a Partner attachment was deleted.
          "type": "A String", # The type of interconnect attachment this is, which can take one of the following values: - DEDICATED: an attachment to a Dedicated Interconnect. - PARTNER: an attachment to a Partner Interconnect, created by the customer. - PARTNER_PROVIDER: an attachment to a Partner Interconnect, created by the partner.
          "vlanTag8021q": 42, # The IEEE 802.1Q VLAN tag for this attachment, in the range 2-4094. Only specified at creation time.
        },
      ],
      "kind": "compute#interconnectAttachmentList", # [Output Only] Type of resource. Always compute#interconnectAttachmentList for lists of interconnect attachments.
      "nextPageToken": "A String", # [Output Only] This token allows you to get the next page of results for list requests. If the number of results is larger than maxResults, use the nextPageToken as a value for the query parameter pageToken in the next list request. Subsequent list requests will have their own nextPageToken to continue paging through the results.
      "selfLink": "A String", # [Output Only] Server-defined URL for this resource.
      "warning": { # [Output Only] Informational warning message.
        "code": "A String", # [Output Only] A warning code, if applicable. For example, Compute Engine returns NO_RESULTS_ON_PAGE if there are no results in the response.
        "data": [ # [Output Only] Metadata about this warning in key: value format. For example: "data": [ { "key": "scope", "value": "zones/us-east1-d" }
          {
            "key": "A String", # [Output Only] A key that provides more detail on the warning being returned. For example, for warnings where there are no results in a list request for a particular zone, this key might be scope and the key value might be the zone name. Other examples might be a key indicating a deprecated resource and a suggested replacement, or a warning about invalid network settings (for example, if an instance attempts to perform IP forwarding but is not enabled for IP forwarding).
            "value": "A String", # [Output Only] A warning data value corresponding to the key.
          },
        ],
        "message": "A String", # [Output Only] A human-readable description of the warning code.
      },
    }

`list_next(previous_request, previous_response)`

    Retrieves the next page of results.

    Args:
      previous_request: The request for the previous page. (required)
      previous_response: The response from the request for the previous page. (required)

    Returns:
      A request object that you can call 'execute()' on to request the next
      page. Returns None if there are no more items in the collection.

`patch(project, region, interconnectAttachment, body=None, requestId=None, x__xgafv=None)`

    Updates the specified interconnect attachment with the data included in the request. This method supports PATCH semantics and uses the JSON merge patch format and processing rules.

    Args:
      project: string, Project ID for this request. (required)
      region: string, Name of the region scoping this request. (required)
      interconnectAttachment: string, Name of the interconnect attachment to patch. (required)
      body: object, The request body.
        The object takes the form of:

    { # Represents an Interconnect Attachment (VLAN) resource. You can use Interconnect attachments (VLANS) to connect your Virtual Private Cloud networks to your on-premises networks through an Interconnect. For more information, read Creating VLAN Attachments.
      "adminEnabled": True or False, # Determines whether this Attachment will carry packets. Not present for PARTNER_PROVIDER.
      "bandwidth": "A String", # Provisioned bandwidth capacity for the interconnect attachment. For attachments of type DEDICATED, the user can set the bandwidth. For attachments of type PARTNER, the Google Partner that is operating the interconnect must set the bandwidth. Output only for PARTNER type, mutable for PARTNER_PROVIDER and DEDICATED, and can take one of the following values: - BPS_50M: 50 Mbit/s - BPS_100M: 100 Mbit/s - BPS_200M: 200 Mbit/s - BPS_300M: 300 Mbit/s - BPS_400M: 400 Mbit/s - BPS_500M: 500 Mbit/s - BPS_1G: 1 Gbit/s - BPS_2G: 2 Gbit/s - BPS_5G: 5 Gbit/s - BPS_10G: 10 Gbit/s - BPS_20G: 20 Gbit/s - BPS_50G: 50 Gbit/s
      "candidateIpv6Subnets": [ # Up to 16 candidate prefixes that control the allocation of cloudRouterIpv6Address and customerRouterIpv6Address for this attachment. Each prefix must be in the Global Unique Address (GUA) space. It is highly recommended that it be in a range owned by the requestor. A GUA in a range owned by Google will cause the request to fail. Google will select an available prefix from the supplied candidates or fail the request. If not supplied, a /125 from a Google-owned GUA block will be selected.
        "A String",
      ],
      "candidateSubnets": [ # Up to 16 candidate prefixes that can be used to restrict the allocation of cloudRouterIpAddress and customerRouterIpAddress for this attachment. All prefixes must be within link-local address space (169.254.0.0/16) and must be /29 or shorter (/28, /27, etc). Google will attempt to select an unused /29 from the supplied candidate prefix(es). The request will fail if all possible /29s are in use on Google's edge. If not supplied, Google will randomly select an unused /29 from all of link-local space.
        "A String",
      ],
      "cloudRouterIpAddress": "A String", # [Output Only] IPv4 address + prefix length to be configured on Cloud Router Interface for this interconnect attachment.
      "cloudRouterIpv6Address": "A String", # [Output Only] IPv6 address + prefix length to be configured on Cloud Router Interface for this interconnect attachment.
      "cloudRouterIpv6InterfaceId": "A String", # If supplied, the interface id (index within the subnet) to be used for the cloud router address. The id must be in the range of 1 to 6. If a subnet mask is supplied, it must be /125, and the subnet should either be 0 or match the selected subnet.
      "creationTimestamp": "A String", # [Output Only] Creation timestamp in RFC3339 text format.
      "customerRouterIpAddress": "A String", # [Output Only] IPv4 address + prefix length to be configured on the customer router subinterface for this interconnect attachment.
      "customerRouterIpv6Address": "A String", # [Output Only] IPv6 address + prefix length to be configured on the customer router subinterface for this interconnect attachment.
      "customerRouterIpv6InterfaceId": "A String", # If supplied, the interface id (index within the subnet) to be used for the customer router address. The id must be in the range of 1 to 6. If a subnet mask is supplied, it must be /125, and the subnet should either be 0 or match the selected subnet.
      "dataplaneVersion": 42, # [Output Only] Dataplane version for this InterconnectAttachment.
      "description": "A String", # An optional description of this resource.
      "edgeAvailabilityDomain": "A String", # Desired availability domain for the attachment. Only available for type PARTNER, at creation time, and can take one of the following values: - AVAILABILITY_DOMAIN_ANY - AVAILABILITY_DOMAIN_1 - AVAILABILITY_DOMAIN_2 For improved reliability, customers should configure a pair of attachments, one per availability domain. The selected availability domain will be provided to the Partner via the pairing key, so that the provisioned circuit will lie in the specified domain. If not specified, the value will default to AVAILABILITY_DOMAIN_ANY.
      "encryption": "A String", # Indicates the user-supplied encryption option of this VLAN attachment (interconnectAttachment). Can only be specified at attachment creation for PARTNER or DEDICATED attachments. Possible values are: - NONE - This is the default value, which means that the VLAN attachment carries unencrypted traffic. VMs are able to send traffic to, or receive traffic from, such a VLAN attachment. - IPSEC - The VLAN attachment carries only encrypted traffic that is encrypted by an IPsec device, such as an HA VPN gateway or third-party IPsec VPN. VMs cannot directly send traffic to, or receive traffic from, such a VLAN attachment. To use *IPsec-encrypted Cloud Interconnect*, the VLAN attachment must be created with this option. Not currently available publicly.
      "googleReferenceId": "A String", # [Output Only] Google reference ID, to be used when raising support tickets with Google or otherwise to debug backend connectivity issues. [Deprecated] This field is not used.
      "id": "A String", # [Output Only] The unique identifier for the resource. This identifier is defined by the server.
      "interconnect": "A String", # URL of the underlying Interconnect object that this attachment's traffic will traverse through.
      "ipsecInternalAddresses": [ # A list of URLs of addresses that have been reserved for the VLAN attachment. Used only for the VLAN attachment that has the encryption option as IPSEC. The addresses must be regional internal IP address ranges. When creating an HA VPN gateway over the VLAN attachment, if the attachment is configured to use a regional internal IP address, then the VPN gateway's IP address is allocated from the IP address range specified here. For example, if the HA VPN gateway's interface 0 is paired to this VLAN attachment, then a regional internal IP address for the VPN gateway interface 0 will be allocated from the IP address specified for this VLAN attachment. If this field is not specified when creating the VLAN attachment, then later on when creating an HA VPN gateway on this VLAN attachment, the HA VPN gateway's IP address is allocated from the regional external IP address pool. Not currently available publicly.
        "A String",
      ],
      "kind": "compute#interconnectAttachment", # [Output Only] Type of the resource. Always compute#interconnectAttachment for interconnect attachments.
      "labelFingerprint": "A String", # A fingerprint for the labels being applied to this InterconnectAttachment, which is essentially a hash of the labels set used for optimistic locking. The fingerprint is initially generated by Compute Engine and changes after every request to modify or update labels. You must always provide an up-to-date fingerprint hash in order to update or change labels, otherwise the request will fail with error 412 conditionNotMet. To see the latest fingerprint, make a get() request to retrieve an InterconnectAttachment.
      "labels": { # Labels for this resource. These can only be added or modified by the setLabels method. Each label key/value pair must comply with RFC1035. Label values may be empty.
        "a_key": "A String",
      },
      "mtu": 42, # Maximum Transmission Unit (MTU), in bytes, of packets passing through this interconnect attachment. Only 1440 and 1500 are allowed. If not specified, the value will default to 1440.
      "name": "A String", # Name of the resource. Provided by the client when the resource is created. The name must be 1-63 characters long, and comply with RFC1035. Specifically, the name must be 1-63 characters long and match the regular expression `[a-z]([-a-z0-9]*[a-z0-9])?` which means the first character must be a lowercase letter, and all following characters must be a dash, lowercase letter, or digit, except the last character, which cannot be a dash.
      "operationalStatus": "A String", # [Output Only] The current status of whether or not this interconnect attachment is functional, which can take one of the following values: - OS_ACTIVE: The attachment has been turned up and is ready to use. - OS_UNPROVISIONED: The attachment is not ready to use yet, because turnup is not complete.
      "pairingKey": "A String", # [Output only for type PARTNER. Input only for PARTNER_PROVIDER. Not present for DEDICATED]. The opaque identifier of an PARTNER attachment used to initiate provisioning with a selected partner. Of the form "XXXXX/region/domain"
      "partnerAsn": "A String", # Optional BGP ASN for the router supplied by a Layer 3 Partner if they configured BGP on behalf of the customer. Output only for PARTNER type, input only for PARTNER_PROVIDER, not available for DEDICATED.
      "partnerMetadata": { # Informational metadata about Partner attachments from Partners to display to customers. These fields are propagated from PARTNER_PROVIDER attachments to their corresponding PARTNER attachments. # Informational metadata about Partner attachments from Partners to display to customers. Output only for for PARTNER type, mutable for PARTNER_PROVIDER, not available for DEDICATED.
        "interconnectName": "A String", # Plain text name of the Interconnect this attachment is connected to, as displayed in the Partner's portal. For instance "Chicago 1". This value may be validated to match approved Partner values.
        "partnerName": "A String", # Plain text name of the Partner providing this attachment. This value may be validated to match approved Partner values.
        "portalUrl": "A String", # URL of the Partner's portal for this Attachment. Partners may customise this to be a deep link to the specific resource on the Partner portal. This value may be validated to match approved Partner values.
      },
      "privateInterconnectInfo": { # Information for an interconnect attachment when this belongs to an interconnect of type DEDICATED. # [Output Only] Information specific to an InterconnectAttachment. This property is populated if the interconnect that this is attached to is of type DEDICATED.
        "tag8021q": 42, # [Output Only] 802.1q encapsulation tag to be used for traffic between Google and the customer, going to and from this network and region.
      },
      "region": "A String", # [Output Only] URL of the region where the regional interconnect attachment resides. You must specify this field as part of the HTTP request URL. It is not settable as a field in the request body.
      "router": "A String", # URL of the Cloud Router to be used for dynamic routing. This router must be in the same region as this InterconnectAttachment. The InterconnectAttachment will automatically connect the Interconnect to the network & region within which the Cloud Router is configured.
      "satisfiesPzs": True or False, # [Output Only] Set to true if the resource satisfies the zone separation organization policy constraints and false otherwise. Defaults to false if the field is not present.
      "selfLink": "A String", # [Output Only] Server-defined URL for the resource.
      "selfLinkWithId": "A String", # [Output Only] Server-defined URL for this resource with the resource id.
      "stackType": "A String", # The stack type for this interconnect attachment to identify whether the IPv6 feature is enabled or not. If not specified, IPV4_ONLY will be used. This field can be both set at interconnect attachments creation and update interconnect attachment operations.
      "state": "A String", # [Output Only] The current state of this attachment's functionality. Enum values ACTIVE and UNPROVISIONED are shared by DEDICATED/PRIVATE, PARTNER, and PARTNER_PROVIDER interconnect attachments, while enum values PENDING_PARTNER, PARTNER_REQUEST_RECEIVED, and PENDING_CUSTOMER are used for only PARTNER and PARTNER_PROVIDER interconnect attachments. This state can take one of the following values: - ACTIVE: The attachment has been turned up and is ready to use. - UNPROVISIONED: The attachment is not ready to use yet, because turnup is not complete. - PENDING_PARTNER: A newly-created PARTNER attachment that has not yet been configured on the Partner side. - PARTNER_REQUEST_RECEIVED: A PARTNER attachment is in the process of provisioning after a PARTNER_PROVIDER attachment was created that references it. - PENDING_CUSTOMER: A PARTNER or PARTNER_PROVIDER attachment that is waiting for a customer to activate it. - DEFUNCT: The attachment was deleted externally and is no longer functional. This could be because the associated Interconnect was removed, or because the other side of a Partner attachment was deleted.
      "type": "A String", # The type of interconnect attachment this is, which can take one of the following values: - DEDICATED: an attachment to a Dedicated Interconnect. - PARTNER: an attachment to a Partner Interconnect, created by the customer. - PARTNER_PROVIDER: an attachment to a Partner Interconnect, created by the partner.
      "vlanTag8021q": 42, # The IEEE 802.1Q VLAN tag for this attachment, in the range 2-4094. Only specified at creation time.
    }

      requestId: string, An optional request ID to identify requests. Specify a unique request ID so that if you must retry your request, the server will know to ignore the request if it has already been completed. For example, consider a situation where you make an initial request and the request times out. If you make the request again with the same request ID, the server can check if original operation with the same request ID was received, and if so, will ignore the second request. This prevents clients from accidentally creating duplicate commitments. The request ID must be a valid UUID with the exception that zero UUID is not supported ( 00000000-0000-0000-0000-000000000000).
      x__xgafv: string, V1 error format.
        Allowed values
          1 - v1 error format
          2 - v2 error format

    Returns:
      An object of the form:

        { # Represents an Operation resource. Google Compute Engine has three Operation resources: * [Global](/compute/docs/reference/rest/alpha/globalOperations) * [Regional](/compute/docs/reference/rest/alpha/regionOperations) * [Zonal](/compute/docs/reference/rest/alpha/zoneOperations) You can use an operation resource to manage asynchronous API requests. For more information, read Handling API responses. Operations can be global, regional or zonal. - For global operations, use the `globalOperations` resource. - For regional operations, use the `regionOperations` resource. - For zonal operations, use the `zonalOperations` resource. For more information, read Global, Regional, and Zonal Resources.
      "clientOperationId": "A String", # [Output Only] The value of `requestId` if you provided it in the request. Not present otherwise.
      "creationTimestamp": "A String", # [Deprecated] This field is deprecated.
      "description": "A String", # [Output Only] A textual description of the operation, which is set when the operation is created.
      "endTime": "A String", # [Output Only] The time that this operation was completed. This value is in RFC3339 text format.
      "error": { # [Output Only] If errors are generated during processing of the operation, this field will be populated.
        "errors": [ # [Output Only] The array of errors encountered while processing this operation.
          {
            "code": "A String", # [Output Only] The error type identifier for this error.
            "location": "A String", # [Output Only] Indicates the field in the request that caused the error. This property is optional.
            "message": "A String", # [Output Only] An optional, human-readable error message.
          },
        ],
      },
      "httpErrorMessage": "A String", # [Output Only] If the operation fails, this field contains the HTTP error message that was returned, such as `NOT FOUND`.
      "httpErrorStatusCode": 42, # [Output Only] If the operation fails, this field contains the HTTP error status code that was returned. For example, a `404` means the resource was not found.
      "id": "A String", # [Output Only] The unique identifier for the operation. This identifier is defined by the server.
      "insertTime": "A String", # [Output Only] The time that this operation was requested. This value is in RFC3339 text format.
      "kind": "compute#operation", # [Output Only] Type of the resource. Always `compute#operation` for Operation resources.
      "name": "A String", # [Output Only] Name of the operation.
      "operationGroupId": "A String", # [Output Only] An ID that represents a group of operations, such as when a group of operations results from a `bulkInsert` API request.
      "operationType": "A String", # [Output Only] The type of operation, such as `insert`, `update`, or `delete`, and so on.
      "progress": 42, # [Output Only] An optional progress indicator that ranges from 0 to 100. There is no requirement that this be linear or support any granularity of operations. This should not be used to guess when the operation will be complete. This number should monotonically increase as the operation progresses.
      "region": "A String", # [Output Only] The URL of the region where the operation resides. Only applicable when performing regional operations.
      "selfLink": "A String", # [Output Only] Server-defined URL for the resource.
      "selfLinkWithId": "A String", # [Output Only] Server-defined URL for this resource with the resource id.
      "startTime": "A String", # [Output Only] The time that this operation was started by the server. This value is in RFC3339 text format.
      "status": "A String", # [Output Only] The status of the operation, which can be one of the following: `PENDING`, `RUNNING`, or `DONE`.
      "statusMessage": "A String", # [Output Only] An optional textual description of the current status of the operation.
      "targetId": "A String", # [Output Only] The unique target ID, which identifies a specific incarnation of the target resource.
      "targetLink": "A String", # [Output Only] The URL of the resource that the operation modifies. For operations related to creating a snapshot, this points to the persistent disk that the snapshot was created from.
      "user": "A String", # [Output Only] User who requested the operation, for example: `user@example.com`.
      "warnings": [ # [Output Only] If warning messages are generated during processing of the operation, this field will be populated.
        {
          "code": "A String", # [Output Only] A warning code, if applicable. For example, Compute Engine returns NO_RESULTS_ON_PAGE if there are no results in the response.
          "data": [ # [Output Only] Metadata about this warning in key: value format. For example: "data": [ { "key": "scope", "value": "zones/us-east1-d" }
            {
              "key": "A String", # [Output Only] A key that provides more detail on the warning being returned. For example, for warnings where there are no results in a list request for a particular zone, this key might be scope and the key value might be the zone name. Other examples might be a key indicating a deprecated resource and a suggested replacement, or a warning about invalid network settings (for example, if an instance attempts to perform IP forwarding but is not enabled for IP forwarding).
              "value": "A String", # [Output Only] A warning data value corresponding to the key.
            },
          ],
          "message": "A String", # [Output Only] A human-readable description of the warning code.
        },
      ],
      "zone": "A String", # [Output Only] The URL of the zone where the operation resides. Only applicable when performing per-zone operations.
    }

`setIamPolicy(project, region, resource, body=None, x__xgafv=None)`

    Sets the access control policy on the specified resource. Replaces any existing policy.

    Args:
      project: string, Project ID for this request. (required)
      region: string, The name of the region for this request. (required)
      resource: string, Name or id of the resource for this request. (required)
      body: object, The request body.
        The object takes the form of:

    {
      "bindings": [ # Flatten Policy to create a backwacd compatible wire-format. Deprecated. Use 'policy' to specify bindings.
        { # Associates `members` with a `role`.
          "bindingId": "A String", # This is deprecated and has no effect. Do not use.
          "condition": { # Represents a textual expression in the Common Expression Language (CEL) syntax. CEL is a C-like expression language. The syntax and semantics of CEL are documented at https://github.com/google/cel-spec. Example (Comparison): title: "Summary size limit" description: "Determines if a summary is less than 100 chars" expression: "document.summary.size() < 100" Example (Equality): title: "Requestor is owner" description: "Determines if requestor is the document owner" expression: "document.owner == request.auth.claims.email" Example (Logic): title: "Public documents" description: "Determine whether the document should be publicly visible" expression: "document.type != 'private' && document.type != 'internal'" Example (Data Manipulation): title: "Notification string" description: "Create a notification string with a timestamp." expression: "'New message received at ' + string(document.create_time)" The exact variables and functions that may be referenced within an expression are determined by the service that evaluates it. See the service documentation for additional information. # The condition that is associated with this binding. If the condition evaluates to `true`, then this binding applies to the current request. If the condition evaluates to `false`, then this binding does not apply to the current request. However, a different role binding might grant the same role to one or more of the members in this binding. To learn which resources support conditions in their IAM policies, see the [IAM documentation](https://cloud.google.com/iam/help/conditions/resource-policies).
            "description": "A String", # Optional. Description of the expression. This is a longer text which describes the expression, e.g. when hovered over it in a UI.
            "expression": "A String", # Textual representation of an expression in Common Expression Language syntax.
            "location": "A String", # Optional. String indicating the location of the expression for error reporting, e.g. a file name and a position in the file.
            "title": "A String", # Optional. Title for the expression, i.e. a short string describing its purpose. This can be used e.g. in UIs which allow to enter the expression.
          },
          "members": [ # Specifies the identities requesting access for a Cloud Platform resource. `members` can have the following values: * `allUsers`: A special identifier that represents anyone who is on the internet; with or without a Google account. * `allAuthenticatedUsers`: A special identifier that represents anyone who is authenticated with a Google account or a service account. * `user:{emailid}`: An email address that represents a specific Google account. For example, `alice@example.com` . * `serviceAccount:{emailid}`: An email address that represents a service account. For example, `my-other-app@appspot.gserviceaccount.com`. * `group:{emailid}`: An email address that represents a Google group. For example, `admins@example.com`. * `deleted:user:{emailid}?uid={uniqueid}`: An email address (plus unique identifier) representing a user that has been recently deleted. For example, `alice@example.com?uid=123456789012345678901`. If the user is recovered, this value reverts to `user:{emailid}` and the recovered user retains the role in the binding. * `deleted:serviceAccount:{emailid}?uid={uniqueid}`: An email address (plus unique identifier) representing a service account that has been recently deleted. For example, `my-other-app@appspot.gserviceaccount.com?uid=123456789012345678901`. If the service account is undeleted, this value reverts to `serviceAccount:{emailid}` and the undeleted service account retains the role in the binding. * `deleted:group:{emailid}?uid={uniqueid}`: An email address (plus unique identifier) representing a Google group that has been recently deleted. For example, `admins@example.com?uid=123456789012345678901`. If the group is recovered, this value reverts to `group:{emailid}` and the recovered group retains the role in the binding. * `domain:{domain}`: The G Suite domain (primary) that represents all the users of that domain. For example, `google.com` or `example.com`.
            "A String",
          ],
          "role": "A String", # Role that is assigned to `members`. For example, `roles/viewer`, `roles/editor`, or `roles/owner`.
        },
      ],
      "etag": "A String", # Flatten Policy to create a backward compatible wire-format. Deprecated. Use 'policy' to specify the etag.
      "policy": { # An Identity and Access Management (IAM) policy, which specifies access controls for Google Cloud resources. A `Policy` is a collection of `bindings`. A `binding` binds one or more `members` to a single `role`. Members can be user accounts, service accounts, Google groups, and domains (such as G Suite). A `role` is a named list of permissions; each `role` can be an IAM predefined role or a user-created custom role. For some types of Google Cloud resources, a `binding` can also specify a `condition`, which is a logical expression that allows access to a resource only if the expression evaluates to `true`. A condition can add constraints based on attributes of the request, the resource, or both. To learn which resources support conditions in their IAM policies, see the [IAM documentation](https://cloud.google.com/iam/help/conditions/resource-policies). **JSON example:** { "bindings": [ { "role": "roles/resourcemanager.organizationAdmin", "members": [ "user:mike@example.com", "group:admins@example.com", "domain:google.com", "serviceAccount:my-project-id@appspot.gserviceaccount.com" ] }, { "role": "roles/resourcemanager.organizationViewer", "members": [ "user:eve@example.com" ], "condition": { "title": "expirable access", "description": "Does not grant access after Sep 2020", "expression": "request.time < timestamp('2020-10-01T00:00:00.000Z')", } } ], "etag": "BwWWja0YfJA=", "version": 3 } **YAML example:** bindings: - members: - user:mike@example.com - group:admins@example.com - domain:google.com - serviceAccount:my-project-id@appspot.gserviceaccount.com role: roles/resourcemanager.organizationAdmin - members: - user:eve@example.com role: roles/resourcemanager.organizationViewer condition: title: expirable access description: Does not grant access after Sep 2020 expression: request.time < timestamp('2020-10-01T00:00:00.000Z') etag: BwWWja0YfJA= version: 3 For a description of IAM and its features, see the [IAM documentation](https://cloud.google.com/iam/docs/). # REQUIRED: The complete policy to be applied to the 'resource'. The size of the policy is limited to a few 10s of KB. An empty policy is in general a valid policy but certain services (like Projects) might reject them.
        "auditConfigs": [ # Specifies cloud audit logging configuration for this policy.
          { # Specifies the audit configuration for a service. The configuration determines which permission types are logged, and what identities, if any, are exempted from logging. An AuditConfig must have one or more AuditLogConfigs. If there are AuditConfigs for both `allServices` and a specific service, the union of the two AuditConfigs is used for that service: the log_types specified in each AuditConfig are enabled, and the exempted_members in each AuditLogConfig are exempted. Example Policy with multiple AuditConfigs: { "audit_configs": [ { "service": "allServices", "audit_log_configs": [ { "log_type": "DATA_READ", "exempted_members": [ "user:jose@example.com" ] }, { "log_type": "DATA_WRITE" }, { "log_type": "ADMIN_READ" } ] }, { "service": "sampleservice.googleapis.com", "audit_log_configs": [ { "log_type": "DATA_READ" }, { "log_type": "DATA_WRITE", "exempted_members": [ "user:aliya@example.com" ] } ] } ] } For sampleservice, this policy enables DATA_READ, DATA_WRITE and ADMIN_READ logging. It also exempts jose@example.com from DATA_READ logging, and aliya@example.com from DATA_WRITE logging.
            "auditLogConfigs": [ # The configuration for logging of each type of permission.
              { # Provides the configuration for logging a type of permissions. Example: { "audit_log_configs": [ { "log_type": "DATA_READ", "exempted_members": [ "user:jose@example.com" ] }, { "log_type": "DATA_WRITE" } ] } This enables 'DATA_READ' and 'DATA_WRITE' logging, while exempting jose@example.com from DATA_READ logging.
                "exemptedMembers": [ # Specifies the identities that do not cause logging for this type of permission. Follows the same format of Binding.members.
                  "A String",
                ],
                "ignoreChildExemptions": True or False, # This is deprecated and has no effect. Do not use.
                "logType": "A String", # The log type that this config enables.
              },
            ],
            "exemptedMembers": [ # This is deprecated and has no effect. Do not use.
              "A String",
            ],
            "service": "A String", # Specifies a service that will be enabled for audit logging. For example, `storage.googleapis.com`, `cloudsql.googleapis.com`. `allServices` is a special value that covers all services.
          },
        ],
        "bindings": [ # Associates a list of `members` to a `role`. Optionally, may specify a `condition` that determines how and when the `bindings` are applied. Each of the `bindings` must contain at least one member.
          { # Associates `members` with a `role`.
            "bindingId": "A String", # This is deprecated and has no effect. Do not use.
            "condition": { # Represents a textual expression in the Common Expression Language (CEL) syntax. CEL is a C-like expression language. The syntax and semantics of CEL are documented at https://github.com/google/cel-spec. Example (Comparison): title: "Summary size limit" description: "Determines if a summary is less than 100 chars" expression: "document.summary.size() < 100" Example (Equality): title: "Requestor is owner" description: "Determines if requestor is the document owner" expression: "document.owner == request.auth.claims.email" Example (Logic): title: "Public documents" description: "Determine whether the document should be publicly visible" expression: "document.type != 'private' && document.type != 'internal'" Example (Data Manipulation): title: "Notification string" description: "Create a notification string with a timestamp." expression: "'New message received at ' + string(document.create_time)" The exact variables and functions that may be referenced within an expression are determined by the service that evaluates it. See the service documentation for additional information. # The condition that is associated with this binding. If the condition evaluates to `true`, then this binding applies to the current request. If the condition evaluates to `false`, then this binding does not apply to the current request. However, a different role binding might grant the same role to one or more of the members in this binding. To learn which resources support conditions in their IAM policies, see the [IAM documentation](https://cloud.google.com/iam/help/conditions/resource-policies).
              "description": "A String", # Optional. Description of the expression. This is a longer text which describes the expression, e.g. when hovered over it in a UI.
              "expression": "A String", # Textual representation of an expression in Common Expression Language syntax.
              "location": "A String", # Optional. String indicating the location of the expression for error reporting, e.g. a file name and a position in the file.
              "title": "A String", # Optional. Title for the expression, i.e. a short string describing its purpose. This can be used e.g. in UIs which allow to enter the expression.
            },
            "members": [ # Specifies the identities requesting access for a Cloud Platform resource. `members` can have the following values: * `allUsers`: A special identifier that represents anyone who is on the internet; with or without a Google account. * `allAuthenticatedUsers`: A special identifier that represents anyone who is authenticated with a Google account or a service account. * `user:{emailid}`: An email address that represents a specific Google account. For example, `alice@example.com` . * `serviceAccount:{emailid}`: An email address that represents a service account. For example, `my-other-app@appspot.gserviceaccount.com`. * `group:{emailid}`: An email address that represents a Google group. For example, `admins@example.com`. * `deleted:user:{emailid}?uid={uniqueid}`: An email address (plus unique identifier) representing a user that has been recently deleted. For example, `alice@example.com?uid=123456789012345678901`. If the user is recovered, this value reverts to `user:{emailid}` and the recovered user retains the role in the binding. * `deleted:serviceAccount:{emailid}?uid={uniqueid}`: An email address (plus unique identifier) representing a service account that has been recently deleted. For example, `my-other-app@appspot.gserviceaccount.com?uid=123456789012345678901`. If the service account is undeleted, this value reverts to `serviceAccount:{emailid}` and the undeleted service account retains the role in the binding. * `deleted:group:{emailid}?uid={uniqueid}`: An email address (plus unique identifier) representing a Google group that has been recently deleted. For example, `admins@example.com?uid=123456789012345678901`. If the group is recovered, this value reverts to `group:{emailid}` and the recovered group retains the role in the binding. * `domain:{domain}`: The G Suite domain (primary) that represents all the users of that domain. For example, `google.com` or `example.com`.
              "A String",
            ],
            "role": "A String", # Role that is assigned to `members`. For example, `roles/viewer`, `roles/editor`, or `roles/owner`.
          },
        ],
        "etag": "A String", # `etag` is used for optimistic concurrency control as a way to help prevent simultaneous updates of a policy from overwriting each other. It is strongly suggested that systems make use of the `etag` in the read-modify-write cycle to perform policy updates in order to avoid race conditions: An `etag` is returned in the response to `getIamPolicy`, and systems are expected to put that etag in the request to `setIamPolicy` to ensure that their change will be applied to the same version of the policy. **Important:** If you use IAM Conditions, you must include the `etag` field whenever you call `setIamPolicy`. If you omit this field, then IAM allows you to overwrite a version `3` policy with a version `1` policy, and all of the conditions in the version `3` policy are lost.
        "iamOwned": True or False, # This is deprecated and has no effect. Do not use.
        "rules": [ # This is deprecated and has no effect. Do not use.
          { # This is deprecated and has no effect. Do not use.
            "action": "A String", # This is deprecated and has no effect. Do not use.
            "conditions": [ # This is deprecated and has no effect. Do not use.
              { # This is deprecated and has no effect. Do not use.
                "iam": "A String", # This is deprecated and has no effect. Do not use.
                "op": "A String", # This is deprecated and has no effect. Do not use.
                "svc": "A String", # This is deprecated and has no effect. Do not use.
                "sys": "A String", # This is deprecated and has no effect. Do not use.
                "values": [ # This is deprecated and has no effect. Do not use.
                  "A String",
                ],
              },
            ],
            "description": "A String", # This is deprecated and has no effect. Do not use.
            "ins": [ # This is deprecated and has no effect. Do not use.
              "A String",
            ],
            "logConfigs": [ # This is deprecated and has no effect. Do not use.
              { # This is deprecated and has no effect. Do not use.
                "cloudAudit": { # This is deprecated and has no effect. Do not use. # This is deprecated and has no effect. Do not use.
                  "authorizationLoggingOptions": { # This is deprecated and has no effect. Do not use. # This is deprecated and has no effect. Do not use.
                    "permissionType": "A String", # This is deprecated and has no effect. Do not use.
                  },
                  "logName": "A String", # This is deprecated and has no effect. Do not use.
                },
                "counter": { # This is deprecated and has no effect. Do not use. # This is deprecated and has no effect. Do not use.
                  "customFields": [ # This is deprecated and has no effect. Do not use.
                    { # This is deprecated and has no effect. Do not use.
                      "name": "A String", # This is deprecated and has no effect. Do not use.
                      "value": "A String", # This is deprecated and has no effect. Do not use.
                    },
                  ],
                  "field": "A String", # This is deprecated and has no effect. Do not use.
                  "metric": "A String", # This is deprecated and has no effect. Do not use.
                },
                "dataAccess": { # This is deprecated and has no effect. Do not use. # This is deprecated and has no effect. Do not use.
                  "logMode": "A String", # This is deprecated and has no effect. Do not use.
                },
              },
            ],
            "notIns": [ # This is deprecated and has no effect. Do not use.
              "A String",
            ],
            "permissions": [ # This is deprecated and has no effect. Do not use.
              "A String",
            ],
          },
        ],
        "version": 42, # Specifies the format of the policy. Valid values are `0`, `1`, and `3`. Requests that specify an invalid value are rejected. Any operation that affects conditional role bindings must specify version `3`. This requirement applies to the following operations: * Getting a policy that includes a conditional role binding * Adding a conditional role binding to a policy * Changing a conditional role binding in a policy * Removing any role binding, with or without a condition, from a policy that includes conditions **Important:** If you use IAM Conditions, you must include the `etag` field whenever you call `setIamPolicy`. If you omit this field, then IAM allows you to overwrite a version `3` policy with a version `1` policy, and all of the conditions in the version `3` policy are lost. If a policy does not include any conditions, operations on that policy may specify any valid version or leave the field unset. To learn which resources support conditions in their IAM policies, see the [IAM documentation](https://cloud.google.com/iam/help/conditions/resource-policies).
      },
    }

      x__xgafv: string, V1 error format.
        Allowed values
          1 - v1 error format
          2 - v2 error format

    Returns:
      An object of the form:

        { # An Identity and Access Management (IAM) policy, which specifies access controls for Google Cloud resources. A `Policy` is a collection of `bindings`. A `binding` binds one or more `members` to a single `role`. Members can be user accounts, service accounts, Google groups, and domains (such as G Suite). A `role` is a named list of permissions; each `role` can be an IAM predefined role or a user-created custom role. For some types of Google Cloud resources, a `binding` can also specify a `condition`, which is a logical expression that allows access to a resource only if the expression evaluates to `true`. A condition can add constraints based on attributes of the request, the resource, or both. To learn which resources support conditions in their IAM policies, see the [IAM documentation](https://cloud.google.com/iam/help/conditions/resource-policies). **JSON example:** { "bindings": [ { "role": "roles/resourcemanager.organizationAdmin", "members": [ "user:mike@example.com", "group:admins@example.com", "domain:google.com", "serviceAccount:my-project-id@appspot.gserviceaccount.com" ] }, { "role": "roles/resourcemanager.organizationViewer", "members": [ "user:eve@example.com" ], "condition": { "title": "expirable access", "description": "Does not grant access after Sep 2020", "expression": "request.time < timestamp('2020-10-01T00:00:00.000Z')", } } ], "etag": "BwWWja0YfJA=", "version": 3 } **YAML example:** bindings: - members: - user:mike@example.com - group:admins@example.com - domain:google.com - serviceAccount:my-project-id@appspot.gserviceaccount.com role: roles/resourcemanager.organizationAdmin - members: - user:eve@example.com role: roles/resourcemanager.organizationViewer condition: title: expirable access description: Does not grant access after Sep 2020 expression: request.time < timestamp('2020-10-01T00:00:00.000Z') etag: BwWWja0YfJA= version: 3 For a description of IAM and its features, see the [IAM documentation](https://cloud.google.com/iam/docs/).
      "auditConfigs": [ # Specifies cloud audit logging configuration for this policy.
        { # Specifies the audit configuration for a service. The configuration determines which permission types are logged, and what identities, if any, are exempted from logging. An AuditConfig must have one or more AuditLogConfigs. If there are AuditConfigs for both `allServices` and a specific service, the union of the two AuditConfigs is used for that service: the log_types specified in each AuditConfig are enabled, and the exempted_members in each AuditLogConfig are exempted. Example Policy with multiple AuditConfigs: { "audit_configs": [ { "service": "allServices", "audit_log_configs": [ { "log_type": "DATA_READ", "exempted_members": [ "user:jose@example.com" ] }, { "log_type": "DATA_WRITE" }, { "log_type": "ADMIN_READ" } ] }, { "service": "sampleservice.googleapis.com", "audit_log_configs": [ { "log_type": "DATA_READ" }, { "log_type": "DATA_WRITE", "exempted_members": [ "user:aliya@example.com" ] } ] } ] } For sampleservice, this policy enables DATA_READ, DATA_WRITE and ADMIN_READ logging. It also exempts jose@example.com from DATA_READ logging, and aliya@example.com from DATA_WRITE logging.
          "auditLogConfigs": [ # The configuration for logging of each type of permission.
            { # Provides the configuration for logging a type of permissions. Example: { "audit_log_configs": [ { "log_type": "DATA_READ", "exempted_members": [ "user:jose@example.com" ] }, { "log_type": "DATA_WRITE" } ] } This enables 'DATA_READ' and 'DATA_WRITE' logging, while exempting jose@example.com from DATA_READ logging.
              "exemptedMembers": [ # Specifies the identities that do not cause logging for this type of permission. Follows the same format of Binding.members.
                "A String",
              ],
              "ignoreChildExemptions": True or False, # This is deprecated and has no effect. Do not use.
              "logType": "A String", # The log type that this config enables.
            },
          ],
          "exemptedMembers": [ # This is deprecated and has no effect. Do not use.
            "A String",
          ],
          "service": "A String", # Specifies a service that will be enabled for audit logging. For example, `storage.googleapis.com`, `cloudsql.googleapis.com`. `allServices` is a special value that covers all services.
        },
      ],
      "bindings": [ # Associates a list of `members` to a `role`. Optionally, may specify a `condition` that determines how and when the `bindings` are applied. Each of the `bindings` must contain at least one member.
        { # Associates `members` with a `role`.
          "bindingId": "A String", # This is deprecated and has no effect. Do not use.
          "condition": { # Represents a textual expression in the Common Expression Language (CEL) syntax. CEL is a C-like expression language. The syntax and semantics of CEL are documented at https://github.com/google/cel-spec. Example (Comparison): title: "Summary size limit" description: "Determines if a summary is less than 100 chars" expression: "document.summary.size() < 100" Example (Equality): title: "Requestor is owner" description: "Determines if requestor is the document owner" expression: "document.owner == request.auth.claims.email" Example (Logic): title: "Public documents" description: "Determine whether the document should be publicly visible" expression: "document.type != 'private' && document.type != 'internal'" Example (Data Manipulation): title: "Notification string" description: "Create a notification string with a timestamp." expression: "'New message received at ' + string(document.create_time)" The exact variables and functions that may be referenced within an expression are determined by the service that evaluates it. See the service documentation for additional information. # The condition that is associated with this binding. If the condition evaluates to `true`, then this binding applies to the current request. If the condition evaluates to `false`, then this binding does not apply to the current request. However, a different role binding might grant the same role to one or more of the members in this binding. To learn which resources support conditions in their IAM policies, see the [IAM documentation](https://cloud.google.com/iam/help/conditions/resource-policies).
            "description": "A String", # Optional. Description of the expression. This is a longer text which describes the expression, e.g. when hovered over it in a UI.
            "expression": "A String", # Textual representation of an expression in Common Expression Language syntax.
            "location": "A String", # Optional. String indicating the location of the expression for error reporting, e.g. a file name and a position in the file.
            "title": "A String", # Optional. Title for the expression, i.e. a short string describing its purpose. This can be used e.g. in UIs which allow to enter the expression.
          },
          "members": [ # Specifies the identities requesting access for a Cloud Platform resource. `members` can have the following values: * `allUsers`: A special identifier that represents anyone who is on the internet; with or without a Google account. * `allAuthenticatedUsers`: A special identifier that represents anyone who is authenticated with a Google account or a service account. * `user:{emailid}`: An email address that represents a specific Google account. For example, `alice@example.com` . * `serviceAccount:{emailid}`: An email address that represents a service account. For example, `my-other-app@appspot.gserviceaccount.com`. * `group:{emailid}`: An email address that represents a Google group. For example, `admins@example.com`. * `deleted:user:{emailid}?uid={uniqueid}`: An email address (plus unique identifier) representing a user that has been recently deleted. For example, `alice@example.com?uid=123456789012345678901`. If the user is recovered, this value reverts to `user:{emailid}` and the recovered user retains the role in the binding. * `deleted:serviceAccount:{emailid}?uid={uniqueid}`: An email address (plus unique identifier) representing a service account that has been recently deleted. For example, `my-other-app@appspot.gserviceaccount.com?uid=123456789012345678901`. If the service account is undeleted, this value reverts to `serviceAccount:{emailid}` and the undeleted service account retains the role in the binding. * `deleted:group:{emailid}?uid={uniqueid}`: An email address (plus unique identifier) representing a Google group that has been recently deleted. For example, `admins@example.com?uid=123456789012345678901`. If the group is recovered, this value reverts to `group:{emailid}` and the recovered group retains the role in the binding. * `domain:{domain}`: The G Suite domain (primary) that represents all the users of that domain. For example, `google.com` or `example.com`.
            "A String",
          ],
          "role": "A String", # Role that is assigned to `members`. For example, `roles/viewer`, `roles/editor`, or `roles/owner`.
        },
      ],
      "etag": "A String", # `etag` is used for optimistic concurrency control as a way to help prevent simultaneous updates of a policy from overwriting each other. It is strongly suggested that systems make use of the `etag` in the read-modify-write cycle to perform policy updates in order to avoid race conditions: An `etag` is returned in the response to `getIamPolicy`, and systems are expected to put that etag in the request to `setIamPolicy` to ensure that their change will be applied to the same version of the policy. **Important:** If you use IAM Conditions, you must include the `etag` field whenever you call `setIamPolicy`. If you omit this field, then IAM allows you to overwrite a version `3` policy with a version `1` policy, and all of the conditions in the version `3` policy are lost.
      "iamOwned": True or False, # This is deprecated and has no effect. Do not use.
      "rules": [ # This is deprecated and has no effect. Do not use.
        { # This is deprecated and has no effect. Do not use.
          "action": "A String", # This is deprecated and has no effect. Do not use.
          "conditions": [ # This is deprecated and has no effect. Do not use.
            { # This is deprecated and has no effect. Do not use.
              "iam": "A String", # This is deprecated and has no effect. Do not use.
              "op": "A String", # This is deprecated and has no effect. Do not use.
              "svc": "A String", # This is deprecated and has no effect. Do not use.
              "sys": "A String", # This is deprecated and has no effect. Do not use.
              "values": [ # This is deprecated and has no effect. Do not use.
                "A String",
              ],
            },
          ],
          "description": "A String", # This is deprecated and has no effect. Do not use.
          "ins": [ # This is deprecated and has no effect. Do not use.
            "A String",
          ],
          "logConfigs": [ # This is deprecated and has no effect. Do not use.
            { # This is deprecated and has no effect. Do not use.
              "cloudAudit": { # This is deprecated and has no effect. Do not use. # This is deprecated and has no effect. Do not use.
                "authorizationLoggingOptions": { # This is deprecated and has no effect. Do not use. # This is deprecated and has no effect. Do not use.
                  "permissionType": "A String", # This is deprecated and has no effect. Do not use.
                },
                "logName": "A String", # This is deprecated and has no effect. Do not use.
              },
              "counter": { # This is deprecated and has no effect. Do not use. # This is deprecated and has no effect. Do not use.
                "customFields": [ # This is deprecated and has no effect. Do not use.
                  { # This is deprecated and has no effect. Do not use.
                    "name": "A String", # This is deprecated and has no effect. Do not use.
                    "value": "A String", # This is deprecated and has no effect. Do not use.
                  },
                ],
                "field": "A String", # This is deprecated and has no effect. Do not use.
                "metric": "A String", # This is deprecated and has no effect. Do not use.
              },
              "dataAccess": { # This is deprecated and has no effect. Do not use. # This is deprecated and has no effect. Do not use.
                "logMode": "A String", # This is deprecated and has no effect. Do not use.
              },
            },
          ],
          "notIns": [ # This is deprecated and has no effect. Do not use.
            "A String",
          ],
          "permissions": [ # This is deprecated and has no effect. Do not use.
            "A String",
          ],
        },
      ],
      "version": 42, # Specifies the format of the policy. Valid values are `0`, `1`, and `3`. Requests that specify an invalid value are rejected. Any operation that affects conditional role bindings must specify version `3`. This requirement applies to the following operations: * Getting a policy that includes a conditional role binding * Adding a conditional role binding to a policy * Changing a conditional role binding in a policy * Removing any role binding, with or without a condition, from a policy that includes conditions **Important:** If you use IAM Conditions, you must include the `etag` field whenever you call `setIamPolicy`. If you omit this field, then IAM allows you to overwrite a version `3` policy with a version `1` policy, and all of the conditions in the version `3` policy are lost. If a policy does not include any conditions, operations on that policy may specify any valid version or leave the field unset. To learn which resources support conditions in their IAM policies, see the [IAM documentation](https://cloud.google.com/iam/help/conditions/resource-policies).
    }

`setLabels(project, region, resource, body=None, requestId=None, x__xgafv=None)`

    Sets the labels on an InterconnectAttachment. To learn more about labels, read the Labeling Resources documentation.

    Args:
      project: string, Project ID for this request. (required)
      region: string, The region for this request. (required)
      resource: string, Name or id of the resource for this request. (required)
      body: object, The request body.
        The object takes the form of:

    {
      "labelFingerprint": "A String", # The fingerprint of the previous set of labels for this resource, used to detect conflicts. The fingerprint is initially generated by Compute Engine and changes after every request to modify or update labels. You must always provide an up-to-date fingerprint hash in order to update or change labels. Make a get() request to the resource to get the latest fingerprint.
      "labels": { # The labels to set for this resource.
        "a_key": "A String",
      },
    }

      requestId: string, An optional request ID to identify requests. Specify a unique request ID so that if you must retry your request, the server will know to ignore the request if it has already been completed. For example, consider a situation where you make an initial request and the request times out. If you make the request again with the same request ID, the server can check if original operation with the same request ID was received, and if so, will ignore the second request. This prevents clients from accidentally creating duplicate commitments. The request ID must be a valid UUID with the exception that zero UUID is not supported ( 00000000-0000-0000-0000-000000000000).
      x__xgafv: string, V1 error format.
        Allowed values
          1 - v1 error format
          2 - v2 error format

    Returns:
      An object of the form:

        { # Represents an Operation resource. Google Compute Engine has three Operation resources: * [Global](/compute/docs/reference/rest/alpha/globalOperations) * [Regional](/compute/docs/reference/rest/alpha/regionOperations) * [Zonal](/compute/docs/reference/rest/alpha/zoneOperations) You can use an operation resource to manage asynchronous API requests. For more information, read Handling API responses. Operations can be global, regional or zonal. - For global operations, use the `globalOperations` resource. - For regional operations, use the `regionOperations` resource. - For zonal operations, use the `zonalOperations` resource. For more information, read Global, Regional, and Zonal Resources.
      "clientOperationId": "A String", # [Output Only] The value of `requestId` if you provided it in the request. Not present otherwise.
      "creationTimestamp": "A String", # [Deprecated] This field is deprecated.
      "description": "A String", # [Output Only] A textual description of the operation, which is set when the operation is created.
      "endTime": "A String", # [Output Only] The time that this operation was completed. This value is in RFC3339 text format.
      "error": { # [Output Only] If errors are generated during processing of the operation, this field will be populated.
        "errors": [ # [Output Only] The array of errors encountered while processing this operation.
          {
            "code": "A String", # [Output Only] The error type identifier for this error.
            "location": "A String", # [Output Only] Indicates the field in the request that caused the error. This property is optional.
            "message": "A String", # [Output Only] An optional, human-readable error message.
          },
        ],
      },
      "httpErrorMessage": "A String", # [Output Only] If the operation fails, this field contains the HTTP error message that was returned, such as `NOT FOUND`.
      "httpErrorStatusCode": 42, # [Output Only] If the operation fails, this field contains the HTTP error status code that was returned. For example, a `404` means the resource was not found.
      "id": "A String", # [Output Only] The unique identifier for the operation. This identifier is defined by the server.
      "insertTime": "A String", # [Output Only] The time that this operation was requested. This value is in RFC3339 text format.
      "kind": "compute#operation", # [Output Only] Type of the resource. Always `compute#operation` for Operation resources.
      "name": "A String", # [Output Only] Name of the operation.
      "operationGroupId": "A String", # [Output Only] An ID that represents a group of operations, such as when a group of operations results from a `bulkInsert` API request.
      "operationType": "A String", # [Output Only] The type of operation, such as `insert`, `update`, or `delete`, and so on.
      "progress": 42, # [Output Only] An optional progress indicator that ranges from 0 to 100. There is no requirement that this be linear or support any granularity of operations. This should not be used to guess when the operation will be complete. This number should monotonically increase as the operation progresses.
      "region": "A String", # [Output Only] The URL of the region where the operation resides. Only applicable when performing regional operations.
      "selfLink": "A String", # [Output Only] Server-defined URL for the resource.
      "selfLinkWithId": "A String", # [Output Only] Server-defined URL for this resource with the resource id.
      "startTime": "A String", # [Output Only] The time that this operation was started by the server. This value is in RFC3339 text format.
      "status": "A String", # [Output Only] The status of the operation, which can be one of the following: `PENDING`, `RUNNING`, or `DONE`.
      "statusMessage": "A String", # [Output Only] An optional textual description of the current status of the operation.
      "targetId": "A String", # [Output Only] The unique target ID, which identifies a specific incarnation of the target resource.
      "targetLink": "A String", # [Output Only] The URL of the resource that the operation modifies. For operations related to creating a snapshot, this points to the persistent disk that the snapshot was created from.
      "user": "A String", # [Output Only] User who requested the operation, for example: `user@example.com`.
      "warnings": [ # [Output Only] If warning messages are generated during processing of the operation, this field will be populated.
        {
          "code": "A String", # [Output Only] A warning code, if applicable. For example, Compute Engine returns NO_RESULTS_ON_PAGE if there are no results in the response.
          "data": [ # [Output Only] Metadata about this warning in key: value format. For example: "data": [ { "key": "scope", "value": "zones/us-east1-d" }
            {
              "key": "A String", # [Output Only] A key that provides more detail on the warning being returned. For example, for warnings where there are no results in a list request for a particular zone, this key might be scope and the key value might be the zone name. Other examples might be a key indicating a deprecated resource and a suggested replacement, or a warning about invalid network settings (for example, if an instance attempts to perform IP forwarding but is not enabled for IP forwarding).
              "value": "A String", # [Output Only] A warning data value corresponding to the key.
            },
          ],
          "message": "A String", # [Output Only] A human-readable description of the warning code.
        },
      ],
      "zone": "A String", # [Output Only] The URL of the zone where the operation resides. Only applicable when performing per-zone operations.
    }

`testIamPermissions(project, region, resource, body=None, x__xgafv=None)`

    Returns permissions that a caller has on the specified resource.

    Args:
      project: string, Project ID for this request. (required)
      region: string, The name of the region for this request. (required)
      resource: string, Name or id of the resource for this request. (required)
      body: object, The request body.
        The object takes the form of:

    {
      "permissions": [ # The set of permissions to check for the 'resource'. Permissions with wildcards (such as '*' or 'storage.*') are not allowed.
        "A String",
      ],
    }

      x__xgafv: string, V1 error format.
        Allowed values
          1 - v1 error format
          2 - v2 error format

    Returns:
      An object of the form:

        {
      "permissions": [ # A subset of `TestPermissionsRequest.permissions` that the caller is allowed.
        "A String",
      ],
    }