Calibration Flash v5
====================

This example shows how to flash calibration data of version 5 (gen1 calibration data) to the device.

.. rubric:: Similar samples:

- :ref:`Calibration Flash`
- :ref:`Calibration Reader`
- :ref:`Calibration Load`

Setup
#####

.. include::  /includes/install_from_pypi.rst

Source code
###########

.. tabs::

    .. tab:: Python

        Also `available on GitHub <https://github.com/luxonis/depthai-python/blob/main/examples/calibration/calibration_flash_v5.py>`__

        .. literalinclude:: ../../../../examples/calibration/calibration_flash_v5.py
           :language: python
           :linenos:

    .. tab:: C++

        Also `available on GitHub <https://github.com/luxonis/depthai-core/blob/main/examples/calibration/calibration_flash_v5.cpp>`__

        .. literalinclude:: ../../../../depthai-core/examples/calibration/calibration_flash_v5.cpp
           :language: cpp
           :linenos:

.. include::  /includes/footer-short.rst
