# Compute Engine API . regionInstanceTemplates

## Instance Methods

Close httplib2 connections.

Deletes the specified instance template. Deleting an instance template is permanent and cannot be undone.

Returns the specified instance template. Gets a list of available instance templates by making a list() request.

Creates an instance template in the specified project and region using the global instance template whose URL is included in the request.

Retrieves a list of instance templates that are contained within the specified project and region.

Retrieves the next page of results.

### Method Details

`close()`

    Close httplib2 connections.

`delete(project, region, instanceTemplate, requestId=None, x__xgafv=None)`

    Deletes the specified instance template. Deleting an instance template is permanent and cannot be undone.

    Args:
      project: string, Project ID for this request. (required)
      region: string, The name of the region for this request. (required)
      instanceTemplate: string, The name of the instance template to delete. (required)
      requestId: string, An optional request ID to identify requests. Specify a unique request ID so that if you must retry your request, the server will know to ignore the request if it has already been completed. For example, consider a situation where you make an initial request and the request times out. If you make the request again with the same request ID, the server can check if original operation with the same request ID was received, and if so, will ignore the second request. This prevents clients from accidentally creating duplicate commitments. The request ID must be a valid UUID with the exception that zero UUID is not supported ( 00000000-0000-0000-0000-000000000000).
      x__xgafv: string, V1 error format.
        Allowed values
          1 - v1 error format
          2 - v2 error format

    Returns:
      An object of the form:

        { # Represents an Operation resource. Google Compute Engine has three Operation resources: * [Global](/compute/docs/reference/rest/alpha/globalOperations) * [Regional](/compute/docs/reference/rest/alpha/regionOperations) * [Zonal](/compute/docs/reference/rest/alpha/zoneOperations) You can use an operation resource to manage asynchronous API requests. For more information, read Handling API responses. Operations can be global, regional or zonal. - For global operations, use the `globalOperations` resource. - For regional operations, use the `regionOperations` resource. - For zonal operations, use the `zonalOperations` resource. For more information, read Global, Regional, and Zonal Resources.
      "clientOperationId": "A String", # [Output Only] The value of `requestId` if you provided it in the request. Not present otherwise.
      "creationTimestamp": "A String", # [Deprecated] This field is deprecated.
      "description": "A String", # [Output Only] A textual description of the operation, which is set when the operation is created.
      "endTime": "A String", # [Output Only] The time that this operation was completed. This value is in RFC3339 text format.
      "error": { # [Output Only] If errors are generated during processing of the operation, this field will be populated.
        "errors": [ # [Output Only] The array of errors encountered while processing this operation.
          {
            "code": "A String", # [Output Only] The error type identifier for this error.
            "errorDetails": [ # [Output Only] An optional list of messages that contain the error details. There is a set of defined message types to use for providing details.The syntax depends on the error code. For example, QuotaExceededInfo will have details when the error code is QUOTA_EXCEEDED.
              {
                "errorInfo": { # Describes the cause of the error with structured details. Example of an error when contacting the "pubsub.googleapis.com" API when it is not enabled: { "reason": "API_DISABLED" "domain": "googleapis.com" "metadata": { "resource": "projects/123", "service": "pubsub.googleapis.com" } } This response indicates that the pubsub.googleapis.com API is not enabled. Example of an error that is returned when attempting to create a Spanner instance in a region that is out of stock: { "reason": "STOCKOUT" "domain": "spanner.googleapis.com", "metadata": { "availableRegions": "us-central1,us-east2" } }
                  "domain": "A String", # The logical grouping to which the "reason" belongs. The error domain is typically the registered service name of the tool or product that generates the error. Example: "pubsub.googleapis.com". If the error is generated by some common infrastructure, the error domain must be a globally unique value that identifies the infrastructure. For Google API infrastructure, the error domain is "googleapis.com".
                  "metadatas": { # Additional structured details about this error. Keys should match /[a-zA-Z0-9-_]/ and be limited to 64 characters in length. When identifying the current value of an exceeded limit, the units should be contained in the key, not the value. For example, rather than {"instanceLimit": "100/request"}, should be returned as, {"instanceLimitPerRequest": "100"}, if the client exceeds the number of instances that can be created in a single (batch) request.
                    "a_key": "A String",
                  },
                  "reason": "A String", # The reason of the error. This is a constant value that identifies the proximate cause of the error. Error reasons are unique within a particular domain of errors. This should be at most 63 characters and match /[A-Z0-9_]+/.
                },
                "help": { # Provides links to documentation or for performing an out of band action. For example, if a quota check failed with an error indicating the calling project hasn't enabled the accessed service, this can contain a URL pointing directly to the right place in the developer console to flip the bit.
                  "links": [ # URL(s) pointing to additional information on handling the current error.
                    { # Describes a URL link.
                      "description": "A String", # Describes what the link offers.
                      "url": "A String", # The URL of the link.
                    },
                  ],
                },
                "localizedMessage": { # Provides a localized error message that is safe to return to the user which can be attached to an RPC error.
                  "locale": "A String", # The locale used following the specification defined at http://www.rfc-editor.org/rfc/bcp/bcp47.txt. Examples are: "en-US", "fr-CH", "es-MX"
                  "message": "A String", # The localized error message in the above locale.
                },
                "quotaInfo": { # Additional details for quota exceeded error for resource quota.
                  "dimensions": { # The map holding related quota dimensions.
                    "a_key": "A String",
                  },
                  "limit": 3.14, # Current effective quota limit. The limit's unit depends on the quota type or metric.
                  "limitName": "A String", # The name of the quota limit.
                  "metricName": "A String", # The Compute Engine quota metric name.
                },
              },
            ],
            "location": "A String", # [Output Only] Indicates the field in the request that caused the error. This property is optional.
            "message": "A String", # [Output Only] An optional, human-readable error message.
          },
        ],
      },
      "httpErrorMessage": "A String", # [Output Only] If the operation fails, this field contains the HTTP error message that was returned, such as `NOT FOUND`.
      "httpErrorStatusCode": 42, # [Output Only] If the operation fails, this field contains the HTTP error status code that was returned. For example, a `404` means the resource was not found.
      "id": "A String", # [Output Only] The unique identifier for the operation. This identifier is defined by the server.
      "insertTime": "A String", # [Output Only] The time that this operation was requested. This value is in RFC3339 text format.
      "kind": "compute#operation", # [Output Only] Type of the resource. Always `compute#operation` for Operation resources.
      "metadata": { # [Output Only] Service-specific metadata attached to this operation.
        "a_key": "", # Properties of the object. Contains field @type with type URL.
      },
      "name": "A String", # [Output Only] Name of the operation.
      "operationGroupId": "A String", # [Output Only] An ID that represents a group of operations, such as when a group of operations results from a `bulkInsert` API request.
      "operationType": "A String", # [Output Only] The type of operation, such as `insert`, `update`, or `delete`, and so on.
      "progress": 42, # [Output Only] An optional progress indicator that ranges from 0 to 100. There is no requirement that this be linear or support any granularity of operations. This should not be used to guess when the operation will be complete. This number should monotonically increase as the operation progresses.
      "region": "A String", # [Output Only] The URL of the region where the operation resides. Only applicable when performing regional operations.
      "selfLink": "A String", # [Output Only] Server-defined URL for the resource.
      "selfLinkWithId": "A String", # [Output Only] Server-defined URL for this resource with the resource id.
      "startTime": "A String", # [Output Only] The time that this operation was started by the server. This value is in RFC3339 text format.
      "status": "A String", # [Output Only] The status of the operation, which can be one of the following: `PENDING`, `RUNNING`, or `DONE`.
      "statusMessage": "A String", # [Output Only] An optional textual description of the current status of the operation.
      "targetId": "A String", # [Output Only] The unique target ID, which identifies a specific incarnation of the target resource.
      "targetLink": "A String", # [Output Only] The URL of the resource that the operation modifies. For operations related to creating a snapshot, this points to the persistent disk that the snapshot was created from.
      "user": "A String", # [Output Only] User who requested the operation, for example: `user@example.com`.
      "warnings": [ # [Output Only] If warning messages are generated during processing of the operation, this field will be populated.
        {
          "code": "A String", # [Output Only] A warning code, if applicable. For example, Compute Engine returns NO_RESULTS_ON_PAGE if there are no results in the response.
          "data": [ # [Output Only] Metadata about this warning in key: value format. For example: "data": [ { "key": "scope", "value": "zones/us-east1-d" }
            {
              "key": "A String", # [Output Only] A key that provides more detail on the warning being returned. For example, for warnings where there are no results in a list request for a particular zone, this key might be scope and the key value might be the zone name. Other examples might be a key indicating a deprecated resource and a suggested replacement, or a warning about invalid network settings (for example, if an instance attempts to perform IP forwarding but is not enabled for IP forwarding).
              "value": "A String", # [Output Only] A warning data value corresponding to the key.
            },
          ],
          "message": "A String", # [Output Only] A human-readable description of the warning code.
        },
      ],
      "zone": "A String", # [Output Only] The URL of the zone where the operation resides. Only applicable when performing per-zone operations.
    }

`get(project, region, instanceTemplate, x__xgafv=None)`

    Returns the specified instance template. Gets a list of available instance templates by making a list() request.

    Args:
      project: string, Project ID for this request. (required)
      region: string, The name of the region for this request. (required)
      instanceTemplate: string, The name of the instance template. (required)
      x__xgafv: string, V1 error format.
        Allowed values
          1 - v1 error format
          2 - v2 error format

    Returns:
      An object of the form:

        { # Represents an Instance Template resource. You can use instance templates to create VM instances and managed instance groups. For more information, read Instance Templates.
      "creationTimestamp": "A String", # [Output Only] The creation timestamp for this instance template in RFC3339 text format.
      "description": "A String", # An optional description of this resource. Provide this property when you create the resource.
      "id": "A String", # [Output Only] A unique identifier for this instance template. The server defines this identifier.
      "kind": "compute#instanceTemplate", # [Output Only] The resource type, which is always compute#instanceTemplate for instance templates.
      "name": "A String", # Name of the resource; provided by the client when the resource is created. The name must be 1-63 characters long, and comply with RFC1035. Specifically, the name must be 1-63 characters long and match the regular expression `[a-z]([-a-z0-9]*[a-z0-9])?` which means the first character must be a lowercase letter, and all following characters must be a dash, lowercase letter, or digit, except the last character, which cannot be a dash.
      "properties": { # The instance properties for this instance template.
        "advancedMachineFeatures": { # Specifies options for controlling advanced machine features. Options that would traditionally be configured in a BIOS belong here. Features that require operating system support may have corresponding entries in the GuestOsFeatures of an Image (e.g., whether or not the OS in the Image supports nested virtualization being enabled or disabled). # Controls for advanced machine-related behavior features. Note that for MachineImage, this is not supported yet.
          "enableNestedVirtualization": True or False, # Whether to enable nested virtualization or not (default is false).
          "enableUefiNetworking": True or False, # Whether to enable UEFI networking for instance creation.
          "numaNodeCount": 42, # The number of vNUMA nodes.
          "threadsPerCore": 42, # The number of threads per physical core. To disable simultaneous multithreading (SMT) set this to 1. If unset, the maximum number of threads supported per core by the underlying processor is assumed.
          "visibleCoreCount": 42, # The number of physical cores to expose to an instance. Multiply by the number of threads per core to compute the total number of virtual CPUs to expose to the instance. If unset, the number of cores is inferred from the instance's nominal CPU count and the underlying platform's SMT width.
        },
        "canIpForward": True or False, # Enables instances created based on these properties to send packets with source IP addresses other than their own and receive packets with destination IP addresses other than their own. If these instances will be used as an IP gateway or it will be set as the next-hop in a Route resource, specify true. If unsure, leave this set to false. See the Enable IP forwarding documentation for more information.
        "confidentialInstanceConfig": { # A set of Confidential Instance options. # Specifies the Confidential Instance options. Note that for MachineImage, this is not supported yet.
          "confidentialInstanceType": "A String", # Defines the type of technology used by the confidential instance.
          "enableConfidentialCompute": True or False, # Defines whether the instance should have confidential compute enabled.
        },
        "description": "A String", # An optional text description for the instances that are created from these properties.
        "disks": [ # An array of disks that are associated with the instances that are created from these properties.
          { # An instance-attached disk resource.
            "architecture": "A String", # [Output Only] The architecture of the attached disk. Valid values are ARM64 or X86_64.
            "autoDelete": True or False, # Specifies whether the disk will be auto-deleted when the instance is deleted (but not when the disk is detached from the instance).
            "boot": True or False, # Indicates that this is a boot disk. The virtual machine will use the first partition of the disk for its root filesystem.
            "deviceName": "A String", # Specifies a unique device name of your choice that is reflected into the /dev/disk/by-id/google-* tree of a Linux operating system running within the instance. This name can be used to reference the device for mounting, resizing, and so on, from within the instance. If not specified, the server chooses a default device name to apply to this disk, in the form persistent-disk-x, where x is a number assigned by Google Compute Engine. This field is only applicable for persistent disks.
            "diskEncryptionKey": { # Encrypts or decrypts a disk using a customer-supplied encryption key. If you are creating a new disk, this field encrypts the new disk using an encryption key that you provide. If you are attaching an existing disk that is already encrypted, this field decrypts the disk using the customer-supplied encryption key. If you encrypt a disk using a customer-supplied key, you must provide the same key again when you attempt to use this resource at a later time. For example, you must provide the key when you create a snapshot or an image from the disk or when you attach the disk to a virtual machine instance. If you do not provide an encryption key, then the disk will be encrypted using an automatically generated key and you do not need to provide a key to use the disk later. Instance templates do not store customer-supplied encryption keys, so you cannot use your own keys to encrypt disks in a managed instance group.
              "kmsKeyName": "A String", # The name of the encryption key that is stored in Google Cloud KMS. For example: "kmsKeyName": "projects/kms_project_id/locations/region/keyRings/ key_region/cryptoKeys/key
              "kmsKeyServiceAccount": "A String", # The service account being used for the encryption request for the given KMS key. If absent, the Compute Engine default service account is used. For example: "kmsKeyServiceAccount": "name@project_id.iam.gserviceaccount.com/
              "rawKey": "A String", # Specifies a 256-bit customer-supplied encryption key, encoded in RFC 4648 base64 to either encrypt or decrypt this resource. You can provide either the rawKey or the rsaEncryptedKey. For example: "rawKey": "SGVsbG8gZnJvbSBHb29nbGUgQ2xvdWQgUGxhdGZvcm0="
              "rsaEncryptedKey": "A String", # Specifies an RFC 4648 base64 encoded, RSA-wrapped 2048-bit customer-supplied encryption key to either encrypt or decrypt this resource. You can provide either the rawKey or the rsaEncryptedKey. For example: "rsaEncryptedKey": "ieCx/NcW06PcT7Ep1X6LUTc/hLvUDYyzSZPPVCVPTVEohpeHASqC8uw5TzyO9U+Fka9JFH z0mBibXUInrC/jEk014kCK/NPjYgEMOyssZ4ZINPKxlUh2zn1bV+MCaTICrdmuSBTWlUUiFoD D6PYznLwh8ZNdaheCeZ8ewEXgFQ8V+sDroLaN3Xs3MDTXQEMMoNUXMCZEIpg9Vtp9x2oe==" The key must meet the following requirements before you can provide it to Compute Engine: 1. The key is wrapped using a RSA public key certificate provided by Google. 2. After being wrapped, the key must be encoded in RFC 4648 base64 encoding. Gets the RSA public key certificate provided by Google at: https://cloud-certs.storage.googleapis.com/google-cloud-csek-ingress.pem
              "sha256": "A String", # [Output only] The RFC 4648 base64 encoded SHA-256 hash of the customer-supplied encryption key that protects this resource.
            },
            "diskSizeGb": "A String", # The size of the disk in GB.
            "forceAttach": True or False, # [Input Only] Whether to force attach the regional disk even if it's currently attached to another instance. If you try to force attach a zonal disk to an instance, you will receive an error.
            "guestOsFeatures": [ # A list of features to enable on the guest operating system. Applicable only for bootable images. Read Enabling guest operating system features to see a list of available options.
              { # Guest OS features.
                "type": "A String", # The ID of a supported feature. To add multiple values, use commas to separate values. Set to one or more of the following values: - VIRTIO_SCSI_MULTIQUEUE - WINDOWS - MULTI_IP_SUBNET - UEFI_COMPATIBLE - GVNIC - SEV_CAPABLE - SUSPEND_RESUME_COMPATIBLE - SEV_SNP_CAPABLE For more information, see Enabling guest operating system features.
              },
            ],
            "index": 42, # [Output Only] A zero-based index to this disk, where 0 is reserved for the boot disk. If you have many disks attached to an instance, each disk would have a unique index number.
            "initializeParams": { # [Input Only] Specifies the parameters for a new disk that will be created alongside the new instance. Use initialization parameters to create boot disks or local SSDs attached to the new instance. This field is persisted and returned for instanceTemplate and not returned in the context of instance. This property is mutually exclusive with the source property; you can only define one or the other, but not both. # [Input Only] Specifies the parameters for a new disk that will be created alongside the new instance. Use initialization parameters to create boot disks or local SSDs attached to the new instance. This property is mutually exclusive with the source property; you can only define one or the other, but not both.
              "architecture": "A String", # The architecture of the attached disk. Valid values are arm64 or x86_64.
              "description": "A String", # An optional description. Provide this property when creating the disk.
              "diskName": "A String", # Specifies the disk name. If not specified, the default is to use the name of the instance. If a disk with the same name already exists in the given region, the existing disk is attached to the new instance and the new disk is not created.
              "diskSizeGb": "A String", # Specifies the size of the disk in base-2 GB. The size must be at least 10 GB. If you specify a sourceImage, which is required for boot disks, the default size is the size of the sourceImage. If you do not specify a sourceImage, the default disk size is 500 GB.
              "diskType": "A String", # Specifies the disk type to use to create the instance. If not specified, the default is pd-standard, specified using the full URL. For example: https://www.googleapis.com/compute/v1/projects/project/zones/zone /diskTypes/pd-standard For a full list of acceptable values, see Persistent disk types. If you define this field, you can provide either the full or partial URL. For example, the following are valid values: - https://www.googleapis.com/compute/v1/projects/project/zones/zone /diskTypes/diskType - projects/project/zones/zone/diskTypes/diskType - zones/zone/diskTypes/diskType Note that for InstanceTemplate, this is the name of the disk type, not URL.
              "guestOsFeatures": [ # A list of features to enable on the guest operating system. Applicable only for bootable images. Read Enabling guest operating system features to see a list of available options. Guest OS features are applied by merging initializeParams.guestOsFeatures and disks.guestOsFeatures
                { # Guest OS features.
                  "type": "A String", # The ID of a supported feature. To add multiple values, use commas to separate values. Set to one or more of the following values: - VIRTIO_SCSI_MULTIQUEUE - WINDOWS - MULTI_IP_SUBNET - UEFI_COMPATIBLE - GVNIC - SEV_CAPABLE - SUSPEND_RESUME_COMPATIBLE - SEV_SNP_CAPABLE For more information, see Enabling guest operating system features.
                },
              ],
              "interface": "A String", # [Deprecated] Specifies the disk interface to use for attaching this disk, which is either SCSI or NVME. The default is SCSI.
              "labels": { # Labels to apply to this disk. These can be later modified by the disks.setLabels method. This field is only applicable for persistent disks.
                "a_key": "A String",
              },
              "licenseCodes": [ # Integer license codes indicating which licenses are attached to this disk.
                "A String",
              ],
              "licenses": [ # A list of publicly visible licenses. Reserved for Google's use.
                "A String",
              ],
              "multiWriter": True or False, # Indicates whether or not the disk can be read/write attached to more than one instance.
              "onUpdateAction": "A String", # Specifies which action to take on instance update with this disk. Default is to use the existing disk.
              "provisionedIops": "A String", # Indicates how many IOPS to provision for the disk. This sets the number of I/O operations per second that the disk can handle. Values must be between 10,000 and 120,000. For more details, see the Extreme persistent disk documentation.
              "replicaZones": [ # URLs of the zones where the disk should be replicated to. Only applicable for regional resources.
                "A String",
              ],
              "resourcePolicies": [ # Resource policies applied to this disk for automatic snapshot creations. Specified using the full or partial URL. For instance template, specify only the resource policy name.
                "A String",
              ],
              "sourceImage": "A String", # The source image to create this disk. When creating a new instance, one of initializeParams.sourceImage or initializeParams.sourceSnapshot or disks.source is required except for local SSD. To create a disk with one of the public operating system images, specify the image by its family name. For example, specify family/debian-9 to use the latest Debian 9 image: projects/debian-cloud/global/images/family/debian-9 Alternatively, use a specific version of a public operating system image: projects/debian-cloud/global/images/debian-9-stretch-vYYYYMMDD To create a disk with a custom image that you created, specify the image name in the following format: global/images/my-custom-image You can also specify a custom image by its image family, which returns the latest version of the image in that family. Replace the image name with family/family-name: global/images/family/my-image-family If the source image is deleted later, this field will not be set.
              "sourceImageEncryptionKey": { # The customer-supplied encryption key of the source image. Required if the source image is protected by a customer-supplied encryption key. Instance templates do not store customer-supplied encryption keys, so you cannot create disks for instances in a managed instance group if the source images are encrypted with your own keys.
                "kmsKeyName": "A String", # The name of the encryption key that is stored in Google Cloud KMS. For example: "kmsKeyName": "projects/kms_project_id/locations/region/keyRings/ key_region/cryptoKeys/key
                "kmsKeyServiceAccount": "A String", # The service account being used for the encryption request for the given KMS key. If absent, the Compute Engine default service account is used. For example: "kmsKeyServiceAccount": "name@project_id.iam.gserviceaccount.com/
                "rawKey": "A String", # Specifies a 256-bit customer-supplied encryption key, encoded in RFC 4648 base64 to either encrypt or decrypt this resource. You can provide either the rawKey or the rsaEncryptedKey. For example: "rawKey": "SGVsbG8gZnJvbSBHb29nbGUgQ2xvdWQgUGxhdGZvcm0="
                "rsaEncryptedKey": "A String", # Specifies an RFC 4648 base64 encoded, RSA-wrapped 2048-bit customer-supplied encryption key to either encrypt or decrypt this resource. You can provide either the rawKey or the rsaEncryptedKey. For example: "rsaEncryptedKey": "ieCx/NcW06PcT7Ep1X6LUTc/hLvUDYyzSZPPVCVPTVEohpeHASqC8uw5TzyO9U+Fka9JFH z0mBibXUInrC/jEk014kCK/NPjYgEMOyssZ4ZINPKxlUh2zn1bV+MCaTICrdmuSBTWlUUiFoD D6PYznLwh8ZNdaheCeZ8ewEXgFQ8V+sDroLaN3Xs3MDTXQEMMoNUXMCZEIpg9Vtp9x2oe==" The key must meet the following requirements before you can provide it to Compute Engine: 1. The key is wrapped using a RSA public key certificate provided by Google. 2. After being wrapped, the key must be encoded in RFC 4648 base64 encoding. Gets the RSA public key certificate provided by Google at: https://cloud-certs.storage.googleapis.com/google-cloud-csek-ingress.pem
                "sha256": "A String", # [Output only] The RFC 4648 base64 encoded SHA-256 hash of the customer-supplied encryption key that protects this resource.
              },
              "sourceInstantSnapshot": "A String", # The source instant-snapshot to create this disk. When creating a new instance, one of initializeParams.sourceSnapshot or initializeParams.sourceInstantSnapshot initializeParams.sourceImage or disks.source is required except for local SSD. To create a disk with a snapshot that you created, specify the snapshot name in the following format: us-central1-a/instantSnapshots/my-backup If the source instant-snapshot is deleted later, this field will not be set.
              "sourceSnapshot": "A String", # The source snapshot to create this disk. When creating a new instance, one of initializeParams.sourceSnapshot or initializeParams.sourceImage or disks.source is required except for local SSD. To create a disk with a snapshot that you created, specify the snapshot name in the following format: global/snapshots/my-backup If the source snapshot is deleted later, this field will not be set.
              "sourceSnapshotEncryptionKey": { # The customer-supplied encryption key of the source snapshot.
                "kmsKeyName": "A String", # The name of the encryption key that is stored in Google Cloud KMS. For example: "kmsKeyName": "projects/kms_project_id/locations/region/keyRings/ key_region/cryptoKeys/key
                "kmsKeyServiceAccount": "A String", # The service account being used for the encryption request for the given KMS key. If absent, the Compute Engine default service account is used. For example: "kmsKeyServiceAccount": "name@project_id.iam.gserviceaccount.com/
                "rawKey": "A String", # Specifies a 256-bit customer-supplied encryption key, encoded in RFC 4648 base64 to either encrypt or decrypt this resource. You can provide either the rawKey or the rsaEncryptedKey. For example: "rawKey": "SGVsbG8gZnJvbSBHb29nbGUgQ2xvdWQgUGxhdGZvcm0="
                "rsaEncryptedKey": "A String", # Specifies an RFC 4648 base64 encoded, RSA-wrapped 2048-bit customer-supplied encryption key to either encrypt or decrypt this resource. You can provide either the rawKey or the rsaEncryptedKey. For example: "rsaEncryptedKey": "ieCx/NcW06PcT7Ep1X6LUTc/hLvUDYyzSZPPVCVPTVEohpeHASqC8uw5TzyO9U+Fka9JFH z0mBibXUInrC/jEk014kCK/NPjYgEMOyssZ4ZINPKxlUh2zn1bV+MCaTICrdmuSBTWlUUiFoD D6PYznLwh8ZNdaheCeZ8ewEXgFQ8V+sDroLaN3Xs3MDTXQEMMoNUXMCZEIpg9Vtp9x2oe==" The key must meet the following requirements before you can provide it to Compute Engine: 1. The key is wrapped using a RSA public key certificate provided by Google. 2. After being wrapped, the key must be encoded in RFC 4648 base64 encoding. Gets the RSA public key certificate provided by Google at: https://cloud-certs.storage.googleapis.com/google-cloud-csek-ingress.pem
                "sha256": "A String", # [Output only] The RFC 4648 base64 encoded SHA-256 hash of the customer-supplied encryption key that protects this resource.
              },
            },
            "interface": "A String", # Specifies the disk interface to use for attaching this disk, which is either SCSI or NVME. The default is SCSI. Persistent disks must always use SCSI and the request will fail if you attempt to attach a persistent disk in any other format than SCSI. Local SSDs can use either NVME or SCSI. For performance characteristics of SCSI over NVMe, see Local SSD performance.
            "kind": "compute#attachedDisk", # [Output Only] Type of the resource. Always compute#attachedDisk for attached disks.
            "licenses": [ # [Output Only] Any valid publicly visible licenses.
              "A String",
            ],
            "locked": True or False, # [Output Only] Whether to indicate the attached disk is locked. The locked disk is not allowed to be detached from the instance, or to be used as the source of the snapshot creation, and the image creation. The instance with at least one locked attached disk is not allow to be used as source of machine image creation, instant snapshot creation, and not allowed to be deleted with --keep-disk parameter set to true for locked disks.
            "mode": "A String", # The mode in which to attach this disk, either READ_WRITE or READ_ONLY. If not specified, the default is to attach the disk in READ_WRITE mode.
            "savedState": "A String", # For LocalSSD disks on VM Instances in STOPPED or SUSPENDED state, this field is set to PRESERVED if the LocalSSD data has been saved to a persistent location by customer request. (see the discard_local_ssd option on Stop/Suspend). Read-only in the api.
            "shieldedInstanceInitialState": { # Initial State for shielded instance, these are public keys which are safe to store in public # [Output Only] shielded vm initial state stored on disk
              "dbs": [ # The Key Database (db).
                {
                  "content": "A String", # The raw content in the secure keys file.
                  "fileType": "A String", # The file type of source file.
                },
              ],
              "dbxs": [ # The forbidden key database (dbx).
                {
                  "content": "A String", # The raw content in the secure keys file.
                  "fileType": "A String", # The file type of source file.
                },
              ],
              "keks": [ # The Key Exchange Key (KEK).
                {
                  "content": "A String", # The raw content in the secure keys file.
                  "fileType": "A String", # The file type of source file.
                },
              ],
              "pk": { # The Platform Key (PK).
                "content": "A String", # The raw content in the secure keys file.
                "fileType": "A String", # The file type of source file.
              },
            },
            "source": "A String", # Specifies a valid partial or full URL to an existing Persistent Disk resource. When creating a new instance, one of initializeParams.sourceImage or initializeParams.sourceSnapshot or disks.source is required except for local SSD. If desired, you can also attach existing non-root persistent disks using this property. This field is only applicable for persistent disks. Note that for InstanceTemplate, specify the disk name for zonal disk, and the URL for regional disk.
            "type": "A String", # Specifies the type of the disk, either SCRATCH or PERSISTENT. If not specified, the default is PERSISTENT.
            "userLicenses": [ # [Output Only] A list of user provided licenses. It represents a list of URLs to the license resource. Unlike regular licenses, user provided licenses can be modified after the disk is created.
              "A String",
            ],
          },
        ],
        "displayDevice": { # A set of Display Device options # Display Device properties to enable support for remote display products like: Teradici, VNC and TeamViewer Note that for MachineImage, this is not supported yet.
          "enableDisplay": True or False, # Defines whether the instance has Display enabled.
        },
        "guestAccelerators": [ # A list of guest accelerator cards' type and count to use for instances created from these properties.
          { # A specification of the type and number of accelerator cards attached to the instance.
            "acceleratorCount": 42, # The number of the guest accelerator cards exposed to this instance.
            "acceleratorType": "A String", # Full or partial URL of the accelerator type resource to attach to this instance. For example: projects/my-project/zones/us-central1-c/acceleratorTypes/nvidia-tesla-p100 If you are creating an instance template, specify only the accelerator name. See GPUs on Compute Engine for a full list of accelerator types.
          },
        ],
        "keyRevocationActionType": "A String", # KeyRevocationActionType of the instance. Supported options are "STOP" and "NONE". The default value is "NONE" if it is not specified.
        "labels": { # Labels to apply to instances that are created from these properties.
          "a_key": "A String",
        },
        "machineType": "A String", # The machine type to use for instances that are created from these properties.
        "metadata": { # A metadata key/value entry. # The metadata key/value pairs to assign to instances that are created from these properties. These pairs can consist of custom metadata or predefined keys. See Project and instance metadata for more information.
          "fingerprint": "A String", # Specifies a fingerprint for this request, which is essentially a hash of the metadata's contents and used for optimistic locking. The fingerprint is initially generated by Compute Engine and changes after every request to modify or update metadata. You must always provide an up-to-date fingerprint hash in order to update or change metadata, otherwise the request will fail with error 412 conditionNotMet. To see the latest fingerprint, make a get() request to retrieve the resource.
          "items": [ # Array of key/value pairs. The total size of all keys and values must be less than 512 KB.
            { # Metadata
              "key": "A String", # Key for the metadata entry. Keys must conform to the following regexp: [a-zA-Z0-9-_]+, and be less than 128 bytes in length. This is reflected as part of a URL in the metadata server. Additionally, to avoid ambiguity, keys must not conflict with any other metadata keys for the project.
              "value": "A String", # Value for the metadata entry. These are free-form strings, and only have meaning as interpreted by the image running in the instance. The only restriction placed on values is that their size must be less than or equal to 262144 bytes (256 KiB).
            },
          ],
          "kind": "compute#metadata", # [Output Only] Type of the resource. Always compute#metadata for metadata.
        },
        "minCpuPlatform": "A String", # Minimum cpu/platform to be used by instances. The instance may be scheduled on the specified or newer cpu/platform. Applicable values are the friendly names of CPU platforms, such as minCpuPlatform: "Intel Haswell" or minCpuPlatform: "Intel Sandy Bridge". For more information, read Specifying a Minimum CPU Platform.
        "networkInterfaces": [ # An array of network access configurations for this interface.
          { # A network interface resource attached to an instance.
            "accessConfigs": [ # An array of configurations for this interface. Currently, only one access config, ONE_TO_ONE_NAT, is supported. If there are no accessConfigs specified, then this instance will have no external internet access.
              { # An access configuration attached to an instance's network interface. Only one access config per instance is supported.
                "externalIpv6": "A String", # The first IPv6 address of the external IPv6 range associated with this instance, prefix length is stored in externalIpv6PrefixLength in ipv6AccessConfig. The field is output only, an IPv6 address from a subnetwork associated with the instance will be allocated dynamically.
                "externalIpv6PrefixLength": 42, # The prefix length of the external IPv6 range.
                "kind": "compute#accessConfig", # [Output Only] Type of the resource. Always compute#accessConfig for access configs.
                "name": "A String", # The name of this access configuration. The default and recommended name is External NAT, but you can use any arbitrary string, such as My external IP or Network Access.
                "natIP": "A String", # An external IP address associated with this instance. Specify an unused static external IP address available to the project or leave this field undefined to use an IP from a shared ephemeral IP address pool. If you specify a static external IP address, it must live in the same region as the zone of the instance.
                "networkTier": "A String", # This signifies the networking tier used for configuring this access configuration and can only take the following values: PREMIUM, STANDARD. If an AccessConfig is specified without a valid external IP address, an ephemeral IP will be created with this networkTier. If an AccessConfig with a valid external IP address is specified, it must match that of the networkTier associated with the Address resource owning that IP.
                "publicDnsName": "A String", # [Output Only] The public DNS domain name for the instance.
                "publicPtrDomainName": "A String", # The DNS domain name for the public PTR record. You can set this field only if the `setPublicPtr` field is enabled in accessConfig. If this field is unspecified in ipv6AccessConfig, a default PTR record will be createc for first IP in associated external IPv6 range.
                "setPublicDns": True or False, # Specifies whether a public DNS 'A' record should be created for the external IP address of this access configuration.
                "setPublicPtr": True or False, # Specifies whether a public DNS 'PTR' record should be created to map the external IP address of the instance to a DNS domain name. This field is not used in ipv6AccessConfig. A default PTR record will be created if the VM has external IPv6 range associated.
                "type": "ONE_TO_ONE_NAT", # The type of configuration. The default and only option is ONE_TO_ONE_NAT.
              },
            ],
            "aliasIpRanges": [ # An array of alias IP ranges for this network interface. You can only specify this field for network interfaces in VPC networks.
              { # An alias IP range attached to an instance's network interface.
                "ipCidrRange": "A String", # The IP alias ranges to allocate for this interface. This IP CIDR range must belong to the specified subnetwork and cannot contain IP addresses reserved by system or used by other network interfaces. This range may be a single IP address (such as 10.2.3.4), a netmask (such as /24) or a CIDR-formatted string (such as 10.1.2.0/24).
                "subnetworkRangeName": "A String", # The name of a subnetwork secondary IP range from which to allocate an IP alias range. If not specified, the primary range of the subnetwork is used.
              },
            ],
            "fingerprint": "A String", # Fingerprint hash of contents stored in this network interface. This field will be ignored when inserting an Instance or adding a NetworkInterface. An up-to-date fingerprint must be provided in order to update the NetworkInterface. The request will fail with error 400 Bad Request if the fingerprint is not provided, or 412 Precondition Failed if the fingerprint is out of date.
            "internalIpv6PrefixLength": 42, # The prefix length of the primary internal IPv6 range.
            "ipv6AccessConfigs": [ # An array of IPv6 access configurations for this interface. Currently, only one IPv6 access config, DIRECT_IPV6, is supported. If there is no ipv6AccessConfig specified, then this instance will have no external IPv6 Internet access.
              { # An access configuration attached to an instance's network interface. Only one access config per instance is supported.
                "externalIpv6": "A String", # The first IPv6 address of the external IPv6 range associated with this instance, prefix length is stored in externalIpv6PrefixLength in ipv6AccessConfig. The field is output only, an IPv6 address from a subnetwork associated with the instance will be allocated dynamically.
                "externalIpv6PrefixLength": 42, # The prefix length of the external IPv6 range.
                "kind": "compute#accessConfig", # [Output Only] Type of the resource. Always compute#accessConfig for access configs.
                "name": "A String", # The name of this access configuration. The default and recommended name is External NAT, but you can use any arbitrary string, such as My external IP or Network Access.
                "natIP": "A String", # An external IP address associated with this instance. Specify an unused static external IP address available to the project or leave this field undefined to use an IP from a shared ephemeral IP address pool. If you specify a static external IP address, it must live in the same region as the zone of the instance.
                "networkTier": "A String", # This signifies the networking tier used for configuring this access configuration and can only take the following values: PREMIUM, STANDARD. If an AccessConfig is specified without a valid external IP address, an ephemeral IP will be created with this networkTier. If an AccessConfig with a valid external IP address is specified, it must match that of the networkTier associated with the Address resource owning that IP.
                "publicDnsName": "A String", # [Output Only] The public DNS domain name for the instance.
                "publicPtrDomainName": "A String", # The DNS domain name for the public PTR record. You can set this field only if the `setPublicPtr` field is enabled in accessConfig. If this field is unspecified in ipv6AccessConfig, a default PTR record will be createc for first IP in associated external IPv6 range.
                "setPublicDns": True or False, # Specifies whether a public DNS 'A' record should be created for the external IP address of this access configuration.
                "setPublicPtr": True or False, # Specifies whether a public DNS 'PTR' record should be created to map the external IP address of the instance to a DNS domain name. This field is not used in ipv6AccessConfig. A default PTR record will be created if the VM has external IPv6 range associated.
                "type": "ONE_TO_ONE_NAT", # The type of configuration. The default and only option is ONE_TO_ONE_NAT.
              },
            ],
            "ipv6AccessType": "A String", # [Output Only] One of EXTERNAL, INTERNAL to indicate whether the IP can be accessed from the Internet. This field is always inherited from its subnetwork. Valid only if stackType is IPV4_IPV6.
            "ipv6Address": "A String", # An IPv6 internal network address for this network interface.
            "kind": "compute#networkInterface", # [Output Only] Type of the resource. Always compute#networkInterface for network interfaces.
            "name": "A String", # [Output Only] The name of the network interface, which is generated by the server. For a VM, the network interface uses the nicN naming format. Where N is a value between 0 and 7. The default interface value is nic0.
            "network": "A String", # URL of the VPC network resource for this instance. When creating an instance, if neither the network nor the subnetwork is specified, the default network global/networks/default is used. If the selected project doesn't have the default network, you must specify a network or subnet. If the network is not specified but the subnetwork is specified, the network is inferred. If you specify this property, you can specify the network as a full or partial URL. For example, the following are all valid URLs: - https://www.googleapis.com/compute/v1/projects/project/global/networks/ network - projects/project/global/networks/network - global/networks/default
            "networkIP": "A String", # An IPv4 internal IP address to assign to the instance for this network interface. If not specified by the user, an unused internal IP is assigned by the system.
            "nicType": "A String", # The type of vNIC to be used on this interface. This may be gVNIC or VirtioNet.
            "queueCount": 42, # The networking queue count that's specified by users for the network interface. Both Rx and Tx queues will be set to this number. It'll be empty if not specified by the users.
            "stackType": "A String", # The stack type for this network interface to identify whether the IPv6 feature is enabled or not. If not specified, IPV4_ONLY will be used. This field can be both set at instance creation and update network interface operations.
            "subinterfaces": [ # SubInterfaces help enable L2 communication for the instance over subnetworks that support L2. Every network interface will get a default untagged (vlan not specified) subinterface. Users can specify additional tagged subinterfaces which are sub-fields to the Network Interface.
              {
                "ipAddress": "A String", # An IPv4 internal IP address to assign to the instance for this subinterface. If specified, ip_allocation_mode should be set to ALLOCATE_IP.
                "ipAllocationMode": "A String",
                "subnetwork": "A String", # If specified, this subnetwork must belong to the same network as that of the network interface. If not specified the subnet of network interface will be used. If you specify this property, you can specify the subnetwork as a full or partial URL. For example, the following are all valid URLs: - https://www.googleapis.com/compute/v1/projects/project/regions/region /subnetworks/subnetwork - regions/region/subnetworks/subnetwork
                "vlan": 42, # VLAN tag. Should match the VLAN(s) supported by the subnetwork to which this subinterface is connecting.
              },
            ],
            "subnetwork": "A String", # The URL of the Subnetwork resource for this instance. If the network resource is in legacy mode, do not specify this field. If the network is in auto subnet mode, specifying the subnetwork is optional. If the network is in custom subnet mode, specifying the subnetwork is required. If you specify this field, you can specify the subnetwork as a full or partial URL. For example, the following are all valid URLs: - https://www.googleapis.com/compute/v1/projects/project/regions/region /subnetworks/subnetwork - regions/region/subnetworks/subnetwork
          },
        ],
        "networkPerformanceConfig": { # Note that for MachineImage, this is not supported yet.
          "externalIpEgressBandwidthTier": "A String",
          "totalEgressBandwidthTier": "A String",
        },
        "postKeyRevocationActionType": "A String", # PostKeyRevocationActionType of the instance.
        "privateIpv6GoogleAccess": "A String", # The private IPv6 google access type for VMs. If not specified, use INHERIT_FROM_SUBNETWORK as default. Note that for MachineImage, this is not supported yet.
        "reservationAffinity": { # Specifies the reservations that this instance can consume from. # Specifies the reservations that instances can consume from. Note that for MachineImage, this is not supported yet.
          "consumeReservationType": "A String", # Specifies the type of reservation from which this instance can consume resources: ANY_RESERVATION (default), SPECIFIC_RESERVATION, or NO_RESERVATION. See Consuming reserved instances for examples.
          "key": "A String", # Corresponds to the label key of a reservation resource. To target a SPECIFIC_RESERVATION by name, specify googleapis.com/reservation-name as the key and specify the name of your reservation as its value.
          "values": [ # Corresponds to the label values of a reservation resource. This can be either a name to a reservation in the same project or "projects/different-project/reservations/some-reservation-name" to target a shared reservation in the same zone but in a different project.
            "A String",
          ],
        },
        "resourceManagerTags": { # Resource manager tags to be bound to the instance. Tag keys and values have the same definition as resource manager tags. Keys must be in the format `tagKeys/{tag_key_id}`, and values are in the format `tagValues/456`. The field is ignored (both PUT & PATCH) when empty.
          "a_key": "A String",
        },
        "resourcePolicies": [ # Resource policies (names, not URLs) applied to instances created from these properties. Note that for MachineImage, this is not supported yet.
          "A String",
        ],
        "scheduling": { # Sets the scheduling options for an Instance. NextID: 21 # Specifies the scheduling options for the instances that are created from these properties.
          "automaticRestart": True or False, # Specifies whether the instance should be automatically restarted if it is terminated by Compute Engine (not terminated by a user). You can only set the automatic restart option for standard instances. Preemptible instances cannot be automatically restarted. By default, this is set to true so an instance is automatically restarted if it is terminated by Compute Engine.
          "availabilityDomain": 42, # Specifies the availability domain (AD), which this instance should be scheduled on. The AD belongs to the spread GroupPlacementPolicy resource policy that has been assigned to the instance. Specify a value between 1-max count of availability domains in your GroupPlacementPolicy. See go/placement-policy-extension for more details.
          "currentCpus": 42, # Current number of vCPUs available for VM. 0 or unset means default vCPUs of the current machine type.
          "currentMemoryMb": "A String", # Current amount of memory (in MB) available for VM. 0 or unset means default amount of memory of the current machine type.
          "hostErrorTimeoutSeconds": 42, # Specify the time in seconds for host error detection, the value must be within the range of [90, 330] with the increment of 30, if unset, the default behavior of host error recovery will be used.
          "instanceTerminationAction": "A String", # Specifies the termination action for the instance.
          "latencyTolerant": True or False, # Defines whether the instance is tolerant of higher cpu latency. This can only be set during instance creation, or when the instance is not currently running. It must not be set if the preemptible option is also set.
          "locationHint": "A String", # An opaque location hint used to place the instance close to other resources. This field is for use by internal tools that use the public API.
          "maintenanceFreezeDurationHours": 42, # Specifies the number of hours after VM instance creation where the VM won't be scheduled for maintenance.
          "maintenanceInterval": "A String", # For more information about maintenance intervals, see Setting maintenance intervals.
          "maxRunDuration": { # A Duration represents a fixed-length span of time represented as a count of seconds and fractions of seconds at nanosecond resolution. It is independent of any calendar and concepts like "day" or "month". Range is approximately 10,000 years. # Specifies the max run duration for the given instance. If specified, the instance termination action will be performed at the end of the run duration.
            "nanos": 42, # Span of time that's a fraction of a second at nanosecond resolution. Durations less than one second are represented with a 0 `seconds` field and a positive `nanos` field. Must be from 0 to 999,999,999 inclusive.
            "seconds": "A String", # Span of time at a resolution of a second. Must be from 0 to 315,576,000,000 inclusive. Note: these bounds are computed from: 60 sec/min * 60 min/hr * 24 hr/day * 365.25 days/year * 10000 years
          },
          "minNodeCpus": 42, # The minimum number of virtual CPUs this instance will consume when running on a sole-tenant node.
          "nodeAffinities": [ # A set of node affinity and anti-affinity configurations. Refer to Configuring node affinity for more information. Overrides reservationAffinity.
            { # Node Affinity: the configuration of desired nodes onto which this Instance could be scheduled.
              "key": "A String", # Corresponds to the label key of Node resource.
              "operator": "A String", # Defines the operation of node selection. Valid operators are IN for affinity and NOT_IN for anti-affinity.
              "values": [ # Corresponds to the label values of Node resource.
                "A String",
              ],
            },
          ],
          "onHostMaintenance": "A String", # Defines the maintenance behavior for this instance. For standard instances, the default behavior is MIGRATE. For preemptible instances, the default and only possible behavior is TERMINATE. For more information, see Set VM host maintenance policy.
          "preemptible": True or False, # Defines whether the instance is preemptible. This can only be set during instance creation or while the instance is stopped and therefore, in a `TERMINATED` state. See Instance Life Cycle for more information on the possible instance states.
          "provisioningModel": "A String", # Specifies the provisioning model of the instance.
          "terminationTime": "A String", # Specifies the timestamp, when the instance will be terminated, in RFC3339 text format. If specified, the instance termination action will be performed at the termination time.
        },
        "secureTags": [ # [Input Only] Secure tags to apply to this instance. Maximum number of secure tags allowed is 50. Note that for MachineImage, this is not supported yet.
          "A String",
        ],
        "serviceAccounts": [ # A list of service accounts with specified scopes. Access tokens for these service accounts are available to the instances that are created from these properties. Use metadata queries to obtain the access tokens for these instances.
          { # A service account.
            "email": "A String", # Email address of the service account.
            "scopes": [ # The list of scopes to be made available for this service account.
              "A String",
            ],
          },
        ],
        "shieldedInstanceConfig": { # A set of Shielded Instance options. # Note that for MachineImage, this is not supported yet.
          "enableIntegrityMonitoring": True or False, # Defines whether the instance has integrity monitoring enabled. Enabled by default.
          "enableSecureBoot": True or False, # Defines whether the instance has Secure Boot enabled. Disabled by default.
          "enableVtpm": True or False, # Defines whether the instance has the vTPM enabled. Enabled by default.
        },
        "shieldedVmConfig": { # A set of Shielded VM options. # Specifies the Shielded VM options for the instances that are created from these properties.
          "enableIntegrityMonitoring": True or False, # Defines whether the instance has integrity monitoring enabled.
          "enableSecureBoot": True or False, # Defines whether the instance has Secure Boot enabled.
          "enableVtpm": True or False, # Defines whether the instance has the vTPM enabled.
        },
        "tags": { # A set of instance tags. # A list of tags to apply to the instances that are created from these properties. The tags identify valid sources or targets for network firewalls. The setTags method can modify this list of tags. Each tag within the list must comply with RFC1035.
          "fingerprint": "A String", # Specifies a fingerprint for this request, which is essentially a hash of the tags' contents and used for optimistic locking. The fingerprint is initially generated by Compute Engine and changes after every request to modify or update tags. You must always provide an up-to-date fingerprint hash in order to update or change tags. To see the latest fingerprint, make get() request to the instance.
          "items": [ # An array of tags. Each tag must be 1-63 characters long, and comply with RFC1035.
            "A String",
          ],
        },
      },
      "region": "A String", # [Output Only] URL of the region where the instance template resides. Only applicable for regional resources.
      "selfLink": "A String", # [Output Only] The URL for this instance template. The server defines this URL.
      "selfLinkWithId": "A String", # [Output Only] Server-defined URL for this resource with the resource id.
      "sourceInstance": "A String", # The source instance used to create the template. You can provide this as a partial or full URL to the resource. For example, the following are valid values: - https://www.googleapis.com/compute/v1/projects/project/zones/zone /instances/instance - projects/project/zones/zone/instances/instance
      "sourceInstanceParams": { # A specification of the parameters to use when creating the instance template from a source instance. # The source instance params to use to create this instance template.
        "diskConfigs": [ # Attached disks configuration. If not provided, defaults are applied: For boot disk and any other R/W disks, new custom images will be created from each disk. For read-only disks, they will be attached in read-only mode. Local SSD disks will be created as blank volumes.
          { # A specification of the desired way to instantiate a disk in the instance template when its created from a source instance.
            "autoDelete": True or False, # Specifies whether the disk will be auto-deleted when the instance is deleted (but not when the disk is detached from the instance).
            "customImage": "A String", # The custom source image to be used to restore this disk when instantiating this instance template.
            "deviceName": "A String", # Specifies the device name of the disk to which the configurations apply to.
            "instantiateFrom": "A String", # Specifies whether to include the disk and what image to use. Possible values are: - source-image: to use the same image that was used to create the source instance's corresponding disk. Applicable to the boot disk and additional read-write disks. - source-image-family: to use the same image family that was used to create the source instance's corresponding disk. Applicable to the boot disk and additional read-write disks. - custom-image: to use a user-provided image url for disk creation. Applicable to the boot disk and additional read-write disks. - attach-read-only: to attach a read-only disk. Applicable to read-only disks. - do-not-include: to exclude a disk from the template. Applicable to additional read-write disks, local SSDs, and read-only disks.
          },
        ],
      },
    }

`insert(project, region, body=None, requestId=None, x__xgafv=None)`

    Creates an instance template in the specified project and region using the global instance template whose URL is included in the request.

    Args:
      project: string, Project ID for this request. (required)
      region: string, The name of the region for this request. (required)
      body: object, The request body.
        The object takes the form of:

    { # Represents an Instance Template resource. You can use instance templates to create VM instances and managed instance groups. For more information, read Instance Templates.
      "creationTimestamp": "A String", # [Output Only] The creation timestamp for this instance template in RFC3339 text format.
      "description": "A String", # An optional description of this resource. Provide this property when you create the resource.
      "id": "A String", # [Output Only] A unique identifier for this instance template. The server defines this identifier.
      "kind": "compute#instanceTemplate", # [Output Only] The resource type, which is always compute#instanceTemplate for instance templates.
      "name": "A String", # Name of the resource; provided by the client when the resource is created. The name must be 1-63 characters long, and comply with RFC1035. Specifically, the name must be 1-63 characters long and match the regular expression `[a-z]([-a-z0-9]*[a-z0-9])?` which means the first character must be a lowercase letter, and all following characters must be a dash, lowercase letter, or digit, except the last character, which cannot be a dash.
      "properties": { # The instance properties for this instance template.
        "advancedMachineFeatures": { # Specifies options for controlling advanced machine features. Options that would traditionally be configured in a BIOS belong here. Features that require operating system support may have corresponding entries in the GuestOsFeatures of an Image (e.g., whether or not the OS in the Image supports nested virtualization being enabled or disabled). # Controls for advanced machine-related behavior features. Note that for MachineImage, this is not supported yet.
          "enableNestedVirtualization": True or False, # Whether to enable nested virtualization or not (default is false).
          "enableUefiNetworking": True or False, # Whether to enable UEFI networking for instance creation.
          "numaNodeCount": 42, # The number of vNUMA nodes.
          "threadsPerCore": 42, # The number of threads per physical core. To disable simultaneous multithreading (SMT) set this to 1. If unset, the maximum number of threads supported per core by the underlying processor is assumed.
          "visibleCoreCount": 42, # The number of physical cores to expose to an instance. Multiply by the number of threads per core to compute the total number of virtual CPUs to expose to the instance. If unset, the number of cores is inferred from the instance's nominal CPU count and the underlying platform's SMT width.
        },
        "canIpForward": True or False, # Enables instances created based on these properties to send packets with source IP addresses other than their own and receive packets with destination IP addresses other than their own. If these instances will be used as an IP gateway or it will be set as the next-hop in a Route resource, specify true. If unsure, leave this set to false. See the Enable IP forwarding documentation for more information.
        "confidentialInstanceConfig": { # A set of Confidential Instance options. # Specifies the Confidential Instance options. Note that for MachineImage, this is not supported yet.
          "confidentialInstanceType": "A String", # Defines the type of technology used by the confidential instance.
          "enableConfidentialCompute": True or False, # Defines whether the instance should have confidential compute enabled.
        },
        "description": "A String", # An optional text description for the instances that are created from these properties.
        "disks": [ # An array of disks that are associated with the instances that are created from these properties.
          { # An instance-attached disk resource.
            "architecture": "A String", # [Output Only] The architecture of the attached disk. Valid values are ARM64 or X86_64.
            "autoDelete": True or False, # Specifies whether the disk will be auto-deleted when the instance is deleted (but not when the disk is detached from the instance).
            "boot": True or False, # Indicates that this is a boot disk. The virtual machine will use the first partition of the disk for its root filesystem.
            "deviceName": "A String", # Specifies a unique device name of your choice that is reflected into the /dev/disk/by-id/google-* tree of a Linux operating system running within the instance. This name can be used to reference the device for mounting, resizing, and so on, from within the instance. If not specified, the server chooses a default device name to apply to this disk, in the form persistent-disk-x, where x is a number assigned by Google Compute Engine. This field is only applicable for persistent disks.
            "diskEncryptionKey": { # Encrypts or decrypts a disk using a customer-supplied encryption key. If you are creating a new disk, this field encrypts the new disk using an encryption key that you provide. If you are attaching an existing disk that is already encrypted, this field decrypts the disk using the customer-supplied encryption key. If you encrypt a disk using a customer-supplied key, you must provide the same key again when you attempt to use this resource at a later time. For example, you must provide the key when you create a snapshot or an image from the disk or when you attach the disk to a virtual machine instance. If you do not provide an encryption key, then the disk will be encrypted using an automatically generated key and you do not need to provide a key to use the disk later. Instance templates do not store customer-supplied encryption keys, so you cannot use your own keys to encrypt disks in a managed instance group.
              "kmsKeyName": "A String", # The name of the encryption key that is stored in Google Cloud KMS. For example: "kmsKeyName": "projects/kms_project_id/locations/region/keyRings/ key_region/cryptoKeys/key
              "kmsKeyServiceAccount": "A String", # The service account being used for the encryption request for the given KMS key. If absent, the Compute Engine default service account is used. For example: "kmsKeyServiceAccount": "name@project_id.iam.gserviceaccount.com/
              "rawKey": "A String", # Specifies a 256-bit customer-supplied encryption key, encoded in RFC 4648 base64 to either encrypt or decrypt this resource. You can provide either the rawKey or the rsaEncryptedKey. For example: "rawKey": "SGVsbG8gZnJvbSBHb29nbGUgQ2xvdWQgUGxhdGZvcm0="
              "rsaEncryptedKey": "A String", # Specifies an RFC 4648 base64 encoded, RSA-wrapped 2048-bit customer-supplied encryption key to either encrypt or decrypt this resource. You can provide either the rawKey or the rsaEncryptedKey. For example: "rsaEncryptedKey": "ieCx/NcW06PcT7Ep1X6LUTc/hLvUDYyzSZPPVCVPTVEohpeHASqC8uw5TzyO9U+Fka9JFH z0mBibXUInrC/jEk014kCK/NPjYgEMOyssZ4ZINPKxlUh2zn1bV+MCaTICrdmuSBTWlUUiFoD D6PYznLwh8ZNdaheCeZ8ewEXgFQ8V+sDroLaN3Xs3MDTXQEMMoNUXMCZEIpg9Vtp9x2oe==" The key must meet the following requirements before you can provide it to Compute Engine: 1. The key is wrapped using a RSA public key certificate provided by Google. 2. After being wrapped, the key must be encoded in RFC 4648 base64 encoding. Gets the RSA public key certificate provided by Google at: https://cloud-certs.storage.googleapis.com/google-cloud-csek-ingress.pem
              "sha256": "A String", # [Output only] The RFC 4648 base64 encoded SHA-256 hash of the customer-supplied encryption key that protects this resource.
            },
            "diskSizeGb": "A String", # The size of the disk in GB.
            "forceAttach": True or False, # [Input Only] Whether to force attach the regional disk even if it's currently attached to another instance. If you try to force attach a zonal disk to an instance, you will receive an error.
            "guestOsFeatures": [ # A list of features to enable on the guest operating system. Applicable only for bootable images. Read Enabling guest operating system features to see a list of available options.
              { # Guest OS features.
                "type": "A String", # The ID of a supported feature. To add multiple values, use commas to separate values. Set to one or more of the following values: - VIRTIO_SCSI_MULTIQUEUE - WINDOWS - MULTI_IP_SUBNET - UEFI_COMPATIBLE - GVNIC - SEV_CAPABLE - SUSPEND_RESUME_COMPATIBLE - SEV_SNP_CAPABLE For more information, see Enabling guest operating system features.
              },
            ],
            "index": 42, # [Output Only] A zero-based index to this disk, where 0 is reserved for the boot disk. If you have many disks attached to an instance, each disk would have a unique index number.
            "initializeParams": { # [Input Only] Specifies the parameters for a new disk that will be created alongside the new instance. Use initialization parameters to create boot disks or local SSDs attached to the new instance. This field is persisted and returned for instanceTemplate and not returned in the context of instance. This property is mutually exclusive with the source property; you can only define one or the other, but not both. # [Input Only] Specifies the parameters for a new disk that will be created alongside the new instance. Use initialization parameters to create boot disks or local SSDs attached to the new instance. This property is mutually exclusive with the source property; you can only define one or the other, but not both.
              "architecture": "A String", # The architecture of the attached disk. Valid values are arm64 or x86_64.
              "description": "A String", # An optional description. Provide this property when creating the disk.
              "diskName": "A String", # Specifies the disk name. If not specified, the default is to use the name of the instance. If a disk with the same name already exists in the given region, the existing disk is attached to the new instance and the new disk is not created.
              "diskSizeGb": "A String", # Specifies the size of the disk in base-2 GB. The size must be at least 10 GB. If you specify a sourceImage, which is required for boot disks, the default size is the size of the sourceImage. If you do not specify a sourceImage, the default disk size is 500 GB.
              "diskType": "A String", # Specifies the disk type to use to create the instance. If not specified, the default is pd-standard, specified using the full URL. For example: https://www.googleapis.com/compute/v1/projects/project/zones/zone /diskTypes/pd-standard For a full list of acceptable values, see Persistent disk types. If you define this field, you can provide either the full or partial URL. For example, the following are valid values: - https://www.googleapis.com/compute/v1/projects/project/zones/zone /diskTypes/diskType - projects/project/zones/zone/diskTypes/diskType - zones/zone/diskTypes/diskType Note that for InstanceTemplate, this is the name of the disk type, not URL.
              "guestOsFeatures": [ # A list of features to enable on the guest operating system. Applicable only for bootable images. Read Enabling guest operating system features to see a list of available options. Guest OS features are applied by merging initializeParams.guestOsFeatures and disks.guestOsFeatures
                { # Guest OS features.
                  "type": "A String", # The ID of a supported feature. To add multiple values, use commas to separate values. Set to one or more of the following values: - VIRTIO_SCSI_MULTIQUEUE - WINDOWS - MULTI_IP_SUBNET - UEFI_COMPATIBLE - GVNIC - SEV_CAPABLE - SUSPEND_RESUME_COMPATIBLE - SEV_SNP_CAPABLE For more information, see Enabling guest operating system features.
                },
              ],
              "interface": "A String", # [Deprecated] Specifies the disk interface to use for attaching this disk, which is either SCSI or NVME. The default is SCSI.
              "labels": { # Labels to apply to this disk. These can be later modified by the disks.setLabels method. This field is only applicable for persistent disks.
                "a_key": "A String",
              },
              "licenseCodes": [ # Integer license codes indicating which licenses are attached to this disk.
                "A String",
              ],
              "licenses": [ # A list of publicly visible licenses. Reserved for Google's use.
                "A String",
              ],
              "multiWriter": True or False, # Indicates whether or not the disk can be read/write attached to more than one instance.
              "onUpdateAction": "A String", # Specifies which action to take on instance update with this disk. Default is to use the existing disk.
              "provisionedIops": "A String", # Indicates how many IOPS to provision for the disk. This sets the number of I/O operations per second that the disk can handle. Values must be between 10,000 and 120,000. For more details, see the Extreme persistent disk documentation.
              "replicaZones": [ # URLs of the zones where the disk should be replicated to. Only applicable for regional resources.
                "A String",
              ],
              "resourcePolicies": [ # Resource policies applied to this disk for automatic snapshot creations. Specified using the full or partial URL. For instance template, specify only the resource policy name.
                "A String",
              ],
              "sourceImage": "A String", # The source image to create this disk. When creating a new instance, one of initializeParams.sourceImage or initializeParams.sourceSnapshot or disks.source is required except for local SSD. To create a disk with one of the public operating system images, specify the image by its family name. For example, specify family/debian-9 to use the latest Debian 9 image: projects/debian-cloud/global/images/family/debian-9 Alternatively, use a specific version of a public operating system image: projects/debian-cloud/global/images/debian-9-stretch-vYYYYMMDD To create a disk with a custom image that you created, specify the image name in the following format: global/images/my-custom-image You can also specify a custom image by its image family, which returns the latest version of the image in that family. Replace the image name with family/family-name: global/images/family/my-image-family If the source image is deleted later, this field will not be set.
              "sourceImageEncryptionKey": { # The customer-supplied encryption key of the source image. Required if the source image is protected by a customer-supplied encryption key. Instance templates do not store customer-supplied encryption keys, so you cannot create disks for instances in a managed instance group if the source images are encrypted with your own keys.
                "kmsKeyName": "A String", # The name of the encryption key that is stored in Google Cloud KMS. For example: "kmsKeyName": "projects/kms_project_id/locations/region/keyRings/ key_region/cryptoKeys/key
                "kmsKeyServiceAccount": "A String", # The service account being used for the encryption request for the given KMS key. If absent, the Compute Engine default service account is used. For example: "kmsKeyServiceAccount": "name@project_id.iam.gserviceaccount.com/
                "rawKey": "A String", # Specifies a 256-bit customer-supplied encryption key, encoded in RFC 4648 base64 to either encrypt or decrypt this resource. You can provide either the rawKey or the rsaEncryptedKey. For example: "rawKey": "SGVsbG8gZnJvbSBHb29nbGUgQ2xvdWQgUGxhdGZvcm0="
                "rsaEncryptedKey": "A String", # Specifies an RFC 4648 base64 encoded, RSA-wrapped 2048-bit customer-supplied encryption key to either encrypt or decrypt this resource. You can provide either the rawKey or the rsaEncryptedKey. For example: "rsaEncryptedKey": "ieCx/NcW06PcT7Ep1X6LUTc/hLvUDYyzSZPPVCVPTVEohpeHASqC8uw5TzyO9U+Fka9JFH z0mBibXUInrC/jEk014kCK/NPjYgEMOyssZ4ZINPKxlUh2zn1bV+MCaTICrdmuSBTWlUUiFoD D6PYznLwh8ZNdaheCeZ8ewEXgFQ8V+sDroLaN3Xs3MDTXQEMMoNUXMCZEIpg9Vtp9x2oe==" The key must meet the following requirements before you can provide it to Compute Engine: 1. The key is wrapped using a RSA public key certificate provided by Google. 2. After being wrapped, the key must be encoded in RFC 4648 base64 encoding. Gets the RSA public key certificate provided by Google at: https://cloud-certs.storage.googleapis.com/google-cloud-csek-ingress.pem
                "sha256": "A String", # [Output only] The RFC 4648 base64 encoded SHA-256 hash of the customer-supplied encryption key that protects this resource.
              },
              "sourceInstantSnapshot": "A String", # The source instant-snapshot to create this disk. When creating a new instance, one of initializeParams.sourceSnapshot or initializeParams.sourceInstantSnapshot initializeParams.sourceImage or disks.source is required except for local SSD. To create a disk with a snapshot that you created, specify the snapshot name in the following format: us-central1-a/instantSnapshots/my-backup If the source instant-snapshot is deleted later, this field will not be set.
              "sourceSnapshot": "A String", # The source snapshot to create this disk. When creating a new instance, one of initializeParams.sourceSnapshot or initializeParams.sourceImage or disks.source is required except for local SSD. To create a disk with a snapshot that you created, specify the snapshot name in the following format: global/snapshots/my-backup If the source snapshot is deleted later, this field will not be set.
              "sourceSnapshotEncryptionKey": { # The customer-supplied encryption key of the source snapshot.
                "kmsKeyName": "A String", # The name of the encryption key that is stored in Google Cloud KMS. For example: "kmsKeyName": "projects/kms_project_id/locations/region/keyRings/ key_region/cryptoKeys/key
                "kmsKeyServiceAccount": "A String", # The service account being used for the encryption request for the given KMS key. If absent, the Compute Engine default service account is used. For example: "kmsKeyServiceAccount": "name@project_id.iam.gserviceaccount.com/
                "rawKey": "A String", # Specifies a 256-bit customer-supplied encryption key, encoded in RFC 4648 base64 to either encrypt or decrypt this resource. You can provide either the rawKey or the rsaEncryptedKey. For example: "rawKey": "SGVsbG8gZnJvbSBHb29nbGUgQ2xvdWQgUGxhdGZvcm0="
                "rsaEncryptedKey": "A String", # Specifies an RFC 4648 base64 encoded, RSA-wrapped 2048-bit customer-supplied encryption key to either encrypt or decrypt this resource. You can provide either the rawKey or the rsaEncryptedKey. For example: "rsaEncryptedKey": "ieCx/NcW06PcT7Ep1X6LUTc/hLvUDYyzSZPPVCVPTVEohpeHASqC8uw5TzyO9U+Fka9JFH z0mBibXUInrC/jEk014kCK/NPjYgEMOyssZ4ZINPKxlUh2zn1bV+MCaTICrdmuSBTWlUUiFoD D6PYznLwh8ZNdaheCeZ8ewEXgFQ8V+sDroLaN3Xs3MDTXQEMMoNUXMCZEIpg9Vtp9x2oe==" The key must meet the following requirements before you can provide it to Compute Engine: 1. The key is wrapped using a RSA public key certificate provided by Google. 2. After being wrapped, the key must be encoded in RFC 4648 base64 encoding. Gets the RSA public key certificate provided by Google at: https://cloud-certs.storage.googleapis.com/google-cloud-csek-ingress.pem
                "sha256": "A String", # [Output only] The RFC 4648 base64 encoded SHA-256 hash of the customer-supplied encryption key that protects this resource.
              },
            },
            "interface": "A String", # Specifies the disk interface to use for attaching this disk, which is either SCSI or NVME. The default is SCSI. Persistent disks must always use SCSI and the request will fail if you attempt to attach a persistent disk in any other format than SCSI. Local SSDs can use either NVME or SCSI. For performance characteristics of SCSI over NVMe, see Local SSD performance.
            "kind": "compute#attachedDisk", # [Output Only] Type of the resource. Always compute#attachedDisk for attached disks.
            "licenses": [ # [Output Only] Any valid publicly visible licenses.
              "A String",
            ],
            "locked": True or False, # [Output Only] Whether to indicate the attached disk is locked. The locked disk is not allowed to be detached from the instance, or to be used as the source of the snapshot creation, and the image creation. The instance with at least one locked attached disk is not allow to be used as source of machine image creation, instant snapshot creation, and not allowed to be deleted with --keep-disk parameter set to true for locked disks.
            "mode": "A String", # The mode in which to attach this disk, either READ_WRITE or READ_ONLY. If not specified, the default is to attach the disk in READ_WRITE mode.
            "savedState": "A String", # For LocalSSD disks on VM Instances in STOPPED or SUSPENDED state, this field is set to PRESERVED if the LocalSSD data has been saved to a persistent location by customer request. (see the discard_local_ssd option on Stop/Suspend). Read-only in the api.
            "shieldedInstanceInitialState": { # Initial State for shielded instance, these are public keys which are safe to store in public # [Output Only] shielded vm initial state stored on disk
              "dbs": [ # The Key Database (db).
                {
                  "content": "A String", # The raw content in the secure keys file.
                  "fileType": "A String", # The file type of source file.
                },
              ],
              "dbxs": [ # The forbidden key database (dbx).
                {
                  "content": "A String", # The raw content in the secure keys file.
                  "fileType": "A String", # The file type of source file.
                },
              ],
              "keks": [ # The Key Exchange Key (KEK).
                {
                  "content": "A String", # The raw content in the secure keys file.
                  "fileType": "A String", # The file type of source file.
                },
              ],
              "pk": { # The Platform Key (PK).
                "content": "A String", # The raw content in the secure keys file.
                "fileType": "A String", # The file type of source file.
              },
            },
            "source": "A String", # Specifies a valid partial or full URL to an existing Persistent Disk resource. When creating a new instance, one of initializeParams.sourceImage or initializeParams.sourceSnapshot or disks.source is required except for local SSD. If desired, you can also attach existing non-root persistent disks using this property. This field is only applicable for persistent disks. Note that for InstanceTemplate, specify the disk name for zonal disk, and the URL for regional disk.
            "type": "A String", # Specifies the type of the disk, either SCRATCH or PERSISTENT. If not specified, the default is PERSISTENT.
            "userLicenses": [ # [Output Only] A list of user provided licenses. It represents a list of URLs to the license resource. Unlike regular licenses, user provided licenses can be modified after the disk is created.
              "A String",
            ],
          },
        ],
        "displayDevice": { # A set of Display Device options # Display Device properties to enable support for remote display products like: Teradici, VNC and TeamViewer Note that for MachineImage, this is not supported yet.
          "enableDisplay": True or False, # Defines whether the instance has Display enabled.
        },
        "guestAccelerators": [ # A list of guest accelerator cards' type and count to use for instances created from these properties.
          { # A specification of the type and number of accelerator cards attached to the instance.
            "acceleratorCount": 42, # The number of the guest accelerator cards exposed to this instance.
            "acceleratorType": "A String", # Full or partial URL of the accelerator type resource to attach to this instance. For example: projects/my-project/zones/us-central1-c/acceleratorTypes/nvidia-tesla-p100 If you are creating an instance template, specify only the accelerator name. See GPUs on Compute Engine for a full list of accelerator types.
          },
        ],
        "keyRevocationActionType": "A String", # KeyRevocationActionType of the instance. Supported options are "STOP" and "NONE". The default value is "NONE" if it is not specified.
        "labels": { # Labels to apply to instances that are created from these properties.
          "a_key": "A String",
        },
        "machineType": "A String", # The machine type to use for instances that are created from these properties.
        "metadata": { # A metadata key/value entry. # The metadata key/value pairs to assign to instances that are created from these properties. These pairs can consist of custom metadata or predefined keys. See Project and instance metadata for more information.
          "fingerprint": "A String", # Specifies a fingerprint for this request, which is essentially a hash of the metadata's contents and used for optimistic locking. The fingerprint is initially generated by Compute Engine and changes after every request to modify or update metadata. You must always provide an up-to-date fingerprint hash in order to update or change metadata, otherwise the request will fail with error 412 conditionNotMet. To see the latest fingerprint, make a get() request to retrieve the resource.
          "items": [ # Array of key/value pairs. The total size of all keys and values must be less than 512 KB.
            { # Metadata
              "key": "A String", # Key for the metadata entry. Keys must conform to the following regexp: [a-zA-Z0-9-_]+, and be less than 128 bytes in length. This is reflected as part of a URL in the metadata server. Additionally, to avoid ambiguity, keys must not conflict with any other metadata keys for the project.
              "value": "A String", # Value for the metadata entry. These are free-form strings, and only have meaning as interpreted by the image running in the instance. The only restriction placed on values is that their size must be less than or equal to 262144 bytes (256 KiB).
            },
          ],
          "kind": "compute#metadata", # [Output Only] Type of the resource. Always compute#metadata for metadata.
        },
        "minCpuPlatform": "A String", # Minimum cpu/platform to be used by instances. The instance may be scheduled on the specified or newer cpu/platform. Applicable values are the friendly names of CPU platforms, such as minCpuPlatform: "Intel Haswell" or minCpuPlatform: "Intel Sandy Bridge". For more information, read Specifying a Minimum CPU Platform.
        "networkInterfaces": [ # An array of network access configurations for this interface.
          { # A network interface resource attached to an instance.
            "accessConfigs": [ # An array of configurations for this interface. Currently, only one access config, ONE_TO_ONE_NAT, is supported. If there are no accessConfigs specified, then this instance will have no external internet access.
              { # An access configuration attached to an instance's network interface. Only one access config per instance is supported.
                "externalIpv6": "A String", # The first IPv6 address of the external IPv6 range associated with this instance, prefix length is stored in externalIpv6PrefixLength in ipv6AccessConfig. The field is output only, an IPv6 address from a subnetwork associated with the instance will be allocated dynamically.
                "externalIpv6PrefixLength": 42, # The prefix length of the external IPv6 range.
                "kind": "compute#accessConfig", # [Output Only] Type of the resource. Always compute#accessConfig for access configs.
                "name": "A String", # The name of this access configuration. The default and recommended name is External NAT, but you can use any arbitrary string, such as My external IP or Network Access.
                "natIP": "A String", # An external IP address associated with this instance. Specify an unused static external IP address available to the project or leave this field undefined to use an IP from a shared ephemeral IP address pool. If you specify a static external IP address, it must live in the same region as the zone of the instance.
                "networkTier": "A String", # This signifies the networking tier used for configuring this access configuration and can only take the following values: PREMIUM, STANDARD. If an AccessConfig is specified without a valid external IP address, an ephemeral IP will be created with this networkTier. If an AccessConfig with a valid external IP address is specified, it must match that of the networkTier associated with the Address resource owning that IP.
                "publicDnsName": "A String", # [Output Only] The public DNS domain name for the instance.
                "publicPtrDomainName": "A String", # The DNS domain name for the public PTR record. You can set this field only if the `setPublicPtr` field is enabled in accessConfig. If this field is unspecified in ipv6AccessConfig, a default PTR record will be createc for first IP in associated external IPv6 range.
                "setPublicDns": True or False, # Specifies whether a public DNS 'A' record should be created for the external IP address of this access configuration.
                "setPublicPtr": True or False, # Specifies whether a public DNS 'PTR' record should be created to map the external IP address of the instance to a DNS domain name. This field is not used in ipv6AccessConfig. A default PTR record will be created if the VM has external IPv6 range associated.
                "type": "ONE_TO_ONE_NAT", # The type of configuration. The default and only option is ONE_TO_ONE_NAT.
              },
            ],
            "aliasIpRanges": [ # An array of alias IP ranges for this network interface. You can only specify this field for network interfaces in VPC networks.
              { # An alias IP range attached to an instance's network interface.
                "ipCidrRange": "A String", # The IP alias ranges to allocate for this interface. This IP CIDR range must belong to the specified subnetwork and cannot contain IP addresses reserved by system or used by other network interfaces. This range may be a single IP address (such as 10.2.3.4), a netmask (such as /24) or a CIDR-formatted string (such as 10.1.2.0/24).
                "subnetworkRangeName": "A String", # The name of a subnetwork secondary IP range from which to allocate an IP alias range. If not specified, the primary range of the subnetwork is used.
              },
            ],
            "fingerprint": "A String", # Fingerprint hash of contents stored in this network interface. This field will be ignored when inserting an Instance or adding a NetworkInterface. An up-to-date fingerprint must be provided in order to update the NetworkInterface. The request will fail with error 400 Bad Request if the fingerprint is not provided, or 412 Precondition Failed if the fingerprint is out of date.
            "internalIpv6PrefixLength": 42, # The prefix length of the primary internal IPv6 range.
            "ipv6AccessConfigs": [ # An array of IPv6 access configurations for this interface. Currently, only one IPv6 access config, DIRECT_IPV6, is supported. If there is no ipv6AccessConfig specified, then this instance will have no external IPv6 Internet access.
              { # An access configuration attached to an instance's network interface. Only one access config per instance is supported.
                "externalIpv6": "A String", # The first IPv6 address of the external IPv6 range associated with this instance, prefix length is stored in externalIpv6PrefixLength in ipv6AccessConfig. The field is output only, an IPv6 address from a subnetwork associated with the instance will be allocated dynamically.
                "externalIpv6PrefixLength": 42, # The prefix length of the external IPv6 range.
                "kind": "compute#accessConfig", # [Output Only] Type of the resource. Always compute#accessConfig for access configs.
                "name": "A String", # The name of this access configuration. The default and recommended name is External NAT, but you can use any arbitrary string, such as My external IP or Network Access.
                "natIP": "A String", # An external IP address associated with this instance. Specify an unused static external IP address available to the project or leave this field undefined to use an IP from a shared ephemeral IP address pool. If you specify a static external IP address, it must live in the same region as the zone of the instance.
                "networkTier": "A String", # This signifies the networking tier used for configuring this access configuration and can only take the following values: PREMIUM, STANDARD. If an AccessConfig is specified without a valid external IP address, an ephemeral IP will be created with this networkTier. If an AccessConfig with a valid external IP address is specified, it must match that of the networkTier associated with the Address resource owning that IP.
                "publicDnsName": "A String", # [Output Only] The public DNS domain name for the instance.
                "publicPtrDomainName": "A String", # The DNS domain name for the public PTR record. You can set this field only if the `setPublicPtr` field is enabled in accessConfig. If this field is unspecified in ipv6AccessConfig, a default PTR record will be createc for first IP in associated external IPv6 range.
                "setPublicDns": True or False, # Specifies whether a public DNS 'A' record should be created for the external IP address of this access configuration.
                "setPublicPtr": True or False, # Specifies whether a public DNS 'PTR' record should be created to map the external IP address of the instance to a DNS domain name. This field is not used in ipv6AccessConfig. A default PTR record will be created if the VM has external IPv6 range associated.
                "type": "ONE_TO_ONE_NAT", # The type of configuration. The default and only option is ONE_TO_ONE_NAT.
              },
            ],
            "ipv6AccessType": "A String", # [Output Only] One of EXTERNAL, INTERNAL to indicate whether the IP can be accessed from the Internet. This field is always inherited from its subnetwork. Valid only if stackType is IPV4_IPV6.
            "ipv6Address": "A String", # An IPv6 internal network address for this network interface.
            "kind": "compute#networkInterface", # [Output Only] Type of the resource. Always compute#networkInterface for network interfaces.
            "name": "A String", # [Output Only] The name of the network interface, which is generated by the server. For a VM, the network interface uses the nicN naming format. Where N is a value between 0 and 7. The default interface value is nic0.
            "network": "A String", # URL of the VPC network resource for this instance. When creating an instance, if neither the network nor the subnetwork is specified, the default network global/networks/default is used. If the selected project doesn't have the default network, you must specify a network or subnet. If the network is not specified but the subnetwork is specified, the network is inferred. If you specify this property, you can specify the network as a full or partial URL. For example, the following are all valid URLs: - https://www.googleapis.com/compute/v1/projects/project/global/networks/ network - projects/project/global/networks/network - global/networks/default
            "networkIP": "A String", # An IPv4 internal IP address to assign to the instance for this network interface. If not specified by the user, an unused internal IP is assigned by the system.
            "nicType": "A String", # The type of vNIC to be used on this interface. This may be gVNIC or VirtioNet.
            "queueCount": 42, # The networking queue count that's specified by users for the network interface. Both Rx and Tx queues will be set to this number. It'll be empty if not specified by the users.
            "stackType": "A String", # The stack type for this network interface to identify whether the IPv6 feature is enabled or not. If not specified, IPV4_ONLY will be used. This field can be both set at instance creation and update network interface operations.
            "subinterfaces": [ # SubInterfaces help enable L2 communication for the instance over subnetworks that support L2. Every network interface will get a default untagged (vlan not specified) subinterface. Users can specify additional tagged subinterfaces which are sub-fields to the Network Interface.
              {
                "ipAddress": "A String", # An IPv4 internal IP address to assign to the instance for this subinterface. If specified, ip_allocation_mode should be set to ALLOCATE_IP.
                "ipAllocationMode": "A String",
                "subnetwork": "A String", # If specified, this subnetwork must belong to the same network as that of the network interface. If not specified the subnet of network interface will be used. If you specify this property, you can specify the subnetwork as a full or partial URL. For example, the following are all valid URLs: - https://www.googleapis.com/compute/v1/projects/project/regions/region /subnetworks/subnetwork - regions/region/subnetworks/subnetwork
                "vlan": 42, # VLAN tag. Should match the VLAN(s) supported by the subnetwork to which this subinterface is connecting.
              },
            ],
            "subnetwork": "A String", # The URL of the Subnetwork resource for this instance. If the network resource is in legacy mode, do not specify this field. If the network is in auto subnet mode, specifying the subnetwork is optional. If the network is in custom subnet mode, specifying the subnetwork is required. If you specify this field, you can specify the subnetwork as a full or partial URL. For example, the following are all valid URLs: - https://www.googleapis.com/compute/v1/projects/project/regions/region /subnetworks/subnetwork - regions/region/subnetworks/subnetwork
          },
        ],
        "networkPerformanceConfig": { # Note that for MachineImage, this is not supported yet.
          "externalIpEgressBandwidthTier": "A String",
          "totalEgressBandwidthTier": "A String",
        },
        "postKeyRevocationActionType": "A String", # PostKeyRevocationActionType of the instance.
        "privateIpv6GoogleAccess": "A String", # The private IPv6 google access type for VMs. If not specified, use INHERIT_FROM_SUBNETWORK as default. Note that for MachineImage, this is not supported yet.
        "reservationAffinity": { # Specifies the reservations that this instance can consume from. # Specifies the reservations that instances can consume from. Note that for MachineImage, this is not supported yet.
          "consumeReservationType": "A String", # Specifies the type of reservation from which this instance can consume resources: ANY_RESERVATION (default), SPECIFIC_RESERVATION, or NO_RESERVATION. See Consuming reserved instances for examples.
          "key": "A String", # Corresponds to the label key of a reservation resource. To target a SPECIFIC_RESERVATION by name, specify googleapis.com/reservation-name as the key and specify the name of your reservation as its value.
          "values": [ # Corresponds to the label values of a reservation resource. This can be either a name to a reservation in the same project or "projects/different-project/reservations/some-reservation-name" to target a shared reservation in the same zone but in a different project.
            "A String",
          ],
        },
        "resourceManagerTags": { # Resource manager tags to be bound to the instance. Tag keys and values have the same definition as resource manager tags. Keys must be in the format `tagKeys/{tag_key_id}`, and values are in the format `tagValues/456`. The field is ignored (both PUT & PATCH) when empty.
          "a_key": "A String",
        },
        "resourcePolicies": [ # Resource policies (names, not URLs) applied to instances created from these properties. Note that for MachineImage, this is not supported yet.
          "A String",
        ],
        "scheduling": { # Sets the scheduling options for an Instance. NextID: 21 # Specifies the scheduling options for the instances that are created from these properties.
          "automaticRestart": True or False, # Specifies whether the instance should be automatically restarted if it is terminated by Compute Engine (not terminated by a user). You can only set the automatic restart option for standard instances. Preemptible instances cannot be automatically restarted. By default, this is set to true so an instance is automatically restarted if it is terminated by Compute Engine.
          "availabilityDomain": 42, # Specifies the availability domain (AD), which this instance should be scheduled on. The AD belongs to the spread GroupPlacementPolicy resource policy that has been assigned to the instance. Specify a value between 1-max count of availability domains in your GroupPlacementPolicy. See go/placement-policy-extension for more details.
          "currentCpus": 42, # Current number of vCPUs available for VM. 0 or unset means default vCPUs of the current machine type.
          "currentMemoryMb": "A String", # Current amount of memory (in MB) available for VM. 0 or unset means default amount of memory of the current machine type.
          "hostErrorTimeoutSeconds": 42, # Specify the time in seconds for host error detection, the value must be within the range of [90, 330] with the increment of 30, if unset, the default behavior of host error recovery will be used.
          "instanceTerminationAction": "A String", # Specifies the termination action for the instance.
          "latencyTolerant": True or False, # Defines whether the instance is tolerant of higher cpu latency. This can only be set during instance creation, or when the instance is not currently running. It must not be set if the preemptible option is also set.
          "locationHint": "A String", # An opaque location hint used to place the instance close to other resources. This field is for use by internal tools that use the public API.
          "maintenanceFreezeDurationHours": 42, # Specifies the number of hours after VM instance creation where the VM won't be scheduled for maintenance.
          "maintenanceInterval": "A String", # For more information about maintenance intervals, see Setting maintenance intervals.
          "maxRunDuration": { # A Duration represents a fixed-length span of time represented as a count of seconds and fractions of seconds at nanosecond resolution. It is independent of any calendar and concepts like "day" or "month". Range is approximately 10,000 years. # Specifies the max run duration for the given instance. If specified, the instance termination action will be performed at the end of the run duration.
            "nanos": 42, # Span of time that's a fraction of a second at nanosecond resolution. Durations less than one second are represented with a 0 `seconds` field and a positive `nanos` field. Must be from 0 to 999,999,999 inclusive.
            "seconds": "A String", # Span of time at a resolution of a second. Must be from 0 to 315,576,000,000 inclusive. Note: these bounds are computed from: 60 sec/min * 60 min/hr * 24 hr/day * 365.25 days/year * 10000 years
          },
          "minNodeCpus": 42, # The minimum number of virtual CPUs this instance will consume when running on a sole-tenant node.
          "nodeAffinities": [ # A set of node affinity and anti-affinity configurations. Refer to Configuring node affinity for more information. Overrides reservationAffinity.
            { # Node Affinity: the configuration of desired nodes onto which this Instance could be scheduled.
              "key": "A String", # Corresponds to the label key of Node resource.
              "operator": "A String", # Defines the operation of node selection. Valid operators are IN for affinity and NOT_IN for anti-affinity.
              "values": [ # Corresponds to the label values of Node resource.
                "A String",
              ],
            },
          ],
          "onHostMaintenance": "A String", # Defines the maintenance behavior for this instance. For standard instances, the default behavior is MIGRATE. For preemptible instances, the default and only possible behavior is TERMINATE. For more information, see Set VM host maintenance policy.
          "preemptible": True or False, # Defines whether the instance is preemptible. This can only be set during instance creation or while the instance is stopped and therefore, in a `TERMINATED` state. See Instance Life Cycle for more information on the possible instance states.
          "provisioningModel": "A String", # Specifies the provisioning model of the instance.
          "terminationTime": "A String", # Specifies the timestamp, when the instance will be terminated, in RFC3339 text format. If specified, the instance termination action will be performed at the termination time.
        },
        "secureTags": [ # [Input Only] Secure tags to apply to this instance. Maximum number of secure tags allowed is 50. Note that for MachineImage, this is not supported yet.
          "A String",
        ],
        "serviceAccounts": [ # A list of service accounts with specified scopes. Access tokens for these service accounts are available to the instances that are created from these properties. Use metadata queries to obtain the access tokens for these instances.
          { # A service account.
            "email": "A String", # Email address of the service account.
            "scopes": [ # The list of scopes to be made available for this service account.
              "A String",
            ],
          },
        ],
        "shieldedInstanceConfig": { # A set of Shielded Instance options. # Note that for MachineImage, this is not supported yet.
          "enableIntegrityMonitoring": True or False, # Defines whether the instance has integrity monitoring enabled. Enabled by default.
          "enableSecureBoot": True or False, # Defines whether the instance has Secure Boot enabled. Disabled by default.
          "enableVtpm": True or False, # Defines whether the instance has the vTPM enabled. Enabled by default.
        },
        "shieldedVmConfig": { # A set of Shielded VM options. # Specifies the Shielded VM options for the instances that are created from these properties.
          "enableIntegrityMonitoring": True or False, # Defines whether the instance has integrity monitoring enabled.
          "enableSecureBoot": True or False, # Defines whether the instance has Secure Boot enabled.
          "enableVtpm": True or False, # Defines whether the instance has the vTPM enabled.
        },
        "tags": { # A set of instance tags. # A list of tags to apply to the instances that are created from these properties. The tags identify valid sources or targets for network firewalls. The setTags method can modify this list of tags. Each tag within the list must comply with RFC1035.
          "fingerprint": "A String", # Specifies a fingerprint for this request, which is essentially a hash of the tags' contents and used for optimistic locking. The fingerprint is initially generated by Compute Engine and changes after every request to modify or update tags. You must always provide an up-to-date fingerprint hash in order to update or change tags. To see the latest fingerprint, make get() request to the instance.
          "items": [ # An array of tags. Each tag must be 1-63 characters long, and comply with RFC1035.
            "A String",
          ],
        },
      },
      "region": "A String", # [Output Only] URL of the region where the instance template resides. Only applicable for regional resources.
      "selfLink": "A String", # [Output Only] The URL for this instance template. The server defines this URL.
      "selfLinkWithId": "A String", # [Output Only] Server-defined URL for this resource with the resource id.
      "sourceInstance": "A String", # The source instance used to create the template. You can provide this as a partial or full URL to the resource. For example, the following are valid values: - https://www.googleapis.com/compute/v1/projects/project/zones/zone /instances/instance - projects/project/zones/zone/instances/instance
      "sourceInstanceParams": { # A specification of the parameters to use when creating the instance template from a source instance. # The source instance params to use to create this instance template.
        "diskConfigs": [ # Attached disks configuration. If not provided, defaults are applied: For boot disk and any other R/W disks, new custom images will be created from each disk. For read-only disks, they will be attached in read-only mode. Local SSD disks will be created as blank volumes.
          { # A specification of the desired way to instantiate a disk in the instance template when its created from a source instance.
            "autoDelete": True or False, # Specifies whether the disk will be auto-deleted when the instance is deleted (but not when the disk is detached from the instance).
            "customImage": "A String", # The custom source image to be used to restore this disk when instantiating this instance template.
            "deviceName": "A String", # Specifies the device name of the disk to which the configurations apply to.
            "instantiateFrom": "A String", # Specifies whether to include the disk and what image to use. Possible values are: - source-image: to use the same image that was used to create the source instance's corresponding disk. Applicable to the boot disk and additional read-write disks. - source-image-family: to use the same image family that was used to create the source instance's corresponding disk. Applicable to the boot disk and additional read-write disks. - custom-image: to use a user-provided image url for disk creation. Applicable to the boot disk and additional read-write disks. - attach-read-only: to attach a read-only disk. Applicable to read-only disks. - do-not-include: to exclude a disk from the template. Applicable to additional read-write disks, local SSDs, and read-only disks.
          },
        ],
      },
    }

      requestId: string, An optional request ID to identify requests. Specify a unique request ID so that if you must retry your request, the server will know to ignore the request if it has already been completed. For example, consider a situation where you make an initial request and the request times out. If you make the request again with the same request ID, the server can check if original operation with the same request ID was received, and if so, will ignore the second request. This prevents clients from accidentally creating duplicate commitments. The request ID must be a valid UUID with the exception that zero UUID is not supported ( 00000000-0000-0000-0000-000000000000).
      x__xgafv: string, V1 error format.
        Allowed values
          1 - v1 error format
          2 - v2 error format

    Returns:
      An object of the form:

        { # Represents an Operation resource. Google Compute Engine has three Operation resources: * [Global](/compute/docs/reference/rest/alpha/globalOperations) * [Regional](/compute/docs/reference/rest/alpha/regionOperations) * [Zonal](/compute/docs/reference/rest/alpha/zoneOperations) You can use an operation resource to manage asynchronous API requests. For more information, read Handling API responses. Operations can be global, regional or zonal. - For global operations, use the `globalOperations` resource. - For regional operations, use the `regionOperations` resource. - For zonal operations, use the `zonalOperations` resource. For more information, read Global, Regional, and Zonal Resources.
      "clientOperationId": "A String", # [Output Only] The value of `requestId` if you provided it in the request. Not present otherwise.
      "creationTimestamp": "A String", # [Deprecated] This field is deprecated.
      "description": "A String", # [Output Only] A textual description of the operation, which is set when the operation is created.
      "endTime": "A String", # [Output Only] The time that this operation was completed. This value is in RFC3339 text format.
      "error": { # [Output Only] If errors are generated during processing of the operation, this field will be populated.
        "errors": [ # [Output Only] The array of errors encountered while processing this operation.
          {
            "code": "A String", # [Output Only] The error type identifier for this error.
            "errorDetails": [ # [Output Only] An optional list of messages that contain the error details. There is a set of defined message types to use for providing details.The syntax depends on the error code. For example, QuotaExceededInfo will have details when the error code is QUOTA_EXCEEDED.
              {
                "errorInfo": { # Describes the cause of the error with structured details. Example of an error when contacting the "pubsub.googleapis.com" API when it is not enabled: { "reason": "API_DISABLED" "domain": "googleapis.com" "metadata": { "resource": "projects/123", "service": "pubsub.googleapis.com" } } This response indicates that the pubsub.googleapis.com API is not enabled. Example of an error that is returned when attempting to create a Spanner instance in a region that is out of stock: { "reason": "STOCKOUT" "domain": "spanner.googleapis.com", "metadata": { "availableRegions": "us-central1,us-east2" } }
                  "domain": "A String", # The logical grouping to which the "reason" belongs. The error domain is typically the registered service name of the tool or product that generates the error. Example: "pubsub.googleapis.com". If the error is generated by some common infrastructure, the error domain must be a globally unique value that identifies the infrastructure. For Google API infrastructure, the error domain is "googleapis.com".
                  "metadatas": { # Additional structured details about this error. Keys should match /[a-zA-Z0-9-_]/ and be limited to 64 characters in length. When identifying the current value of an exceeded limit, the units should be contained in the key, not the value. For example, rather than {"instanceLimit": "100/request"}, should be returned as, {"instanceLimitPerRequest": "100"}, if the client exceeds the number of instances that can be created in a single (batch) request.
                    "a_key": "A String",
                  },
                  "reason": "A String", # The reason of the error. This is a constant value that identifies the proximate cause of the error. Error reasons are unique within a particular domain of errors. This should be at most 63 characters and match /[A-Z0-9_]+/.
                },
                "help": { # Provides links to documentation or for performing an out of band action. For example, if a quota check failed with an error indicating the calling project hasn't enabled the accessed service, this can contain a URL pointing directly to the right place in the developer console to flip the bit.
                  "links": [ # URL(s) pointing to additional information on handling the current error.
                    { # Describes a URL link.
                      "description": "A String", # Describes what the link offers.
                      "url": "A String", # The URL of the link.
                    },
                  ],
                },
                "localizedMessage": { # Provides a localized error message that is safe to return to the user which can be attached to an RPC error.
                  "locale": "A String", # The locale used following the specification defined at http://www.rfc-editor.org/rfc/bcp/bcp47.txt. Examples are: "en-US", "fr-CH", "es-MX"
                  "message": "A String", # The localized error message in the above locale.
                },
                "quotaInfo": { # Additional details for quota exceeded error for resource quota.
                  "dimensions": { # The map holding related quota dimensions.
                    "a_key": "A String",
                  },
                  "limit": 3.14, # Current effective quota limit. The limit's unit depends on the quota type or metric.
                  "limitName": "A String", # The name of the quota limit.
                  "metricName": "A String", # The Compute Engine quota metric name.
                },
              },
            ],
            "location": "A String", # [Output Only] Indicates the field in the request that caused the error. This property is optional.
            "message": "A String", # [Output Only] An optional, human-readable error message.
          },
        ],
      },
      "httpErrorMessage": "A String", # [Output Only] If the operation fails, this field contains the HTTP error message that was returned, such as `NOT FOUND`.
      "httpErrorStatusCode": 42, # [Output Only] If the operation fails, this field contains the HTTP error status code that was returned. For example, a `404` means the resource was not found.
      "id": "A String", # [Output Only] The unique identifier for the operation. This identifier is defined by the server.
      "insertTime": "A String", # [Output Only] The time that this operation was requested. This value is in RFC3339 text format.
      "kind": "compute#operation", # [Output Only] Type of the resource. Always `compute#operation` for Operation resources.
      "metadata": { # [Output Only] Service-specific metadata attached to this operation.
        "a_key": "", # Properties of the object. Contains field @type with type URL.
      },
      "name": "A String", # [Output Only] Name of the operation.
      "operationGroupId": "A String", # [Output Only] An ID that represents a group of operations, such as when a group of operations results from a `bulkInsert` API request.
      "operationType": "A String", # [Output Only] The type of operation, such as `insert`, `update`, or `delete`, and so on.
      "progress": 42, # [Output Only] An optional progress indicator that ranges from 0 to 100. There is no requirement that this be linear or support any granularity of operations. This should not be used to guess when the operation will be complete. This number should monotonically increase as the operation progresses.
      "region": "A String", # [Output Only] The URL of the region where the operation resides. Only applicable when performing regional operations.
      "selfLink": "A String", # [Output Only] Server-defined URL for the resource.
      "selfLinkWithId": "A String", # [Output Only] Server-defined URL for this resource with the resource id.
      "startTime": "A String", # [Output Only] The time that this operation was started by the server. This value is in RFC3339 text format.
      "status": "A String", # [Output Only] The status of the operation, which can be one of the following: `PENDING`, `RUNNING`, or `DONE`.
      "statusMessage": "A String", # [Output Only] An optional textual description of the current status of the operation.
      "targetId": "A String", # [Output Only] The unique target ID, which identifies a specific incarnation of the target resource.
      "targetLink": "A String", # [Output Only] The URL of the resource that the operation modifies. For operations related to creating a snapshot, this points to the persistent disk that the snapshot was created from.
      "user": "A String", # [Output Only] User who requested the operation, for example: `user@example.com`.
      "warnings": [ # [Output Only] If warning messages are generated during processing of the operation, this field will be populated.
        {
          "code": "A String", # [Output Only] A warning code, if applicable. For example, Compute Engine returns NO_RESULTS_ON_PAGE if there are no results in the response.
          "data": [ # [Output Only] Metadata about this warning in key: value format. For example: "data": [ { "key": "scope", "value": "zones/us-east1-d" }
            {
              "key": "A String", # [Output Only] A key that provides more detail on the warning being returned. For example, for warnings where there are no results in a list request for a particular zone, this key might be scope and the key value might be the zone name. Other examples might be a key indicating a deprecated resource and a suggested replacement, or a warning about invalid network settings (for example, if an instance attempts to perform IP forwarding but is not enabled for IP forwarding).
              "value": "A String", # [Output Only] A warning data value corresponding to the key.
            },
          ],
          "message": "A String", # [Output Only] A human-readable description of the warning code.
        },
      ],
      "zone": "A String", # [Output Only] The URL of the zone where the operation resides. Only applicable when performing per-zone operations.
    }

`list(project, region, filter=None, maxResults=None, orderBy=None, pageToken=None, returnPartialSuccess=None, x__xgafv=None)`

    Retrieves a list of instance templates that are contained within the specified project and region.

    Args:
      project: string, Project ID for this request. (required)
      region: string, The name of the regions for this request. (required)
      filter: string, A filter expression that filters resources listed in the response. Most Compute resources support two types of filter expressions: expressions that support regular expressions and expressions that follow API improvement proposal AIP-160. If you want to use AIP-160, your expression must specify the field name, an operator, and the value that you want to use for filtering. The value must be a string, a number, or a boolean. The operator must be either `=`, `!=`, `>`, `<`, `<=`, `>=` or `:`. For example, if you are filtering Compute Engine instances, you can exclude instances named `example-instance` by specifying `name != example-instance`. The `:` operator can be used with string fields to match substrings. For non-string fields it is equivalent to the `=` operator. The `:*` comparison can be used to test whether a key has been defined. For example, to find all objects with `owner` label use: ``` labels.owner:* ``` You can also filter nested fields. For example, you could specify `scheduling.automaticRestart = false` to include instances only if they are not scheduled for automatic restarts. You can use filtering on nested fields to filter based on resource labels. To filter on multiple expressions, provide each separate expression within parentheses. For example: ``` (scheduling.automaticRestart = true) (cpuPlatform = "Intel Skylake") ``` By default, each expression is an `AND` expression. However, you can include `AND` and `OR` expressions explicitly. For example: ``` (cpuPlatform = "Intel Skylake") OR (cpuPlatform = "Intel Broadwell") AND (scheduling.automaticRestart = true) ``` If you want to use a regular expression, use the `eq` (equal) or `ne` (not equal) operator against a single un-parenthesized expression with or without quotes or against multiple parenthesized expressions. Examples: `fieldname eq unquoted literal` `fieldname eq 'single quoted literal'` `fieldname eq "double quoted literal"` `(fieldname1 eq literal) (fieldname2 ne "literal")` The literal value is interpreted as a regular expression using Google RE2 library syntax. The literal value must match the entire field. For example, to filter for instances that do not end with name "instance", you would use `name ne .*instance`.
      maxResults: integer, The maximum number of results per page that should be returned. If the number of available results is larger than `maxResults`, Compute Engine returns a `nextPageToken` that can be used to get the next page of results in subsequent list requests. Acceptable values are `0` to `500`, inclusive. (Default: `500`)
      orderBy: string, Sorts list results by a certain order. By default, results are returned in alphanumerical order based on the resource name. You can also sort results in descending order based on the creation timestamp using `orderBy="creationTimestamp desc"`. This sorts results based on the `creationTimestamp` field in reverse chronological order (newest result first). Use this to sort resources like operations so that the newest operation is returned first. Currently, only sorting by `name` or `creationTimestamp desc` is supported.
      pageToken: string, Specifies a page token to use. Set `pageToken` to the `nextPageToken` returned by a previous list request to get the next page of results.
      returnPartialSuccess: boolean, Opt-in for partial success behavior which provides partial results in case of failure. The default value is false.
      x__xgafv: string, V1 error format.
        Allowed values
          1 - v1 error format
          2 - v2 error format

    Returns:
      An object of the form:

        { # A list of instance templates.
      "id": "A String", # [Output Only] Unique identifier for the resource; defined by the server.
      "items": [ # A list of InstanceTemplate resources.
        { # Represents an Instance Template resource. You can use instance templates to create VM instances and managed instance groups. For more information, read Instance Templates.
          "creationTimestamp": "A String", # [Output Only] The creation timestamp for this instance template in RFC3339 text format.
          "description": "A String", # An optional description of this resource. Provide this property when you create the resource.
          "id": "A String", # [Output Only] A unique identifier for this instance template. The server defines this identifier.
          "kind": "compute#instanceTemplate", # [Output Only] The resource type, which is always compute#instanceTemplate for instance templates.
          "name": "A String", # Name of the resource; provided by the client when the resource is created. The name must be 1-63 characters long, and comply with RFC1035. Specifically, the name must be 1-63 characters long and match the regular expression `[a-z]([-a-z0-9]*[a-z0-9])?` which means the first character must be a lowercase letter, and all following characters must be a dash, lowercase letter, or digit, except the last character, which cannot be a dash.
          "properties": { # The instance properties for this instance template.
            "advancedMachineFeatures": { # Specifies options for controlling advanced machine features. Options that would traditionally be configured in a BIOS belong here. Features that require operating system support may have corresponding entries in the GuestOsFeatures of an Image (e.g., whether or not the OS in the Image supports nested virtualization being enabled or disabled). # Controls for advanced machine-related behavior features. Note that for MachineImage, this is not supported yet.
              "enableNestedVirtualization": True or False, # Whether to enable nested virtualization or not (default is false).
              "enableUefiNetworking": True or False, # Whether to enable UEFI networking for instance creation.
              "numaNodeCount": 42, # The number of vNUMA nodes.
              "threadsPerCore": 42, # The number of threads per physical core. To disable simultaneous multithreading (SMT) set this to 1. If unset, the maximum number of threads supported per core by the underlying processor is assumed.
              "visibleCoreCount": 42, # The number of physical cores to expose to an instance. Multiply by the number of threads per core to compute the total number of virtual CPUs to expose to the instance. If unset, the number of cores is inferred from the instance's nominal CPU count and the underlying platform's SMT width.
            },
            "canIpForward": True or False, # Enables instances created based on these properties to send packets with source IP addresses other than their own and receive packets with destination IP addresses other than their own. If these instances will be used as an IP gateway or it will be set as the next-hop in a Route resource, specify true. If unsure, leave this set to false. See the Enable IP forwarding documentation for more information.
            "confidentialInstanceConfig": { # A set of Confidential Instance options. # Specifies the Confidential Instance options. Note that for MachineImage, this is not supported yet.
              "confidentialInstanceType": "A String", # Defines the type of technology used by the confidential instance.
              "enableConfidentialCompute": True or False, # Defines whether the instance should have confidential compute enabled.
            },
            "description": "A String", # An optional text description for the instances that are created from these properties.
            "disks": [ # An array of disks that are associated with the instances that are created from these properties.
              { # An instance-attached disk resource.
                "architecture": "A String", # [Output Only] The architecture of the attached disk. Valid values are ARM64 or X86_64.
                "autoDelete": True or False, # Specifies whether the disk will be auto-deleted when the instance is deleted (but not when the disk is detached from the instance).
                "boot": True or False, # Indicates that this is a boot disk. The virtual machine will use the first partition of the disk for its root filesystem.
                "deviceName": "A String", # Specifies a unique device name of your choice that is reflected into the /dev/disk/by-id/google-* tree of a Linux operating system running within the instance. This name can be used to reference the device for mounting, resizing, and so on, from within the instance. If not specified, the server chooses a default device name to apply to this disk, in the form persistent-disk-x, where x is a number assigned by Google Compute Engine. This field is only applicable for persistent disks.
                "diskEncryptionKey": { # Encrypts or decrypts a disk using a customer-supplied encryption key. If you are creating a new disk, this field encrypts the new disk using an encryption key that you provide. If you are attaching an existing disk that is already encrypted, this field decrypts the disk using the customer-supplied encryption key. If you encrypt a disk using a customer-supplied key, you must provide the same key again when you attempt to use this resource at a later time. For example, you must provide the key when you create a snapshot or an image from the disk or when you attach the disk to a virtual machine instance. If you do not provide an encryption key, then the disk will be encrypted using an automatically generated key and you do not need to provide a key to use the disk later. Instance templates do not store customer-supplied encryption keys, so you cannot use your own keys to encrypt disks in a managed instance group.
                  "kmsKeyName": "A String", # The name of the encryption key that is stored in Google Cloud KMS. For example: "kmsKeyName": "projects/kms_project_id/locations/region/keyRings/ key_region/cryptoKeys/key
                  "kmsKeyServiceAccount": "A String", # The service account being used for the encryption request for the given KMS key. If absent, the Compute Engine default service account is used. For example: "kmsKeyServiceAccount": "name@project_id.iam.gserviceaccount.com/
                  "rawKey": "A String", # Specifies a 256-bit customer-supplied encryption key, encoded in RFC 4648 base64 to either encrypt or decrypt this resource. You can provide either the rawKey or the rsaEncryptedKey. For example: "rawKey": "SGVsbG8gZnJvbSBHb29nbGUgQ2xvdWQgUGxhdGZvcm0="
                  "rsaEncryptedKey": "A String", # Specifies an RFC 4648 base64 encoded, RSA-wrapped 2048-bit customer-supplied encryption key to either encrypt or decrypt this resource. You can provide either the rawKey or the rsaEncryptedKey. For example: "rsaEncryptedKey": "ieCx/NcW06PcT7Ep1X6LUTc/hLvUDYyzSZPPVCVPTVEohpeHASqC8uw5TzyO9U+Fka9JFH z0mBibXUInrC/jEk014kCK/NPjYgEMOyssZ4ZINPKxlUh2zn1bV+MCaTICrdmuSBTWlUUiFoD D6PYznLwh8ZNdaheCeZ8ewEXgFQ8V+sDroLaN3Xs3MDTXQEMMoNUXMCZEIpg9Vtp9x2oe==" The key must meet the following requirements before you can provide it to Compute Engine: 1. The key is wrapped using a RSA public key certificate provided by Google. 2. After being wrapped, the key must be encoded in RFC 4648 base64 encoding. Gets the RSA public key certificate provided by Google at: https://cloud-certs.storage.googleapis.com/google-cloud-csek-ingress.pem
                  "sha256": "A String", # [Output only] The RFC 4648 base64 encoded SHA-256 hash of the customer-supplied encryption key that protects this resource.
                },
                "diskSizeGb": "A String", # The size of the disk in GB.
                "forceAttach": True or False, # [Input Only] Whether to force attach the regional disk even if it's currently attached to another instance. If you try to force attach a zonal disk to an instance, you will receive an error.
                "guestOsFeatures": [ # A list of features to enable on the guest operating system. Applicable only for bootable images. Read Enabling guest operating system features to see a list of available options.
                  { # Guest OS features.
                    "type": "A String", # The ID of a supported feature. To add multiple values, use commas to separate values. Set to one or more of the following values: - VIRTIO_SCSI_MULTIQUEUE - WINDOWS - MULTI_IP_SUBNET - UEFI_COMPATIBLE - GVNIC - SEV_CAPABLE - SUSPEND_RESUME_COMPATIBLE - SEV_SNP_CAPABLE For more information, see Enabling guest operating system features.
                  },
                ],
                "index": 42, # [Output Only] A zero-based index to this disk, where 0 is reserved for the boot disk. If you have many disks attached to an instance, each disk would have a unique index number.
                "initializeParams": { # [Input Only] Specifies the parameters for a new disk that will be created alongside the new instance. Use initialization parameters to create boot disks or local SSDs attached to the new instance. This field is persisted and returned for instanceTemplate and not returned in the context of instance. This property is mutually exclusive with the source property; you can only define one or the other, but not both. # [Input Only] Specifies the parameters for a new disk that will be created alongside the new instance. Use initialization parameters to create boot disks or local SSDs attached to the new instance. This property is mutually exclusive with the source property; you can only define one or the other, but not both.
                  "architecture": "A String", # The architecture of the attached disk. Valid values are arm64 or x86_64.
                  "description": "A String", # An optional description. Provide this property when creating the disk.
                  "diskName": "A String", # Specifies the disk name. If not specified, the default is to use the name of the instance. If a disk with the same name already exists in the given region, the existing disk is attached to the new instance and the new disk is not created.
                  "diskSizeGb": "A String", # Specifies the size of the disk in base-2 GB. The size must be at least 10 GB. If you specify a sourceImage, which is required for boot disks, the default size is the size of the sourceImage. If you do not specify a sourceImage, the default disk size is 500 GB.
                  "diskType": "A String", # Specifies the disk type to use to create the instance. If not specified, the default is pd-standard, specified using the full URL. For example: https://www.googleapis.com/compute/v1/projects/project/zones/zone /diskTypes/pd-standard For a full list of acceptable values, see Persistent disk types. If you define this field, you can provide either the full or partial URL. For example, the following are valid values: - https://www.googleapis.com/compute/v1/projects/project/zones/zone /diskTypes/diskType - projects/project/zones/zone/diskTypes/diskType - zones/zone/diskTypes/diskType Note that for InstanceTemplate, this is the name of the disk type, not URL.
                  "guestOsFeatures": [ # A list of features to enable on the guest operating system. Applicable only for bootable images. Read Enabling guest operating system features to see a list of available options. Guest OS features are applied by merging initializeParams.guestOsFeatures and disks.guestOsFeatures
                    { # Guest OS features.
                      "type": "A String", # The ID of a supported feature. To add multiple values, use commas to separate values. Set to one or more of the following values: - VIRTIO_SCSI_MULTIQUEUE - WINDOWS - MULTI_IP_SUBNET - UEFI_COMPATIBLE - GVNIC - SEV_CAPABLE - SUSPEND_RESUME_COMPATIBLE - SEV_SNP_CAPABLE For more information, see Enabling guest operating system features.
                    },
                  ],
                  "interface": "A String", # [Deprecated] Specifies the disk interface to use for attaching this disk, which is either SCSI or NVME. The default is SCSI.
                  "labels": { # Labels to apply to this disk. These can be later modified by the disks.setLabels method. This field is only applicable for persistent disks.
                    "a_key": "A String",
                  },
                  "licenseCodes": [ # Integer license codes indicating which licenses are attached to this disk.
                    "A String",
                  ],
                  "licenses": [ # A list of publicly visible licenses. Reserved for Google's use.
                    "A String",
                  ],
                  "multiWriter": True or False, # Indicates whether or not the disk can be read/write attached to more than one instance.
                  "onUpdateAction": "A String", # Specifies which action to take on instance update with this disk. Default is to use the existing disk.
                  "provisionedIops": "A String", # Indicates how many IOPS to provision for the disk. This sets the number of I/O operations per second that the disk can handle. Values must be between 10,000 and 120,000. For more details, see the Extreme persistent disk documentation.
                  "replicaZones": [ # URLs of the zones where the disk should be replicated to. Only applicable for regional resources.
                    "A String",
                  ],
                  "resourcePolicies": [ # Resource policies applied to this disk for automatic snapshot creations. Specified using the full or partial URL. For instance template, specify only the resource policy name.
                    "A String",
                  ],
                  "sourceImage": "A String", # The source image to create this disk. When creating a new instance, one of initializeParams.sourceImage or initializeParams.sourceSnapshot or disks.source is required except for local SSD. To create a disk with one of the public operating system images, specify the image by its family name. For example, specify family/debian-9 to use the latest Debian 9 image: projects/debian-cloud/global/images/family/debian-9 Alternatively, use a specific version of a public operating system image: projects/debian-cloud/global/images/debian-9-stretch-vYYYYMMDD To create a disk with a custom image that you created, specify the image name in the following format: global/images/my-custom-image You can also specify a custom image by its image family, which returns the latest version of the image in that family. Replace the image name with family/family-name: global/images/family/my-image-family If the source image is deleted later, this field will not be set.
                  "sourceImageEncryptionKey": { # The customer-supplied encryption key of the source image. Required if the source image is protected by a customer-supplied encryption key. Instance templates do not store customer-supplied encryption keys, so you cannot create disks for instances in a managed instance group if the source images are encrypted with your own keys.
                    "kmsKeyName": "A String", # The name of the encryption key that is stored in Google Cloud KMS. For example: "kmsKeyName": "projects/kms_project_id/locations/region/keyRings/ key_region/cryptoKeys/key
                    "kmsKeyServiceAccount": "A String", # The service account being used for the encryption request for the given KMS key. If absent, the Compute Engine default service account is used. For example: "kmsKeyServiceAccount": "name@project_id.iam.gserviceaccount.com/
                    "rawKey": "A String", # Specifies a 256-bit customer-supplied encryption key, encoded in RFC 4648 base64 to either encrypt or decrypt this resource. You can provide either the rawKey or the rsaEncryptedKey. For example: "rawKey": "SGVsbG8gZnJvbSBHb29nbGUgQ2xvdWQgUGxhdGZvcm0="
                    "rsaEncryptedKey": "A String", # Specifies an RFC 4648 base64 encoded, RSA-wrapped 2048-bit customer-supplied encryption key to either encrypt or decrypt this resource. You can provide either the rawKey or the rsaEncryptedKey. For example: "rsaEncryptedKey": "ieCx/NcW06PcT7Ep1X6LUTc/hLvUDYyzSZPPVCVPTVEohpeHASqC8uw5TzyO9U+Fka9JFH z0mBibXUInrC/jEk014kCK/NPjYgEMOyssZ4ZINPKxlUh2zn1bV+MCaTICrdmuSBTWlUUiFoD D6PYznLwh8ZNdaheCeZ8ewEXgFQ8V+sDroLaN3Xs3MDTXQEMMoNUXMCZEIpg9Vtp9x2oe==" The key must meet the following requirements before you can provide it to Compute Engine: 1. The key is wrapped using a RSA public key certificate provided by Google. 2. After being wrapped, the key must be encoded in RFC 4648 base64 encoding. Gets the RSA public key certificate provided by Google at: https://cloud-certs.storage.googleapis.com/google-cloud-csek-ingress.pem
                    "sha256": "A String", # [Output only] The RFC 4648 base64 encoded SHA-256 hash of the customer-supplied encryption key that protects this resource.
                  },
                  "sourceInstantSnapshot": "A String", # The source instant-snapshot to create this disk. When creating a new instance, one of initializeParams.sourceSnapshot or initializeParams.sourceInstantSnapshot initializeParams.sourceImage or disks.source is required except for local SSD. To create a disk with a snapshot that you created, specify the snapshot name in the following format: us-central1-a/instantSnapshots/my-backup If the source instant-snapshot is deleted later, this field will not be set.
                  "sourceSnapshot": "A String", # The source snapshot to create this disk. When creating a new instance, one of initializeParams.sourceSnapshot or initializeParams.sourceImage or disks.source is required except for local SSD. To create a disk with a snapshot that you created, specify the snapshot name in the following format: global/snapshots/my-backup If the source snapshot is deleted later, this field will not be set.
                  "sourceSnapshotEncryptionKey": { # The customer-supplied encryption key of the source snapshot.
                    "kmsKeyName": "A String", # The name of the encryption key that is stored in Google Cloud KMS. For example: "kmsKeyName": "projects/kms_project_id/locations/region/keyRings/ key_region/cryptoKeys/key
                    "kmsKeyServiceAccount": "A String", # The service account being used for the encryption request for the given KMS key. If absent, the Compute Engine default service account is used. For example: "kmsKeyServiceAccount": "name@project_id.iam.gserviceaccount.com/
                    "rawKey": "A String", # Specifies a 256-bit customer-supplied encryption key, encoded in RFC 4648 base64 to either encrypt or decrypt this resource. You can provide either the rawKey or the rsaEncryptedKey. For example: "rawKey": "SGVsbG8gZnJvbSBHb29nbGUgQ2xvdWQgUGxhdGZvcm0="
                    "rsaEncryptedKey": "A String", # Specifies an RFC 4648 base64 encoded, RSA-wrapped 2048-bit customer-supplied encryption key to either encrypt or decrypt this resource. You can provide either the rawKey or the rsaEncryptedKey. For example: "rsaEncryptedKey": "ieCx/NcW06PcT7Ep1X6LUTc/hLvUDYyzSZPPVCVPTVEohpeHASqC8uw5TzyO9U+Fka9JFH z0mBibXUInrC/jEk014kCK/NPjYgEMOyssZ4ZINPKxlUh2zn1bV+MCaTICrdmuSBTWlUUiFoD D6PYznLwh8ZNdaheCeZ8ewEXgFQ8V+sDroLaN3Xs3MDTXQEMMoNUXMCZEIpg9Vtp9x2oe==" The key must meet the following requirements before you can provide it to Compute Engine: 1. The key is wrapped using a RSA public key certificate provided by Google. 2. After being wrapped, the key must be encoded in RFC 4648 base64 encoding. Gets the RSA public key certificate provided by Google at: https://cloud-certs.storage.googleapis.com/google-cloud-csek-ingress.pem
                    "sha256": "A String", # [Output only] The RFC 4648 base64 encoded SHA-256 hash of the customer-supplied encryption key that protects this resource.
                  },
                },
                "interface": "A String", # Specifies the disk interface to use for attaching this disk, which is either SCSI or NVME. The default is SCSI. Persistent disks must always use SCSI and the request will fail if you attempt to attach a persistent disk in any other format than SCSI. Local SSDs can use either NVME or SCSI. For performance characteristics of SCSI over NVMe, see Local SSD performance.
                "kind": "compute#attachedDisk", # [Output Only] Type of the resource. Always compute#attachedDisk for attached disks.
                "licenses": [ # [Output Only] Any valid publicly visible licenses.
                  "A String",
                ],
                "locked": True or False, # [Output Only] Whether to indicate the attached disk is locked. The locked disk is not allowed to be detached from the instance, or to be used as the source of the snapshot creation, and the image creation. The instance with at least one locked attached disk is not allow to be used as source of machine image creation, instant snapshot creation, and not allowed to be deleted with --keep-disk parameter set to true for locked disks.
                "mode": "A String", # The mode in which to attach this disk, either READ_WRITE or READ_ONLY. If not specified, the default is to attach the disk in READ_WRITE mode.
                "savedState": "A String", # For LocalSSD disks on VM Instances in STOPPED or SUSPENDED state, this field is set to PRESERVED if the LocalSSD data has been saved to a persistent location by customer request. (see the discard_local_ssd option on Stop/Suspend). Read-only in the api.
                "shieldedInstanceInitialState": { # Initial State for shielded instance, these are public keys which are safe to store in public # [Output Only] shielded vm initial state stored on disk
                  "dbs": [ # The Key Database (db).
                    {
                      "content": "A String", # The raw content in the secure keys file.
                      "fileType": "A String", # The file type of source file.
                    },
                  ],
                  "dbxs": [ # The forbidden key database (dbx).
                    {
                      "content": "A String", # The raw content in the secure keys file.
                      "fileType": "A String", # The file type of source file.
                    },
                  ],
                  "keks": [ # The Key Exchange Key (KEK).
                    {
                      "content": "A String", # The raw content in the secure keys file.
                      "fileType": "A String", # The file type of source file.
                    },
                  ],
                  "pk": { # The Platform Key (PK).
                    "content": "A String", # The raw content in the secure keys file.
                    "fileType": "A String", # The file type of source file.
                  },
                },
                "source": "A String", # Specifies a valid partial or full URL to an existing Persistent Disk resource. When creating a new instance, one of initializeParams.sourceImage or initializeParams.sourceSnapshot or disks.source is required except for local SSD. If desired, you can also attach existing non-root persistent disks using this property. This field is only applicable for persistent disks. Note that for InstanceTemplate, specify the disk name for zonal disk, and the URL for regional disk.
                "type": "A String", # Specifies the type of the disk, either SCRATCH or PERSISTENT. If not specified, the default is PERSISTENT.
                "userLicenses": [ # [Output Only] A list of user provided licenses. It represents a list of URLs to the license resource. Unlike regular licenses, user provided licenses can be modified after the disk is created.
                  "A String",
                ],
              },
            ],
            "displayDevice": { # A set of Display Device options # Display Device properties to enable support for remote display products like: Teradici, VNC and TeamViewer Note that for MachineImage, this is not supported yet.
              "enableDisplay": True or False, # Defines whether the instance has Display enabled.
            },
            "guestAccelerators": [ # A list of guest accelerator cards' type and count to use for instances created from these properties.
              { # A specification of the type and number of accelerator cards attached to the instance.
                "acceleratorCount": 42, # The number of the guest accelerator cards exposed to this instance.
                "acceleratorType": "A String", # Full or partial URL of the accelerator type resource to attach to this instance. For example: projects/my-project/zones/us-central1-c/acceleratorTypes/nvidia-tesla-p100 If you are creating an instance template, specify only the accelerator name. See GPUs on Compute Engine for a full list of accelerator types.
              },
            ],
            "keyRevocationActionType": "A String", # KeyRevocationActionType of the instance. Supported options are "STOP" and "NONE". The default value is "NONE" if it is not specified.
            "labels": { # Labels to apply to instances that are created from these properties.
              "a_key": "A String",
            },
            "machineType": "A String", # The machine type to use for instances that are created from these properties.
            "metadata": { # A metadata key/value entry. # The metadata key/value pairs to assign to instances that are created from these properties. These pairs can consist of custom metadata or predefined keys. See Project and instance metadata for more information.
              "fingerprint": "A String", # Specifies a fingerprint for this request, which is essentially a hash of the metadata's contents and used for optimistic locking. The fingerprint is initially generated by Compute Engine and changes after every request to modify or update metadata. You must always provide an up-to-date fingerprint hash in order to update or change metadata, otherwise the request will fail with error 412 conditionNotMet. To see the latest fingerprint, make a get() request to retrieve the resource.
              "items": [ # Array of key/value pairs. The total size of all keys and values must be less than 512 KB.
                { # Metadata
                  "key": "A String", # Key for the metadata entry. Keys must conform to the following regexp: [a-zA-Z0-9-_]+, and be less than 128 bytes in length. This is reflected as part of a URL in the metadata server. Additionally, to avoid ambiguity, keys must not conflict with any other metadata keys for the project.
                  "value": "A String", # Value for the metadata entry. These are free-form strings, and only have meaning as interpreted by the image running in the instance. The only restriction placed on values is that their size must be less than or equal to 262144 bytes (256 KiB).
                },
              ],
              "kind": "compute#metadata", # [Output Only] Type of the resource. Always compute#metadata for metadata.
            },
            "minCpuPlatform": "A String", # Minimum cpu/platform to be used by instances. The instance may be scheduled on the specified or newer cpu/platform. Applicable values are the friendly names of CPU platforms, such as minCpuPlatform: "Intel Haswell" or minCpuPlatform: "Intel Sandy Bridge". For more information, read Specifying a Minimum CPU Platform.
            "networkInterfaces": [ # An array of network access configurations for this interface.
              { # A network interface resource attached to an instance.
                "accessConfigs": [ # An array of configurations for this interface. Currently, only one access config, ONE_TO_ONE_NAT, is supported. If there are no accessConfigs specified, then this instance will have no external internet access.
                  { # An access configuration attached to an instance's network interface. Only one access config per instance is supported.
                    "externalIpv6": "A String", # The first IPv6 address of the external IPv6 range associated with this instance, prefix length is stored in externalIpv6PrefixLength in ipv6AccessConfig. The field is output only, an IPv6 address from a subnetwork associated with the instance will be allocated dynamically.
                    "externalIpv6PrefixLength": 42, # The prefix length of the external IPv6 range.
                    "kind": "compute#accessConfig", # [Output Only] Type of the resource. Always compute#accessConfig for access configs.
                    "name": "A String", # The name of this access configuration. The default and recommended name is External NAT, but you can use any arbitrary string, such as My external IP or Network Access.
                    "natIP": "A String", # An external IP address associated with this instance. Specify an unused static external IP address available to the project or leave this field undefined to use an IP from a shared ephemeral IP address pool. If you specify a static external IP address, it must live in the same region as the zone of the instance.
                    "networkTier": "A String", # This signifies the networking tier used for configuring this access configuration and can only take the following values: PREMIUM, STANDARD. If an AccessConfig is specified without a valid external IP address, an ephemeral IP will be created with this networkTier. If an AccessConfig with a valid external IP address is specified, it must match that of the networkTier associated with the Address resource owning that IP.
                    "publicDnsName": "A String", # [Output Only] The public DNS domain name for the instance.
                    "publicPtrDomainName": "A String", # The DNS domain name for the public PTR record. You can set this field only if the `setPublicPtr` field is enabled in accessConfig. If this field is unspecified in ipv6AccessConfig, a default PTR record will be createc for first IP in associated external IPv6 range.
                    "setPublicDns": True or False, # Specifies whether a public DNS 'A' record should be created for the external IP address of this access configuration.
                    "setPublicPtr": True or False, # Specifies whether a public DNS 'PTR' record should be created to map the external IP address of the instance to a DNS domain name. This field is not used in ipv6AccessConfig. A default PTR record will be created if the VM has external IPv6 range associated.
                    "type": "ONE_TO_ONE_NAT", # The type of configuration. The default and only option is ONE_TO_ONE_NAT.
                  },
                ],
                "aliasIpRanges": [ # An array of alias IP ranges for this network interface. You can only specify this field for network interfaces in VPC networks.
                  { # An alias IP range attached to an instance's network interface.
                    "ipCidrRange": "A String", # The IP alias ranges to allocate for this interface. This IP CIDR range must belong to the specified subnetwork and cannot contain IP addresses reserved by system or used by other network interfaces. This range may be a single IP address (such as 10.2.3.4), a netmask (such as /24) or a CIDR-formatted string (such as 10.1.2.0/24).
                    "subnetworkRangeName": "A String", # The name of a subnetwork secondary IP range from which to allocate an IP alias range. If not specified, the primary range of the subnetwork is used.
                  },
                ],
                "fingerprint": "A String", # Fingerprint hash of contents stored in this network interface. This field will be ignored when inserting an Instance or adding a NetworkInterface. An up-to-date fingerprint must be provided in order to update the NetworkInterface. The request will fail with error 400 Bad Request if the fingerprint is not provided, or 412 Precondition Failed if the fingerprint is out of date.
                "internalIpv6PrefixLength": 42, # The prefix length of the primary internal IPv6 range.
                "ipv6AccessConfigs": [ # An array of IPv6 access configurations for this interface. Currently, only one IPv6 access config, DIRECT_IPV6, is supported. If there is no ipv6AccessConfig specified, then this instance will have no external IPv6 Internet access.
                  { # An access configuration attached to an instance's network interface. Only one access config per instance is supported.
                    "externalIpv6": "A String", # The first IPv6 address of the external IPv6 range associated with this instance, prefix length is stored in externalIpv6PrefixLength in ipv6AccessConfig. The field is output only, an IPv6 address from a subnetwork associated with the instance will be allocated dynamically.
                    "externalIpv6PrefixLength": 42, # The prefix length of the external IPv6 range.
                    "kind": "compute#accessConfig", # [Output Only] Type of the resource. Always compute#accessConfig for access configs.
                    "name": "A String", # The name of this access configuration. The default and recommended name is External NAT, but you can use any arbitrary string, such as My external IP or Network Access.
                    "natIP": "A String", # An external IP address associated with this instance. Specify an unused static external IP address available to the project or leave this field undefined to use an IP from a shared ephemeral IP address pool. If you specify a static external IP address, it must live in the same region as the zone of the instance.
                    "networkTier": "A String", # This signifies the networking tier used for configuring this access configuration and can only take the following values: PREMIUM, STANDARD. If an AccessConfig is specified without a valid external IP address, an ephemeral IP will be created with this networkTier. If an AccessConfig with a valid external IP address is specified, it must match that of the networkTier associated with the Address resource owning that IP.
                    "publicDnsName": "A String", # [Output Only] The public DNS domain name for the instance.
                    "publicPtrDomainName": "A String", # The DNS domain name for the public PTR record. You can set this field only if the `setPublicPtr` field is enabled in accessConfig. If this field is unspecified in ipv6AccessConfig, a default PTR record will be createc for first IP in associated external IPv6 range.
                    "setPublicDns": True or False, # Specifies whether a public DNS 'A' record should be created for the external IP address of this access configuration.
                    "setPublicPtr": True or False, # Specifies whether a public DNS 'PTR' record should be created to map the external IP address of the instance to a DNS domain name. This field is not used in ipv6AccessConfig. A default PTR record will be created if the VM has external IPv6 range associated.
                    "type": "ONE_TO_ONE_NAT", # The type of configuration. The default and only option is ONE_TO_ONE_NAT.
                  },
                ],
                "ipv6AccessType": "A String", # [Output Only] One of EXTERNAL, INTERNAL to indicate whether the IP can be accessed from the Internet. This field is always inherited from its subnetwork. Valid only if stackType is IPV4_IPV6.
                "ipv6Address": "A String", # An IPv6 internal network address for this network interface.
                "kind": "compute#networkInterface", # [Output Only] Type of the resource. Always compute#networkInterface for network interfaces.
                "name": "A String", # [Output Only] The name of the network interface, which is generated by the server. For a VM, the network interface uses the nicN naming format. Where N is a value between 0 and 7. The default interface value is nic0.
                "network": "A String", # URL of the VPC network resource for this instance. When creating an instance, if neither the network nor the subnetwork is specified, the default network global/networks/default is used. If the selected project doesn't have the default network, you must specify a network or subnet. If the network is not specified but the subnetwork is specified, the network is inferred. If you specify this property, you can specify the network as a full or partial URL. For example, the following are all valid URLs: - https://www.googleapis.com/compute/v1/projects/project/global/networks/ network - projects/project/global/networks/network - global/networks/default
                "networkIP": "A String", # An IPv4 internal IP address to assign to the instance for this network interface. If not specified by the user, an unused internal IP is assigned by the system.
                "nicType": "A String", # The type of vNIC to be used on this interface. This may be gVNIC or VirtioNet.
                "queueCount": 42, # The networking queue count that's specified by users for the network interface. Both Rx and Tx queues will be set to this number. It'll be empty if not specified by the users.
                "stackType": "A String", # The stack type for this network interface to identify whether the IPv6 feature is enabled or not. If not specified, IPV4_ONLY will be used. This field can be both set at instance creation and update network interface operations.
                "subinterfaces": [ # SubInterfaces help enable L2 communication for the instance over subnetworks that support L2. Every network interface will get a default untagged (vlan not specified) subinterface. Users can specify additional tagged subinterfaces which are sub-fields to the Network Interface.
                  {
                    "ipAddress": "A String", # An IPv4 internal IP address to assign to the instance for this subinterface. If specified, ip_allocation_mode should be set to ALLOCATE_IP.
                    "ipAllocationMode": "A String",
                    "subnetwork": "A String", # If specified, this subnetwork must belong to the same network as that of the network interface. If not specified the subnet of network interface will be used. If you specify this property, you can specify the subnetwork as a full or partial URL. For example, the following are all valid URLs: - https://www.googleapis.com/compute/v1/projects/project/regions/region /subnetworks/subnetwork - regions/region/subnetworks/subnetwork
                    "vlan": 42, # VLAN tag. Should match the VLAN(s) supported by the subnetwork to which this subinterface is connecting.
                  },
                ],
                "subnetwork": "A String", # The URL of the Subnetwork resource for this instance. If the network resource is in legacy mode, do not specify this field. If the network is in auto subnet mode, specifying the subnetwork is optional. If the network is in custom subnet mode, specifying the subnetwork is required. If you specify this field, you can specify the subnetwork as a full or partial URL. For example, the following are all valid URLs: - https://www.googleapis.com/compute/v1/projects/project/regions/region /subnetworks/subnetwork - regions/region/subnetworks/subnetwork
              },
            ],
            "networkPerformanceConfig": { # Note that for MachineImage, this is not supported yet.
              "externalIpEgressBandwidthTier": "A String",
              "totalEgressBandwidthTier": "A String",
            },
            "postKeyRevocationActionType": "A String", # PostKeyRevocationActionType of the instance.
            "privateIpv6GoogleAccess": "A String", # The private IPv6 google access type for VMs. If not specified, use INHERIT_FROM_SUBNETWORK as default. Note that for MachineImage, this is not supported yet.
            "reservationAffinity": { # Specifies the reservations that this instance can consume from. # Specifies the reservations that instances can consume from. Note that for MachineImage, this is not supported yet.
              "consumeReservationType": "A String", # Specifies the type of reservation from which this instance can consume resources: ANY_RESERVATION (default), SPECIFIC_RESERVATION, or NO_RESERVATION. See Consuming reserved instances for examples.
              "key": "A String", # Corresponds to the label key of a reservation resource. To target a SPECIFIC_RESERVATION by name, specify googleapis.com/reservation-name as the key and specify the name of your reservation as its value.
              "values": [ # Corresponds to the label values of a reservation resource. This can be either a name to a reservation in the same project or "projects/different-project/reservations/some-reservation-name" to target a shared reservation in the same zone but in a different project.
                "A String",
              ],
            },
            "resourceManagerTags": { # Resource manager tags to be bound to the instance. Tag keys and values have the same definition as resource manager tags. Keys must be in the format `tagKeys/{tag_key_id}`, and values are in the format `tagValues/456`. The field is ignored (both PUT & PATCH) when empty.
              "a_key": "A String",
            },
            "resourcePolicies": [ # Resource policies (names, not URLs) applied to instances created from these properties. Note that for MachineImage, this is not supported yet.
              "A String",
            ],
            "scheduling": { # Sets the scheduling options for an Instance. NextID: 21 # Specifies the scheduling options for the instances that are created from these properties.
              "automaticRestart": True or False, # Specifies whether the instance should be automatically restarted if it is terminated by Compute Engine (not terminated by a user). You can only set the automatic restart option for standard instances. Preemptible instances cannot be automatically restarted. By default, this is set to true so an instance is automatically restarted if it is terminated by Compute Engine.
              "availabilityDomain": 42, # Specifies the availability domain (AD), which this instance should be scheduled on. The AD belongs to the spread GroupPlacementPolicy resource policy that has been assigned to the instance. Specify a value between 1-max count of availability domains in your GroupPlacementPolicy. See go/placement-policy-extension for more details.
              "currentCpus": 42, # Current number of vCPUs available for VM. 0 or unset means default vCPUs of the current machine type.
              "currentMemoryMb": "A String", # Current amount of memory (in MB) available for VM. 0 or unset means default amount of memory of the current machine type.
              "hostErrorTimeoutSeconds": 42, # Specify the time in seconds for host error detection, the value must be within the range of [90, 330] with the increment of 30, if unset, the default behavior of host error recovery will be used.
              "instanceTerminationAction": "A String", # Specifies the termination action for the instance.
              "latencyTolerant": True or False, # Defines whether the instance is tolerant of higher cpu latency. This can only be set during instance creation, or when the instance is not currently running. It must not be set if the preemptible option is also set.
              "locationHint": "A String", # An opaque location hint used to place the instance close to other resources. This field is for use by internal tools that use the public API.
              "maintenanceFreezeDurationHours": 42, # Specifies the number of hours after VM instance creation where the VM won't be scheduled for maintenance.
              "maintenanceInterval": "A String", # For more information about maintenance intervals, see Setting maintenance intervals.
              "maxRunDuration": { # A Duration represents a fixed-length span of time represented as a count of seconds and fractions of seconds at nanosecond resolution. It is independent of any calendar and concepts like "day" or "month". Range is approximately 10,000 years. # Specifies the max run duration for the given instance. If specified, the instance termination action will be performed at the end of the run duration.
                "nanos": 42, # Span of time that's a fraction of a second at nanosecond resolution. Durations less than one second are represented with a 0 `seconds` field and a positive `nanos` field. Must be from 0 to 999,999,999 inclusive.
                "seconds": "A String", # Span of time at a resolution of a second. Must be from 0 to 315,576,000,000 inclusive. Note: these bounds are computed from: 60 sec/min * 60 min/hr * 24 hr/day * 365.25 days/year * 10000 years
              },
              "minNodeCpus": 42, # The minimum number of virtual CPUs this instance will consume when running on a sole-tenant node.
              "nodeAffinities": [ # A set of node affinity and anti-affinity configurations. Refer to Configuring node affinity for more information. Overrides reservationAffinity.
                { # Node Affinity: the configuration of desired nodes onto which this Instance could be scheduled.
                  "key": "A String", # Corresponds to the label key of Node resource.
                  "operator": "A String", # Defines the operation of node selection. Valid operators are IN for affinity and NOT_IN for anti-affinity.
                  "values": [ # Corresponds to the label values of Node resource.
                    "A String",
                  ],
                },
              ],
              "onHostMaintenance": "A String", # Defines the maintenance behavior for this instance. For standard instances, the default behavior is MIGRATE. For preemptible instances, the default and only possible behavior is TERMINATE. For more information, see Set VM host maintenance policy.
              "preemptible": True or False, # Defines whether the instance is preemptible. This can only be set during instance creation or while the instance is stopped and therefore, in a `TERMINATED` state. See Instance Life Cycle for more information on the possible instance states.
              "provisioningModel": "A String", # Specifies the provisioning model of the instance.
              "terminationTime": "A String", # Specifies the timestamp, when the instance will be terminated, in RFC3339 text format. If specified, the instance termination action will be performed at the termination time.
            },
            "secureTags": [ # [Input Only] Secure tags to apply to this instance. Maximum number of secure tags allowed is 50. Note that for MachineImage, this is not supported yet.
              "A String",
            ],
            "serviceAccounts": [ # A list of service accounts with specified scopes. Access tokens for these service accounts are available to the instances that are created from these properties. Use metadata queries to obtain the access tokens for these instances.
              { # A service account.
                "email": "A String", # Email address of the service account.
                "scopes": [ # The list of scopes to be made available for this service account.
                  "A String",
                ],
              },
            ],
            "shieldedInstanceConfig": { # A set of Shielded Instance options. # Note that for MachineImage, this is not supported yet.
              "enableIntegrityMonitoring": True or False, # Defines whether the instance has integrity monitoring enabled. Enabled by default.
              "enableSecureBoot": True or False, # Defines whether the instance has Secure Boot enabled. Disabled by default.
              "enableVtpm": True or False, # Defines whether the instance has the vTPM enabled. Enabled by default.
            },
            "shieldedVmConfig": { # A set of Shielded VM options. # Specifies the Shielded VM options for the instances that are created from these properties.
              "enableIntegrityMonitoring": True or False, # Defines whether the instance has integrity monitoring enabled.
              "enableSecureBoot": True or False, # Defines whether the instance has Secure Boot enabled.
              "enableVtpm": True or False, # Defines whether the instance has the vTPM enabled.
            },
            "tags": { # A set of instance tags. # A list of tags to apply to the instances that are created from these properties. The tags identify valid sources or targets for network firewalls. The setTags method can modify this list of tags. Each tag within the list must comply with RFC1035.
              "fingerprint": "A String", # Specifies a fingerprint for this request, which is essentially a hash of the tags' contents and used for optimistic locking. The fingerprint is initially generated by Compute Engine and changes after every request to modify or update tags. You must always provide an up-to-date fingerprint hash in order to update or change tags. To see the latest fingerprint, make get() request to the instance.
              "items": [ # An array of tags. Each tag must be 1-63 characters long, and comply with RFC1035.
                "A String",
              ],
            },
          },
          "region": "A String", # [Output Only] URL of the region where the instance template resides. Only applicable for regional resources.
          "selfLink": "A String", # [Output Only] The URL for this instance template. The server defines this URL.
          "selfLinkWithId": "A String", # [Output Only] Server-defined URL for this resource with the resource id.
          "sourceInstance": "A String", # The source instance used to create the template. You can provide this as a partial or full URL to the resource. For example, the following are valid values: - https://www.googleapis.com/compute/v1/projects/project/zones/zone /instances/instance - projects/project/zones/zone/instances/instance
          "sourceInstanceParams": { # A specification of the parameters to use when creating the instance template from a source instance. # The source instance params to use to create this instance template.
            "diskConfigs": [ # Attached disks configuration. If not provided, defaults are applied: For boot disk and any other R/W disks, new custom images will be created from each disk. For read-only disks, they will be attached in read-only mode. Local SSD disks will be created as blank volumes.
              { # A specification of the desired way to instantiate a disk in the instance template when its created from a source instance.
                "autoDelete": True or False, # Specifies whether the disk will be auto-deleted when the instance is deleted (but not when the disk is detached from the instance).
                "customImage": "A String", # The custom source image to be used to restore this disk when instantiating this instance template.
                "deviceName": "A String", # Specifies the device name of the disk to which the configurations apply to.
                "instantiateFrom": "A String", # Specifies whether to include the disk and what image to use. Possible values are: - source-image: to use the same image that was used to create the source instance's corresponding disk. Applicable to the boot disk and additional read-write disks. - source-image-family: to use the same image family that was used to create the source instance's corresponding disk. Applicable to the boot disk and additional read-write disks. - custom-image: to use a user-provided image url for disk creation. Applicable to the boot disk and additional read-write disks. - attach-read-only: to attach a read-only disk. Applicable to read-only disks. - do-not-include: to exclude a disk from the template. Applicable to additional read-write disks, local SSDs, and read-only disks.
              },
            ],
          },
        },
      ],
      "kind": "compute#instanceTemplateList", # [Output Only] The resource type, which is always compute#instanceTemplatesListResponse for instance template lists.
      "nextPageToken": "A String", # [Output Only] This token allows you to get the next page of results for list requests. If the number of results is larger than maxResults, use the nextPageToken as a value for the query parameter pageToken in the next list request. Subsequent list requests will have their own nextPageToken to continue paging through the results.
      "selfLink": "A String", # [Output Only] Server-defined URL for this resource.
      "warning": { # [Output Only] Informational warning message.
        "code": "A String", # [Output Only] A warning code, if applicable. For example, Compute Engine returns NO_RESULTS_ON_PAGE if there are no results in the response.
        "data": [ # [Output Only] Metadata about this warning in key: value format. For example: "data": [ { "key": "scope", "value": "zones/us-east1-d" }
          {
            "key": "A String", # [Output Only] A key that provides more detail on the warning being returned. For example, for warnings where there are no results in a list request for a particular zone, this key might be scope and the key value might be the zone name. Other examples might be a key indicating a deprecated resource and a suggested replacement, or a warning about invalid network settings (for example, if an instance attempts to perform IP forwarding but is not enabled for IP forwarding).
            "value": "A String", # [Output Only] A warning data value corresponding to the key.
          },
        ],
        "message": "A String", # [Output Only] A human-readable description of the warning code.
      },
    }

`list_next()`

    Retrieves the next page of results.

            Args:
              previous_request: The request for the previous page. (required)
              previous_response: The response from the request for the previous page. (required)

            Returns:
              A request object that you can call 'execute()' on to request the next
              page. Returns None if there are no more items in the collection.