#cloud-config
## the rsyslog module allows you to configure the systems syslog.
## configuration of syslog is under the top level cloud-config
## entry 'rsyslog'.
##
## Example:
#cloud-config
rsyslog:
  remotes:
    # udp to host 'maas.mydomain' port 514
    maashost: maas.mydomain
    # udp to ipv4 host on port 514
    maas: "@[10.5.1.56]:514"
    # tcp to host ipv6 host on port 555
    maasipv6: "*.* @@[FE80::0202:B3FF:FE1E:8329]:555"
  configs:
    - "*.* @@192.158.1.1"
    - content: "*.*   @@192.0.2.1:10514"
      filename: 01-example.conf
    - content: |
        *.*   @@syslogd.example.com
  config_dir: /etc/rsyslog.d
  config_filename: 20-cloud-config.conf
  service_reload_command: [your, syslog, reload, command]

## Additionally the following legacy format is supported
## it is converted into the format above before use.
##  rsyslog_filename -> rsyslog/config_filename
##  rsyslog_dir -> rsyslog/config_dir
##  rsyslog -> rsyslog/configs
# rsyslog:
#   - "*.* @@192.158.1.1"
#   - content: "*.*   @@192.0.2.1:10514"
#     filename: 01-example.conf
#   - content: |
#       *.*   @@syslogd.example.com
# rsyslog_filename: 20-cloud-config.conf
# rsyslog_dir: /etc/rsyslog.d

## to configure rsyslog to accept remote logging on Ubuntu
## write the following into /etc/rsyslog.d/20-remote-udp.conf
##   $ModLoad imudp
##   $UDPServerRun 514
##   $template LogRemote,"/var/log/maas/rsyslog/%HOSTNAME%/messages"
##   :fromhost-ip, !isequal, "127.0.0.1" ?LogRemote
## then:
## sudo service rsyslog restart
